[38;5;12m                    [39m[38;2;255;187;0m[1m[4mAwesome ESP [0m[38;5;14m[1m[4m![0m[38;2;255;187;0m[1m[4mAwesome[0m[38;5;14m[1m[4m (https://awesome.re/badge.svg)[0m[38;2;255;187;0m[1m[4m (https://awesome.re) [0m[38;5;14m[1m[4m![0m[38;2;255;187;0m[1m[4mContributor Covenant[0m[38;5;14m[1m[4m (https://img.shields.io/badge/Contributor%20Covenant-v2.0%20adopted-ff69b4.svg)[0m[38;2;255;187;0m[1m[4m (code-of-conduct.md)[0m
[38;5;12mA curated list of awesome ESP8266/32 projects and code.[39m



[38;5;11m[1m▐[0m[38;5;12m [39m[38;5;12mBoth[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;14m[1mESP8266[0m[38;5;12m [39m[38;5;12m(http://espressif.com/en/products/hardware/esp8266ex/overview)[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;14m[1mESP32[0m[38;5;12m [39m[38;5;12m(http://espressif.com/en/products/hardware/esp32/overview)[39m[38;5;12m [39m[38;5;12mare[39m[38;5;12m [39m[38;5;12mlow-cost[39m[38;5;12m [39m[38;5;12mWi-Fi[39m[38;5;12m [39m[38;5;12mmicrochips[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mfull[39m[38;5;12m [39m[38;5;12mTCP/IP[39m[38;5;12m [39m[38;5;12mstack[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mmicrocontroller[39m[38;5;12m [39m
[38;5;11m[1m▐[0m[38;5;12m [39m[38;5;12mcapabilities[39m[38;5;12m [39m[38;5;12mproduced[39m[38;5;12m [39m[38;5;12mby[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12mShanghai-based[39m[38;5;12m [39m[38;5;12mmanufacturer[39m[38;5;12m [39m[38;5;12mEspressif[39m[38;5;12m [39m[38;5;12mSystems.[39m
[38;5;11m[1m▐[0m[38;5;12m [39m
[38;5;11m[1m▐[0m[38;5;12m [39m[38;5;12mSee [39m[38;5;14m[1mContributing[0m[38;5;12m (contributing.md) for information on how to contribute to this list.[39m
[38;5;11m[1m▐[0m[38;5;12m [39m
[38;5;238m――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――――[39m

[38;2;255;187;0m[4mContents[0m
[38;5;12m- [39m[38;5;14m[1mFirmware[0m[38;5;12m (#firmware)[39m
[38;5;12m- [39m[38;5;14m[1mTools[0m[38;5;12m (#tools)[39m
[38;5;12m- [39m[38;5;14m[1mProjects[0m[38;5;12m (#projects)[39m
[38;5;12m  - [39m[38;5;14m[1mSmart Home and IoT[0m[38;5;12m (#smart-home-and-iot)[39m
[38;5;12m  - [39m[38;5;14m[1mInfoSec[0m[38;5;12m (#infosec)[39m
[38;5;12m  - [39m[38;5;14m[1mBiomedical[0m[38;5;12m (#biomedical)[39m
[38;5;12m  - [39m[38;5;14m[1mLoRa[0m[38;5;12m (#lora)[39m
[38;5;12m  - [39m[38;5;14m[1mMusic and Audio[0m[38;5;12m (#music-and-audio)[39m
[38;5;12m  - [39m[38;5;14m[1mSmartwatches[0m[38;5;12m (#smartwatches)[39m
[38;5;12m  - [39m[38;5;14m[1mOthers[0m[38;5;12m (#others)[39m
[38;5;12m- [39m[38;5;14m[1mLibraries[0m[38;5;12m (#libraries)[39m

[38;2;255;187;0m[4mFirmware[0m
[38;5;12m- [39m[38;5;14m[1mEspressif AT[0m[38;5;12m (http://bbs.espressif.com/) - The default vanilla firmware for the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mNodeMCU[0m[38;5;12m (https://github.com/nodemcu/nodemcu-firmware) - An eLua-based firmware for the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mESPBasic[0m[38;5;12m (http://www.esp8266basic.com/) - A BASIC firmware for easy and wireless programming, ready for the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mMicroPython[0m[38;5;12m (https://github.com/micropython/micropython/) - An implemention of Python3 for the ESP8266 and 32.[39m
[38;5;12m- [39m[38;5;14m[1mESP3D[0m[38;5;12m (https://github.com/luc-github/ESP3D) - An experimental firmware for 3D Printers, both the ESP32 and 8266.[39m
[38;5;12m- [39m[38;5;14m[1mFrankenstein[0m[38;5;12m (https://github.com/nekromant/esp8266-frankenstein) - A quick and dirty firmware with cool features for the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mMongooseOS[0m[38;5;12m (https://github.com/cesanta/mongoose-os) - An IoT specific firmware, with both C and JS. Available for the ESP32/8266.[39m
[38;5;12m- [39m[38;5;14m[1mDeviceHive[0m[38;5;12m (https://devicehive.com/) - A firmware made as a client for DeviceHive's IoT data platform, only for the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mRT-Thread[0m[38;5;12m (https://github.com/RT-Thread/rt-thread) - Chinese open source firmware available for the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mSming Framework[0m[38;5;12m (https://github.com/SmingHub/Sming) - Superb C/C++ IoT Framework with support for ESP8266 and ESP32.[39m

[38;2;255;187;0m[4mTools[0m
[38;5;12m- [39m[38;5;14m[1mESP Flash Tool[0m[38;5;12m (http://espressif.com/en/support/download/other-tools) - The vanilla firmware flasher for both ESP's.[39m
[38;5;12m- [39m[38;5;14m[1mArduino Core/8266[0m[38;5;12m (https://github.com/esp8266/arduino) - The Arduino core for the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mArduino Core/32[0m[38;5;12m (https://github.com/espressif/arduino-esp32) - The other Arduino core for the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mESPTool[0m[38;5;12m (https://github.com/espressif/esptool) - Espressif's command line tool for bootloader comms in both ESP's.[39m
[38;5;12m- [39m[38;5;14m[1mESP-Open-SDK[0m[38;5;12m (https://github.com/pfalcon/esp-open-sdk) - An open SDK for the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mESPTool-ck[0m[38;5;12m (https://github.com/igrr/esptool-ck) - A CLI tool for flashing in the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mESPTool-gui[0m[38;5;12m (https://github.com/Rodmg/esptool-gui) - A flashing GUI tool based on ESPTool-ck.[39m
[38;5;12m- [39m[38;5;14m[1mLuaNode[0m[38;5;12m (https://github.com/Nicholas3388/LuaNode) - A lua-only SDK for 32/8266.[39m
[38;5;12m- [39m[38;5;14m[1mTuya-Convert[0m[38;5;12m (https://github.com/ct-Open-Source/tuya-convert) - A Wi-Fi firmware flasher ESP8266 that has been pre-loaded with Tuya firmware.[39m
[38;5;12m- [39m[38;5;14m[1mNodeMCU Flasher[0m[38;5;12m (https://github.com/nodemcu/nodemcu-flasher) - The official flashing tool for the NodeMCU OS.[39m
[38;5;12m- [39m[38;5;14m[1mTasmotizer[0m[38;5;12m (https://github.com/tasmota/tasmotizer) - A graphical flashing tool for Tasmota firmware. Can manage Wi-Fi & MQTT settings, modules & templates.[39m
[38;5;12m- [39m[38;5;14m[1mArduino FS Plugin[0m[38;5;12m (https://github.com/esp8266/arduino-esp8266fs-plugin) - An Arduino plugin for filesystem uploads in the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mPlatformIO[0m[38;5;12m (https://github.com/platformio/platformio-core) - Cross Platform IDE and Debugger that supports both the ESP32 and ESP8266.[39m

[38;2;255;187;0m[4mProjects[0m
[38;2;255;187;0m[4mSmart Home and IoT[0m
[38;5;12m- [39m[38;5;14m[1mOpenMQTTGateway[0m[38;5;12m (https://github.com/1technophile/OpenMQTTGateway) - An implementation of a multiprotocol MQTT gateway for both ESP's among other devices.[39m
[38;5;12m- [39m[38;5;14m[1mESPHome[0m[38;5;12m (https://esphome.io/) - A full-featured system for controlling ESP's through simple yet powerful configuration files and Home Automation systems.[39m
[38;5;12m-[39m[38;5;12m [39m[38;5;14m[1mTasmota[0m[38;5;12m [39m[38;5;12m(https://tasmota.github.io/docs/)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mAn[39m[38;5;12m [39m[38;5;12malternative[39m[38;5;12m [39m[38;5;12mfirmware[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;12mSonoff[39m[38;5;12m [39m[38;5;12m&[39m[38;5;12m [39m[38;5;12mother[39m[38;5;12m [39m[38;5;12mESP8266/ESP32[39m[38;5;12m [39m[38;5;12mdevices.[39m[38;5;12m [39m[38;5;12mIncludes[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mlarge[39m[38;5;12m [39m[38;5;12mcollection[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12msensor[39m[38;5;12m [39m[38;5;12mdrivers[39m[38;5;12m [39m[38;5;12m&[39m[38;5;12m [39m[38;5;12mintegrates[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;14m[1mHome[0m[38;5;14m[1m [0m[38;5;14m[1mAssistant[0m[38;5;12m [39m[38;5;12m(https://www.home-assistant.io/)[39m[38;5;12m [39m[38;5;12mnatively[39m[38;5;12m [39m[38;5;12mor[39m[38;5;12m [39m
[38;5;12mvia[39m[38;5;12m [39m[38;5;12mMQTT.[39m
[38;5;12m- [39m[38;5;14m[1mESPEasy[0m[38;5;12m (https://github.com/letscontrolit/ESPEasy) - Easily turn ESP modules into multifunction sensor devices for home automation systems.[39m
[38;5;12m- [39m[38;5;14m[1mSonoff-Homekit[0m[38;5;12m (https://github.com/Gruppio/Sonoff-Homekit) - An alternative firmware for Sonoff devices (and other 8266 devices) which allows control through Apple's Homekit.[39m
[38;5;12m- [39m[38;5;14m[1mDoorsignEPD[0m[38;5;12m (https://github.com/jamct/DoorsignEPD) - A smart doorsign with an E-Paper display using the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mEPaperWeatherDisplay[0m[38;5;12m (https://github.com/henri98/esp32-e-paper-weatherdisplay) - A very cute e-ink weather display using the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mHomePoint[0m[38;5;12m (https://github.com/sieren/Homepoint) - Control MQTT/HomeKit smart home devices from an ESP32-powered screen.[39m
[38;5;12m- [39m[38;5;14m[1mopenHASP[0m[38;5;12m (https://www.openhasp.com/) - Control your home automation devices from a customizable touchscreen UI connected via MQTT.[39m
[38;5;12m- [39m[38;5;14m[1mSuperGreenOS[0m[38;5;12m (https://github.com/supergreenlab/SuperGreenOS) - A full-featured home farming automation software for the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mCanAirIO[0m[38;5;12m (https://github.com/kike-canaries/canairio_firmware#canairio-firmware) - Citizen science project that uses mobile and fixed stations to measure air quality with ESP32 and smartphones.[39m

[38;2;255;187;0m[4mInfoSec[0m
[38;5;12m- [39m[38;5;14m[1mESP32-BLECollector[0m[38;5;12m (https://github.com/tobozo/ESP32-BLECollector) - A wardriving device which displays BLE devices and collects data from them, all in a nice screen interface.[39m
[38;5;12m- [39m[38;5;14m[1mESP32Marauder[0m[38;5;12m (https://github.com/justcallmekoko/ESP32Marauder) - An integrated suite of offensive and defensive tools for WiFi and Bluetooth.[39m
[38;5;12m- [39m[38;5;14m[1mArduinoPcap[0m[38;5;12m (https://github.com/spacehuhn/ArduinoPcap) - A library which allows generation of .pcap files with network traffic, for both ESP's.[39m
[38;5;12m- [39m[38;5;14m[1mWiFi Satellite[0m[38;5;12m (https://hackaday.io/project/28831-wifi-satellite-34c3) - A giant Wifi "satellite" that can monitor all 14 2.4Ghz channels using, well, 14 ESP32s.[39m
[38;5;12m- [39m[38;5;14m[1mESP8266 Deauther[0m[38;5;12m (https://github.com/spacehuhn/esp8266_deauther) - A very cool pseudojammer (deauther) of Wifi networks that uses the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mPacketMonitor[0m[38;5;12m (https://github.com/spacehuhn/PacketMonitor32) - A beautiful OLED monitor for packet activity in a WiFi channel. Two versions for each ESP.[39m
[38;5;12m- [39m[38;5;14m[1mWiFiDuck[0m[38;5;12m (https://github.com/spacehuhn/WiFiDuck) - A wireless-enabled keystroke injector, analogous, but even more awesome than the Rubber Ducky.[39m
[38;5;12m- [39m[38;5;14m[1mESP8266 Beacon Spam[0m[38;5;12m (https://github.com/spacehuhn/esp8266_beaconSpam) - Want to confuse people? This device creates hundreds of fake WiFi networks.[39m
[38;5;12m- [39m[38;5;14m[1mDeauthDetector[0m[38;5;12m (https://github.com/spacehuhn/DeauthDetector) - A small device that shines a light if it detects a WiFi deauth attack. Made by the same guy as the last six projects.[39m

[38;2;255;187;0m[4mBiomedical[0m
[38;5;12m- [39m[38;5;14m[1mHeartyPatch[0m[38;5;12m (https://heartypatch.protocentral.com/) - A wearable BLE and WiFi connected ECG-HR patch which uses the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mHealthyPi v4[0m[38;5;12m (https://www.crowdsupply.com/protocentral/healthypi-v4-unplugged) - An amazing open source vital signs monitor that can monitor ECG, respiration, pulse oximetry and body temperature, all run by an ESP32.[39m

[38;2;255;187;0m[4mLoRa[0m

[38;5;12m- [39m[38;5;14m[1mMeshtastic[0m[38;5;12m (https://www.meshtastic.org/) - ESP32 LoRA boards as secure, long battery life, mesh GPS communicators.[39m
[38;5;12m- [39m[38;5;14m[1mESP32-Paxcounter[0m[38;5;12m (https://github.com/cyberman54/ESP32-Paxcounter#esp32-paxcounter) - Wifi & Bluetooth driven, LoRaWAN enabled, battery powered mini Paxcounter built on cheap ESP32 LoRa IoT boards.[39m
[38;5;12m- [39m[38;5;14m[1mDisaster Radio[0m[38;5;12m (https://disaster.radio/) - A disaster-resilient communications network powered by the sun.[39m

[38;2;255;187;0m[4mMusic and Audio[0m

[38;5;12m- [39m[38;5;14m[1mAlles[0m[38;5;12m (https://github.com/bwhitman/alles) - A many speaker distributed music synthesizer using UDP multicast over WiFi, modeled after the alles machine/AMY.[39m
[38;5;12m- [39m[38;5;14m[1mESP32-Radio[0m[38;5;12m (https://github.com/Edzelf/ESP32-Radio) - Internet radio based on ESP32, VS1053 and a TFT screen.[39m
[38;5;12m- [39m[38;5;14m[1mESPuino[0m[38;5;12m (https://github.com/biologist79/ESPuino) - RFID-controlled music player powered by ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mKnobby[0m[38;5;12m (https://github.com/quadule/knobby) - A handheld Spotify remote that encourages you to explore unfamiliar music.[39m
[38;5;12m- [39m[38;5;14m[1mPedalinoMini[0m[38;5;12m (https://github.com/alf45tar/PedalinoMini) - A wireless MIDI pedal controller for guitarists, built with the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mSqueezelite-esp32[0m[38;5;12m (https://github.com/sle118/squeezelite-esp32) - Streaming audio receiver with multi-room sync, AirPlay, Bluetooth, hardware buttons, display and more.[39m
[38;5;12m- [39m[38;5;14m[1mThingPulse esp8266-spotify-remote[0m[38;5;12m (https://github.com/ThingPulse/esp8266-spotify-remote) - Control your Spotify player from a ESP8266 with color touch display.[39m

[38;2;255;187;0m[4mSmartwatches[0m

[38;5;12m- [39m[38;5;14m[1mmutantW_V1[0m[38;5;12m (https://mutantcybernetics.com/mutantW_V1.html) - An ESP32 based open source smartwatch with 1.7 inch display, WiFi, Bluetooth, NeoPixel and vibration.[39m
[38;5;12m- [39m[38;5;14m[1mOpen SmartWatch[0m[38;5;12m (https://open-smartwatch.github.io/) - A FOSS smartwatch with GPS, an inertial unit and an extremely cool 3D-printed case.[39m
[38;5;12m- [39m[38;5;14m[1mStickWatch[0m[38;5;12m (https://github.com/eggfly/StickWatch) - A smartwatch module based on the M5Stick, using the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mWatchy[0m[38;5;12m (https://watchy.sqfmi.com) - An open source e-paper watch with lots of options for customization.[39m

[38;2;255;187;0m[4mOthers[0m
[38;5;12m- [39m[38;5;14m[1mSoftRF[0m[38;5;12m (https://github.com/lyusupov/SoftRF) - A DIY aviation proximity awareness system that can be used in UAV projects.[39m
[38;5;12m- [39m[38;5;14m[1mRetro ESP32[0m[38;5;12m (https://github.com/retro-esp32/RetroESP32) - An extremely cool launcher for the Odroid Go (with the ESP32), which allows emulating several retro consoles.[39m
[38;5;12m- [39m[38;5;14m[1mDroneBridge[0m[38;5;12m (https://github.com/DroneBridge/ESP32) - An implementation of DroneBridge, a signal link for drones and UAV's on the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mE-TKT[0m[38;5;12m (https://github.com/andreisperid/E-TKT) - An ESP32 powered DIY label maker that mixes both old fashioned and contemporary technology.[39m
[38;5;12m- [39m[38;5;14m[1mFreeTouchDeck[0m[38;5;12m (https://github.com/DustinWatts/FreeTouchDeck) - Open source touch macropad and stream control deck with built-in web configurator.[39m
[38;5;12m- [39m[38;5;14m[1mSmartSpin2k[0m[38;5;12m (https://github.com/doudar/SmartSpin2k) - Transform your spin bike into a smart trainer with automatic resistance knob control in fitness apps like Zwift.[39m
[38;5;12m- [39m[38;5;14m[1mWirelessPrinting[0m[38;5;12m (https://github.com/probonopd/WirelessPrinting) - Print wirelessly from Cura, PrusaSlicer or Slic3r to your 3D printer connected to an ESP module.[39m
[38;5;12m- [39m[38;5;14m[1mWLED[0m[38;5;12m (https://kno.wled.ge/) - Control many types of RGB(W) LED strips with an ESP8266 or ESP32 over WiFi.[39m

[38;2;255;187;0m[4mLibraries[0m
[38;5;12m- [39m[38;5;14m[1mWasm3[0m[38;5;12m (https://github.com/wasm3/wasm3) - A lightning fast WebAssembly interpreter designed for embedded devices, compatible with both ESP's.[39m
[38;5;12m- [39m[38;5;14m[1mHomie8266[0m[38;5;12m (https://github.com/marvinroger/homie-esp8266) - Framework implementation of the Homie protocol for the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mESP-Dash[0m[38;5;12m (https://github.com/ayushsharma82/ESP-DASH) - Beautiful and fast framework for creating remote dashboards in the 8266/32. No internet required.[39m
[38;5;12m- [39m[38;5;14m[1mESP_mqtt[0m[38;5;12m (https://github.com/tuanpmt/esp_mqtt) - MQTT helper library for the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mGUIslice[0m[38;5;12m (https://github.com/ImpulseAdventure/GUIslice) - A drag and drop GUI framework for several devices and screen controllers. Compatible with 8266 and 32.[39m
[38;5;12m- [39m[38;5;14m[1mLVGL[0m[38;5;12m (https://lvgl.io) - An open-source graphics library providing everything you need to create embedded GUIs with easy-to-use graphical elements, beautiful visual effects and low memory footprint.[39m
[38;5;12m- [39m[38;5;14m[1mMicroWebSrv2[0m[38;5;12m (https://github.com/jczic/MicroWebSrv2) - A very powerful MicroPython web server which can be used in the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mIRremoteESP8266[0m[38;5;12m (https://github.com/markszabo/IRremoteESP8266) - Emit and receive IR signals in the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mesphomelib[0m[38;5;12m (https://github.com/OttoWinter/esphomelib) - Framework to integrate with HomeAssistant in the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mTTS[0m[38;5;12m (https://github.com/jscrane/TTS) - A somehow good text to speech library for several Arduino devices, both ESP's included.[39m
[38;5;12m- [39m[38;5;14m[1mFree802.11[0m[38;5;12m (https://github.com/Jeija/esp32free80211) - Library to emit arbitrary 802.11 signals with the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mKoyn[0m[38;5;12m (https://github.com/elkrem/koyn) - A decentralized Bitcoin library for the ESP32 and the ESP8266.[39m
[38;5;12m- [39m[38;5;14m[1mTFTLibrary[0m[38;5;12m (https://github.com/loboris/ESP32_TFT_library) - TFT compatibility for the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mUTFT-ESP[0m[38;5;12m (https://github.com/gnulabis/UTFT-ESP) - UTFT Support for the ESP32/8266.[39m
[38;5;12m- [39m[38;5;14m[1mESPAudio[0m[38;5;12m (https://github.com/earlephilhower/ESP8266Audio) - Library for playing a diverse range of audio formats in the ESP8266/ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mESP32-audioI2S[0m[38;5;12m (https://github.com/schreibfaul1/ESP32-audioI2S) - Plays mp3, m4a and wav files from SD card or stream via I2S interface.[39m
[38;5;12m- [39m[38;5;14m[1mAsyncTCP[0m[38;5;12m (https://github.com/me-no-dev/ESPAsyncTCP) - Asynchronous TCP Library for both the 8266 and the 32.[39m
[38;5;12m- [39m[38;5;14m[1mESP-HomeKit[0m[38;5;12m (https://github.com/maximkulkin/esp-homekit) - Homekit implementation for 8266 on RTOS.[39m
[38;5;12m- [39m[38;5;14m[1mHomeSpan[0m[38;5;12m (https://github.com/HomeSpan/HomeSpan) - A robust and extremely easy-to-use Arduino library for creating your own ESP32-based HomeKit devices.[39m
[38;5;12m- [39m[38;5;14m[1mESPHelper[0m[38;5;12m (https://github.com/ItKindaWorks/ESPHelper) - MQTT and Wi-fi automation-oriented library for the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mESPHelper/32[0m[38;5;12m (https://github.com/ItKindaWorks/ESPHelper32) - Port of the ESPHelper library for the 32.[39m
[38;5;12m- [39m[38;5;14m[1mESP8266Wifi[0m[38;5;12m (https://github.com/ekstrand/ESP8266wifi) - Simple Arduino Wifi library for the 8266.[39m
[38;5;12m- [39m[38;5;14m[1mWiFiESP[0m[38;5;12m (https://github.com/bportaluri/WiFiEsp) - Arduino library for Wifi management, client/server for 8266 board.[39m
[38;5;12m- [39m[38;5;14m[1mTinyGSM[0m[38;5;12m (https://github.com/vshymanskyy/TinyGSM) - A quick and simple Arduino library for interaction with GSM modules which can also control the 8266 through AT commands.[39m
[38;5;12m- [39m[38;5;14m[1mmJS[0m[38;5;12m (https://github.com/cesanta/mjs) - A lightweight and restricted JS engine that is used by MongooseOS, compatible on the 32 and 8266.[39m
[38;5;12m- [39m[38;5;14m[1mESPUI[0m[38;5;12m (https://github.com/s00500/ESPUI) - A simply library for making interactive web interfaces for both ESP's.[39m
[38;5;12m- [39m[38;5;14m[1mESP32 ePaper[0m[38;5;12m (https://github.com/loboris/ESP32_ePaper_example) - A full-featured library for using ePaper modules with the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mTinyUPnP[0m[38;5;12m (https://github.com/ofekp/TinyUPnP) - A lightweight UPnP IGD library for automatic port forwarding on the 8266 and 32.[39m
[38;5;12m- [39m[38;5;14m[1mEsp32SSHClient[0m[38;5;12m (https://github.com/J-Rios/Arduino-esp32sshclient) - A library that implements a SSH client in the ESP32.[39m
[38;5;12m- [39m[38;5;14m[1mpainlessMesh[0m[38;5;12m (https://github.com/gmag11/painlessMesh) - A library that takes care of the particulars of creating a simple mesh network using ESP8266 and ESP32 hardware.[39m
[38;5;12m-[39m[38;5;12m [39m[38;5;14m[1mWifiEspNow[0m[38;5;12m [39m[38;5;12m(https://github.com/yoursunny/WifiEspNow)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mArduino[39m[38;5;12m [39m[38;5;12mlibrary[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;14m[1mESP-NOW[0m[38;5;12m [39m[38;5;12m(https://docs.espressif.com/projects/esp-idf/en/latest/esp32/api-reference/network/esp_now.html),[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mconnectionless[39m[38;5;12m [39m[38;5;12mWiFi[39m[38;5;12m [39m[38;5;12mcommunication[39m[38;5;12m [39m[38;5;12mprotocol[39m[38;5;12m [39m[38;5;12mdefined[39m[38;5;12m [39m
[38;5;12mby[39m[38;5;12m [39m[38;5;14m[1mEspressif[0m[38;5;12m [39m[38;5;12m(https://github.com/espressif).[39m
[38;5;12m- [39m[38;5;14m[1mgo-mcu[0m[38;5;12m (https://github.com/matiasinsaurralde/go-mcu) - Golang package for interacting with NodeMCU-based boards.[39m
[38;5;12m- [39m[38;5;14m[1mCanAirIO SensorLib[0m[38;5;12m (https://github.com/kike-canaries/canairio_sensorlib#canairio-air-quality-sensors-library) - ESP32/8266 library with auto-configuration of multiple PM2.5, CO2 and environment sensors.[39m
[38;5;12m- [39m[38;5;14m[1mDhyara[0m[38;5;12m (https://github.com/neel/dhyara) - A C/C++ library for making a Mobile Ad hoc Network (MANET) using ESP Now.[39m
[38;5;12m- [39m[38;5;14m[1mLedFx[0m[38;5;12m (https://github.com/LedFx/LedFx) - A library for using audio input to create realtime light shows. LedFx can control multiple devices and works great with cheap ESP8266 nodes.[39m
