[38;5;12m                                                                                                                [39m[38;2;255;187;0m[1m[4mAwesome MQTT[0m

[38;5;14m[1m![0m[38;5;12mAwesome[39m[38;5;14m[1m (https://cdn.rawgit.com/sindresorhus/awesome/d7305f38d29fed78fa85652e3a63e154dd8e8829/media/badge.svg)[0m[38;5;12m (https://github.com/sindresorhus/awesome)[39m

[38;5;11m[1m▐[0m[38;5;12m [39m[38;5;12mA curated list of MQTT related stuff.[39m

[38;5;12mMQTT[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mlightweight[39m[38;5;12m [39m[38;5;12mclient-server[39m[38;5;12m [39m[38;5;12mpublish/subscribe[39m[38;5;12m [39m[38;5;12mmessaging[39m[38;5;12m [39m[38;5;12mprotocol,[39m[38;5;12m [39m[38;5;12moptimized[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;12mhigh-latency[39m[38;5;12m [39m[38;5;12mor[39m[38;5;12m [39m[38;5;12munreliable[39m[38;5;12m [39m[38;5;12mnetworks.[39m[38;5;12m [39m[38;5;12mThis[39m[38;5;12m [39m[38;5;12mprotocol[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mgood[39m[38;5;12m [39m[38;5;12mchoice[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;12mInternet[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mThings[39m[38;5;12m [39m[38;5;12mapplications,[39m[38;5;12m [39m[38;5;12mTelemetry,[39m[38;5;12m [39m[38;5;12mSensor[39m[38;5;12m [39m[38;5;12mNetworks,[39m[38;5;12m [39m[38;5;12mSmart[39m[38;5;12m [39m[38;5;12mMetering,[39m
[38;5;12mHome[39m[38;5;12m [39m[38;5;12mAutomation,[39m[38;5;12m [39m[38;5;12mMessaging[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mNotification[39m[38;5;12m [39m[38;5;12mServices.[39m

[38;2;255;187;0m[4mContents[0m

[38;5;12m- [39m[38;5;14m[1mCommunity Resources[0m[38;5;12m (#community-resources)[39m
[38;5;12m- [39m[38;5;14m[1mBroker[0m[38;5;12m (#broker)[39m
[38;5;12m- [39m[38;5;14m[1mCloud[0m[38;5;12m (#cloud)[39m
[38;5;12m- [39m[38;5;14m[1mPlatforms[0m[38;5;12m (#platforms)[39m
[38;5;12m- [39m[38;5;14m[1mTools[0m[38;5;12m (#tools)[39m
[38;5;12m- [39m[38;5;14m[1mClients[0m[38;5;12m (#clients)[39m
[38;5;12m- [39m[38;5;14m[1mScripting[0m[38;5;12m (#scripting)[39m
[38;5;12m- [39m[38;5;14m[1mInterfaces[0m[38;5;12m (#interfaces)[39m
[48;5;235m[38;5;249m- **Makers** (#makers)[49m[39m[48;5;235m[38;5;249m                                                  [49m[39m
[48;5;235m[38;5;249m- **Industry** (#industry)[49m[39m[48;5;235m[38;5;249m                                              [49m[39m
[48;5;235m[38;5;249m- **Telephony, PBX** (#telephony-pbx)[49m[39m[48;5;235m[38;5;249m                                   [49m[39m
[48;5;235m[38;5;249m- **Operating System** (#operating-system)[49m[39m[48;5;235m[38;5;249m                              [49m[39m
[48;5;235m[38;5;249m- **Monitoring** (#monitoring)[49m[39m[48;5;235m[38;5;249m                                          [49m[39m
[48;5;235m[38;5;249m- **Location Tracking** (#location-tracking)[49m[39m[48;5;235m[38;5;249m                            [49m[39m
[48;5;235m[38;5;249m- **Logging** (#logging)[49m[39m[48;5;235m[38;5;249m                                                [49m[39m
[48;5;235m[38;5;249m- **Smart Home Hardware Interfaces** (#smart-home-hardware-interfaces)[49m[39m[48;5;235m[38;5;249m  [49m[39m
[48;5;235m[38;5;249m- **Smart Home Integration Software** (#smart-home-integration-software)[49m[39m
[48;5;235m[38;5;249m- **Lighting** (#lighting)[49m[39m[48;5;235m[38;5;249m                                              [49m[39m
[48;5;235m[38;5;249m- **Home Entertainment** (#home-entertainment)[49m[39m[48;5;235m[38;5;249m                          [49m[39m
[48;5;235m[38;5;249m- **Smart Metering** (#smart-metering)[49m[39m[48;5;235m[38;5;249m                                  [49m[39m
[48;5;235m[38;5;249m- **Messaging** (#messaging)[49m[39m[48;5;235m[38;5;249m                                            [49m[39m
[48;5;235m[38;5;249m- **Misc** (#misc)[49m[39m[48;5;235m[38;5;249m                                                      [49m[39m
[38;5;12m- [39m[38;5;14m[1mVisualization, Dashboards[0m[38;5;12m (#visualization-dashboards)[39m
[38;5;12m- [39m[38;5;14m[1mArchitecture, Convention[0m[38;5;12m (#architecture-convention)[39m
[38;5;12m- [39m[38;5;14m[1mSecurity, Encryption[0m[38;5;12m (#security-encryption)[39m


[38;2;255;187;0m[4mCommunity Resources[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt.org[0m[38;5;12m (https://mqtt.org/).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT community wiki[0m[38;5;12m (https://github.com/mqtt/mqtt.org/wiki).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mGoogle Groups: MQTT[0m[38;5;12m (https://groups.google.com/forum/#!forum/mqtt).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mIRC channel #mqtt on the freenode network[0m[38;5;12m (irc://irc.freenode.net/mqtt).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mA list of public brokers[0m[38;5;12m (http://moxd.io/2015/10/17/public-mqtt-brokers/).[39m

[38;2;255;187;0m[4mBlogs[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mBen Hardill[0m[38;5;12m (https://www.hardill.me.uk/wordpress/tag/mqtt/)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mDominik Obermaier[0m[38;5;12m (http://forkbomb-blog.de/category/mqtt)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mJan-Piet Mens[0m[38;5;12m (https://jpmens.net/)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mNick O'Leary[0m[38;5;12m (https://knolleary.net/)[39m

[38;2;255;187;0m[4mTalks[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mAn Introduction to MQTT: Why HTTP isn't the King of the Internet of Things[0m[38;5;12m (https://www.youtube.com/watch?v=LKz1jYngpcU) - Shinji Kim, Robert Bird - Akamai, Samsung Developer Conference 2017.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mEinführung in MQTT[0m[38;5;12m (https://www.youtube.com/watch?v=INYG4-xsa9c) - Dominik Obermaier & Jens Deters, [39m[38;5;14m[1mBuilding IoT[0m[38;5;12m (https://www.buildingiot.de/index.php) conference 2016 (German).[39m

[38;2;255;187;0m[4mBroker[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mAbly[0m[38;5;12m (https://www.ably.io/documentation/mqtt) - MQTT broker service and protocol adapter[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mActiveMQ[0m[38;5;12m (http://activemq.apache.org/) - A fast Java multiprotocol messaging and Integration Patterns server.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mAedes[0m[38;5;12m (https://github.com/moscajs/aedes) - Barebone MQTT broker that can run on any stream server, the node way.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mEmitter[0m[38;5;12m (https://github.com/emitter-io/emitter) - A distributed, scalable and fault-tolerant publish-subscribe messaging platform based on MQTT protocol and featuring message storage.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mEMQ X[0m[38;5;12m (https://github.com/emqx/emqx) - Scalable and Reliable Real-time MQTT Messaging Engine for IoT in 5G Era.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mesp_uMQTT_broker[0m[38;5;12m (https://github.com/martin-ger/esp_mqtt) - A basic MQTT Broker on the ESP8266.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhbmqtt[0m[38;5;12m (https://github.com/beerfactory/hbmqtt) - Python MQTT broker using asyncio.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHiveMQ[0m[38;5;12m (https://www.hivemq.com/) - Java MQTT Broker that supports MQTT 3.1, 3.1.1 and 5.0. Commercial and open source editions available.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhrotti[0m[38;5;12m (https://github.com/alsm/hrotti) - A MQTT broker written in Go.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mKMQTT[0m[38;5;12m (https://github.com/davidepianca98/KMQTT) - Kotlin Multiplatform MQTT broker, both embeddable and standalone.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMoquette[0m[38;5;12m (https://github.com/moquette-io/moquette) - Java MQTT lightweight broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMosca[0m[38;5;12m (http://www.mosca.io/) - Mosca is a node.js MQTT broker, which can be used Standalone or Embedded in another Node.js application.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMosquitto[0m[38;5;12m (http://mosquitto.org/) - [39m[48;2;30;30;40m[38;5;13m[3m"[0m[38;5;12mThe"[39m[38;5;14m[1m Open Source MQTT Broker. [0m
[48;5;235m[38;5;249m * **Free test server** (https://mqtt.eclipseprojects.io) hosted by the Eclipse Foundation.[49m[39m[48;5;235m[38;5;249m                                            [49m[39m
[48;5;235m[38;5;249m * **Authorization Plugin in Go** (https://github.com/iegomez/mosquitto-go-auth) supports many types of logins.[49m[39m[48;5;235m[38;5;249m                        [49m[39m
[48;5;235m[38;5;249m * **Let's Encrypt Mosquitto Docker Container** (https://hub.docker.com/r/pythonlinks/letsencrypt-mosquitto) makes it easy to encrypt. [49m[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMyQttHub[0m[38;5;12m (https://myqtthub.com) - Cloud MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMystique[0m[38;5;12m (https://github.com/TheThingsIndustries/mystique) - An extendable MQTT broker written in Go, with HTTP capabilities for observability. Implements MQTT v3.1.1.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mRabbitMQ[0m[38;5;12m (https://www.rabbitmq.com/mqtt.html) - RabbitMQ offers a MQTT Adapter.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mSurgeMQ[0m[38;5;12m (https://zhen.org/categories/surgemq/) - High Performance MQTT Server and Client Libraries in Go.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mVerneMQ[0m[38;5;12m (https://vernemq.com/) - an Apache2 licensed distributed MQTT broker, developed in Erlang.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mVert.x MQTT[0m[38;5;12m (https://github.com/vert-x3/vertx-mqtt) - Vert.x component to handle connections, communication and messages exchange with remote MQTT clients.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mWaterstream[0m[38;5;12m (https://waterstream.io/) - MQTT broker leveraging Apache Kafka as its own storage and distribution engine.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mNanoMQ[0m[38;5;12m (https://github.com/nanomq/nanomq) - A light-weight and Blazing-fast MQTT Broker for IoT Edge platform.[39m

[38;2;255;187;0m[4mCloud[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mAdafruit[0m[38;5;14m[1m [0m[38;5;14m[1mIO[0m[38;5;12m [39m[38;5;12m(https://io.adafruit.com)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mAdafruit[39m[38;5;12m [39m[38;5;12mIO[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12measiest[39m[38;5;12m [39m[38;5;12mway[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mconnect[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mproject[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12minternet.[39m[38;5;12m [39m[38;5;12mYou[39m[38;5;12m [39m[38;5;12mcan[39m[38;5;12m [39m[38;5;12measily[39m[38;5;12m [39m[38;5;12mconnect[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mproject[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mAdafruit[39m[38;5;12m [39m[38;5;12mIO[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mdevice-of-choice[39m[38;5;12m [39m[38;5;12mby[39m[38;5;12m [39m[38;5;12musing[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mprogramming[39m[38;5;12m [39m[38;5;12mlanguage[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mchoice[39m
[38;5;12m(we[39m[38;5;12m [39m[38;5;12mhave[39m[38;5;12m [39m[38;5;12mlots[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mlibraries)[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mcontrol[39m[38;5;12m [39m[38;5;12mor[39m[38;5;12m [39m[38;5;12mmonitor[39m[38;5;12m [39m[38;5;12mover[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12minternet.[39m[38;5;12m [39m[38;5;12mData[39m[38;5;12m [39m[38;5;12mstored[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mAdafruit[39m[38;5;12m [39m[38;5;12mIO[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12myours[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mmanage[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mcontrol.[39m
[38;5;12m- [39m[38;5;14m[1mAlibaba Cloud IoT Platform[0m[38;5;12m (https://www.alibabacloud.com/product/iot) - Provides secure and reliable communication between devices and the IoT Platform which allows you to manage a large number of devices on a single IoT Platform.[39m
[38;5;12m-[39m[38;5;12m [39m[38;5;14m[1mAWS[0m[38;5;14m[1m [0m[38;5;14m[1mIoT[0m[38;5;14m[1m [0m[38;5;14m[1mCore[0m[38;5;12m [39m[38;5;12m(https://aws.amazon.com/iot-core/?nc1=h_ls)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mAWS[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mCore[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mmanaged[39m[38;5;12m [39m[38;5;12mcloud[39m[38;5;12m [39m[38;5;12mservice[39m[38;5;12m [39m[38;5;12mthat[39m[38;5;12m [39m[38;5;12mlets[39m[38;5;12m [39m[38;5;12mconnected[39m[38;5;12m [39m[38;5;12mdevices[39m[38;5;12m [39m[38;5;12measily[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12msecurely[39m[38;5;12m [39m[38;5;12minteract[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mcloud[39m[38;5;12m [39m[38;5;12mapplications[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mother[39m[38;5;12m [39m[38;5;12mdevices.[39m[38;5;12m [39m[38;5;12mAWS[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mCore[39m[38;5;12m [39m[38;5;12mcan[39m[38;5;12m [39m[38;5;12msupport[39m[38;5;12m [39m[38;5;12mbillions[39m[38;5;12m [39m
[38;5;12mof[39m[38;5;12m [39m[38;5;12mdevices[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mtrillions[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mmessages,[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mcan[39m[38;5;12m [39m[38;5;12mprocess[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mroute[39m[38;5;12m [39m[38;5;12mthose[39m[38;5;12m [39m[38;5;12mmessages[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mAWS[39m[38;5;12m [39m[38;5;12mendpoints[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mother[39m[38;5;12m [39m[38;5;12mdevices[39m[38;5;12m [39m[38;5;12mreliably[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12msecurely.[39m[38;5;12m [39m[38;5;12mWith[39m[38;5;12m [39m[38;5;12mAWS[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mCore,[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mapplications[39m[38;5;12m [39m[38;5;12mcan[39m[38;5;12m [39m[38;5;12mkeep[39m[38;5;12m [39m[38;5;12mtrack[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mcommunicate[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mall[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mdevices,[39m[38;5;12m [39m
[38;5;12mall[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12mtime,[39m[38;5;12m [39m[38;5;12meven[39m[38;5;12m [39m[38;5;12mwhen[39m[38;5;12m [39m[38;5;12mthey[39m[38;5;12m [39m[38;5;12maren’t[39m[38;5;12m [39m[38;5;12mconnected.[39m
[38;5;12m-[39m[38;5;12m [39m[38;5;14m[1mAzure[0m[38;5;14m[1m [0m[38;5;14m[1mIoT[0m[38;5;14m[1m [0m[38;5;14m[1mHub[0m[38;5;12m [39m[38;5;12m(https://azure.microsoft.com/en-us/services/iot-hub/)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mEnable[39m[38;5;12m [39m[38;5;12mhighly[39m[38;5;12m [39m[38;5;12msecure[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mreliable[39m[38;5;12m [39m[38;5;12mcommunication[39m[38;5;12m [39m[38;5;12mbetween[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mapplication[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12mdevices[39m[38;5;12m [39m[38;5;12mit[39m[38;5;12m [39m[38;5;12mmanages.[39m[38;5;12m [39m[38;5;12mAzure[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mHub[39m[38;5;12m [39m[38;5;12mprovides[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mcloud-hosted[39m[38;5;12m [39m[38;5;12msolution[39m[38;5;12m [39m[38;5;12mbackend[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m
[38;5;12mconnect[39m[38;5;12m [39m[38;5;12mvirtually[39m[38;5;12m [39m[38;5;12many[39m[38;5;12m [39m[38;5;12mdevice.[39m[38;5;12m [39m[38;5;12mExtend[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12msolution[39m[38;5;12m [39m[38;5;12mfrom[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12mcloud[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12medge[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mper-device[39m[38;5;12m [39m[38;5;12mauthentication,[39m[38;5;12m [39m[38;5;12mbuilt-in[39m[38;5;12m [39m[38;5;12mdevice[39m[38;5;12m [39m[38;5;12mmanagement,[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mscaled[39m[38;5;12m [39m[38;5;12mprovisioning.[39m
[38;5;12m- [39m[38;5;14m[1mCloudMQTT[0m[38;5;12m (https://www.cloudmqtt.com/) - Hosted message broker for the Internet of Things. Perfectly configured and optimized message queues for IoT, ready in seconds.[39m
[38;5;12m- [39m[38;5;14m[1mEMQ X MQTT Cloud[0m[38;5;12m (https://cloud.emqx.io/) - A secure, reliable MQTT cloud service with best pratices from EMQ team.[39m
[38;5;12m- [39m[38;5;14m[1mflespi[0m[38;5;12m (https://flespi.com/mqtt-broker) - Free and secure cloud MQTT broker with private namespaces, MQTT 3.1.1 and MQTT 5.0 support and gorgeous limits.[39m
[38;5;12m-[39m[38;5;12m [39m[38;5;14m[1mGoogle[0m[38;5;14m[1m [0m[38;5;14m[1mCloud[0m[38;5;14m[1m [0m[38;5;14m[1mIoT[0m[38;5;12m [39m[38;5;12m(https://cloud.google.com/solutions/iot/)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mGoogle[39m[38;5;12m [39m[38;5;12mCloud[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mcomplete[39m[38;5;12m [39m[38;5;12mset[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mtools[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mconnect,[39m[38;5;12m [39m[38;5;12mprocess,[39m[38;5;12m [39m[38;5;12mstore,[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12manalyze[39m[38;5;12m [39m[38;5;12mdata[39m[38;5;12m [39m[38;5;12mboth[39m[38;5;12m [39m[38;5;12mat[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12medge[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12min[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12mcloud.[39m[38;5;12m [39m[38;5;12mThe[39m[38;5;12m [39m[38;5;12mplatform[39m[38;5;12m [39m[38;5;12mconsists[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mscalable,[39m[38;5;12m [39m[38;5;12mfully-managed[39m[38;5;12m [39m
[38;5;12mcloud[39m[38;5;12m [39m[38;5;12mservices;[39m[38;5;12m [39m[38;5;12man[39m[38;5;12m [39m[38;5;12mintegrated[39m[38;5;12m [39m[38;5;12msoftware[39m[38;5;12m [39m[38;5;12mstack[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;12medge/on-premises[39m[38;5;12m [39m[38;5;12mcomputing[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mmachine[39m[38;5;12m [39m[38;5;12mlearning[39m[38;5;12m [39m[38;5;12mcapabilities[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;12mall[39m[38;5;12m [39m[38;5;12myour[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mneeds.[39m
[38;5;12m-[39m[38;5;12m [39m[38;5;14m[1mHiveMQ[0m[38;5;14m[1m [0m[38;5;14m[1mCloud[0m[38;5;12m [39m[38;5;12m(https://www.hivemq.com/cloud/)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mHiveMQ[39m[38;5;12m [39m[38;5;12mCloud[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mfully[39m[38;5;12m [39m[38;5;12mmanaged[39m[38;5;12m [39m[38;5;12mMQTT[39m[38;5;12m [39m[38;5;12mplatform[39m[38;5;12m [39m[38;5;12mthat[39m[38;5;12m [39m[38;5;12mconnects[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mdevices[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12many[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mcloud[39m[38;5;12m [39m[38;5;12mplatform.[39m[38;5;12m [39m[38;5;12mA[39m[38;5;12m [39m[38;5;12mcloud[39m[38;5;12m [39m[38;5;12mnative[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mmessaging[39m[38;5;12m [39m[38;5;12mplatform[39m[38;5;12m [39m[38;5;12mthat[39m[38;5;12m [39m[38;5;12msimplifies[39m[38;5;12m [39m[38;5;12mreliable[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mscalable[39m[38;5;12m [39m[38;5;12mIoT[39m[38;5;12m [39m[38;5;12mdevice[39m[38;5;12m [39m
[38;5;12mconnectivity.[39m
[38;5;12m- [39m[38;5;14m[1mIBM WATSON[0m[38;5;12m (https://www.ibm.com/watson) - With Watson, you can bring AI tools and apps to your data wherever it resides – whether it's on IBM Cloud, AWS, Azure, Google, or your own private cloud platform.[39m

[38;2;255;187;0m[4mPlatforms[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmainflux[0m[38;5;12m (https://www.mainflux.com/) - device management, data aggregation, data management, data analytics,connectivity and message routing and event management. Supported by Linux Software Foundation.[39m
[38;5;12mCore analytics[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mthingsboard[0m[38;5;12m (https://thingsboard.io/) - Device management, data collection, processing, event management, and visualization for your IoT projects.[39m


[38;2;255;187;0m[4mTools[0m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhivemq-mqtt-web-client[0m[38;5;12m (https://github.com/hivemq/hivemq-mqtt-web-client) - Browser-based MQTT client that utilizes MQTT over websockets. [39m[38;5;14m[1mDirect Link[0m[38;5;12m (http://www.hivemq.com/demos/websocket-client/)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mimqtt[0m[38;5;12m (https://github.com/shafreeck/imqtt) - Interactive MQTT packet manipulation shell based on IPython.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mIoT-Testware[0m[38;5;12m (https://projects.eclipse.org/projects/technology.iottestware) - The Eclipse IoT-Testware is a collection of conformance test suites for IoT protocols enriched with additional tools for fuzzing and performance testing.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmoxy[0m[38;5;12m (https://github.com/jvermillard/moxy) - A Golang MQTT proxy providing useful output traces to monitor and troubleshoot your MQTT communications.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT Board[0m[38;5;12m (https://github.com/flespi-software/MQTT-Board) - Open-source diagnostic-oriented MQTT client tool.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-admin[0m[38;5;12m (https://github.com/hobbyquaker/mqtt-admin/) - Web based MQTT frontend. [39m[38;5;14m[1mDirect Link[0m[38;5;12m (https://hobbyquaker.github.io/mqtt-admin/).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-benchmark[0m[38;5;12m (https://github.com/chirino/mqtt-benchmark) - A benchmarking tool for MQTT Servers.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT CLI[0m[38;5;12m (https://github.com/hivemq/mqtt-cli) - A command line interface for connecting various MQTT clients supporting MQTT 5.0 and 3.1.1.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-client[0m[38;5;12m (https://github.com/sdeancos/mqtt-client) - A Simple MQTT Client command line (Python) (use paho lib)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-forget[0m[38;5;12m (https://github.com/hobbyquaker/mqtt-forget) - Command line tool to remove retained MQTT topics by wildcard.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-fuzz[0m[38;5;12m (https://github.com/F-Secure/mqtt_fuzz) - A simple fuzzer for the MQTT protocol.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-malaria[0m[38;5;12m (https://github.com/etactica/mqtt-malaria) - scalability and load testing utilities for MQTT environments.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-mirror[0m[38;5;12m (https://github.com/4nte/mqtt-mirror) - Mirror MQTT traffic from one broker to another. Available as a CLI tool, helm chart or docker image.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT-PWN[0m[38;5;12m (https://github.com/akamai-threat-research/mqtt-pwn) - MQTT-PWN intends to be a one-stop-shop for IoT Broker penetration-testing and security assessment operations.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt_recorder[0m[38;5;12m (https://github.com/rpdswtk/mqtt_recorder) - Simple cli tool for recording and replaying MQTT messages.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-shell[0m[38;5;12m (https://github.com/pidster-dot-org/mqtt-shell) - A simple interactive shell for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-spy[0m[38;5;12m (http://kamilfb.github.io/mqtt-spy/) - Java based MQTT frontend. Supports scripting.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt_tree[0m[38;5;12m (https://github.com/poggenpower/mqtt_tree) - Displays all Topics in an expandable tree, helps to get an overview if you have a lot of clients publishing. (python, tkinter)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-utils[0m[38;5;12m (https://github.com/dsell/mqtt-utils) - A collection of MQTT utilities.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-wall[0m[38;5;12m (https://github.com/bastlirna/mqtt-wall) - Subscription only web-based client – like Twitter wall for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-wildcard[0m[38;5;12m (https://github.com/hobbyquaker/mqtt-wildcard) - Node.js Module to match a MQTT Topic against wildcards.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT.fx[0m[38;5;12m (https://mqttfx.jensd.de/) - MQTT.fx is a MQTT Client written in Java based on Eclipse Paho. Supports scripting.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttcli[0m[38;5;12m (https://github.com/shirou/mqttcli) - MQTT Client for shell scripting.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTTInspector[0m[38;5;12m (https://github.com/ckrey/MQTTInspector) - A general MQTT testing app for iOS (iPhone and iPad).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTTLens[0m[38;5;12m (https://chrome.google.com/webstore/detail/mqttlens/hemojaaeigabkbcookmlgmdigohjobjm) - A Google Chrome application, which connects to a MQTT broker and is able to subscribe and publish to MQTT topics.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT Explorer[0m[38;5;12m (https://mqtt-explorer.com/) - Tool to visualize your MQTT topics in a topic hierarchy, a MQTT swiss-army knife.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT TUI[0m[38;5;12m (https://github.com/EdJoPaTo/mqttui) - Simple lightweight terminal based MQTT monitor and publisher.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mPython MQTT Client Shell[0m[38;5;12m (https://github.com/bapowell/python-mqtt-client-shell) - a text console-based, interactive shell for exercising various tasks associated with MQTT client communications.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mSimpleMQTT[0m[38;5;12m (https://simplemqtt.theoi.de/) - A Slack app to send messages from Slack to MQTT brokers with slash commands.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mWireshark-MQTT[0m[38;5;12m (https://github.com/menudoproblema/Wireshark-MQTT) - MQTT dissector for Wireshark.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mVSMQTT[0m[38;5;12m (hhttps://github.com/rpdswtk/vsmqtt) - Simple MQTT client integrated in Visual Studio Code.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTTX[0m[38;5;12m (https://github.com/emqx/MQTTX) - MQTTX is a cross-platform MQTT desktop client open sourced by EMQ, which supports macOS, Linux, and Windows.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT-Tiles[0m[38;5;12m (https://github.com/flespi-software/MQTT-Tiles) - MQTT-based IoT dashboard visualization tool. Allows easy dashboards sharing. Works with any MQTT broker supporting the WSS protocol.[39m

[38;2;255;187;0m[4mClients[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1maiomqtt[0m[38;5;12m (https://github.com/mossblaser/aiomqtt) - Async Python MQTT client based on paho-mqtt.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mCocoaMQTT[0m[38;5;12m (https://github.com/emqx/CocoaMQTT) - MQTT for iOS and OS X written with Swift.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1memqttc[0m[38;5;12m (https://github.com/emqx/emqtt) - Asynchronous Erlang MQTT Client.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mgmqtt[0m[38;5;12m (https://github.com/wialon/gmqtt) - Python MQTT v5.0 client (asyncio-based).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhbmqtt[0m[38;5;12m (https://github.com/beerfactory/hbmqtt) - Python MQTT client using asyncio.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhivemq-mqtt-client[0m[38;5;12m (https://github.com/hivemq/hivemq-mqtt-client) - High-performance Java MQTT client library with different API flavours for MQTT 5.0 and 3.1.1.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHulaaki[0m[38;5;12m (https://github.com/suvash/hulaaki) - An Elixir library for clients communicating with MQTT brokers.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mluamqtt[0m[38;5;12m (https://github.com/xHasKx/luamqtt/) - Pure-lua MQTT v3.1.1 and v5.0 client.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMachine Head[0m[38;5;12m (https://github.com/clojurewerkz/machine_head) - A Clojure MQTT Client.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMiniMQTT[0m[38;5;12m (https://github.com/adafruit/Adafruit_CircuitPython_MiniMQTT) - MQTT Client Library for CircuitPython[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMIMIC MQTT Simulator[0m[38;5;12m (https://www.gambitcomm.com/site/mqttsimulator.php) - Simulate up to 100,000 MQTT clients per server for development/testing/deployment of IoT applications.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMoscapsule[0m[38;5;12m (https://github.com/flightonary/Moscapsule) - MQTT Client for iOS written in Swift.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMosquitto-PHP[0m[38;5;12m (https://github.com/mgdm/Mosquitto-PHP) - A wrapper for the Mosquitto MQTT client library for PHP.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt_cpp[0m[38;5;12m (https://github.com/redboltz/mqtt_cpp) - MQTT client for C++14 based on Boost.Asio.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt_lua[0m[38;5;12m (http://geekscape.github.io/mqtt_lua/) - MQTT Client library for the Lua language.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT-C[0m[38;5;12m (https://github.com/LiamBindle/MQTT-C) - A portable MQTT C client for embedded systems and PCs alike.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT-Client-Framework[0m[38;5;12m (https://github.com/novastone-media/MQTT-Client-Framework) - iOS, OSX, tvOS native ObjectiveC MQTT Client Framework.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-client[0m[38;5;12m (https://github.com/centamiv/mqtt-client) - A Polymer Web Component that implements a MQTT client (uses Paho mqttws31.js).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-elements[0m[38;5;12m (https://github.com/mqttjs/mqtt-elements) - Polymer elements for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-rs[0m[38;5;12m (https://github.com/zonyitoo/mqtt-rs) - MQTT protocol library for Rust.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-stats[0m[38;5;12m (https://github.com/gambitcomminc/mqtt-stats) - Subscriber client to monitor MQTT Topic Statistics[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-wrapper[0m[38;5;12m (https://www.webcomponents.org/element/hobbyquaker/mqtt-wrapper/elements/mqtt-wrapper) - Polymer Element that wraps other Elements and links them to MQTT topics.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt.dart[0m[38;5;12m (https://github.com/jnguillerme/mqtt.dart) - Dart MQTT client.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT.js[0m[38;5;12m (https://github.com/mqttjs) - MQTT client for Node.js.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt[0m[38;5;12m (https://github.com/jeffallen/mqtt) - MQTT Clients, Servers and Load Testers in Go.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttex[0m[38;5;12m (https://github.com/alfert/mqttex) - MQTT implementation in Elixir.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTTKit[0m[38;5;12m (https://github.com/mobile-web-messaging/MQTTKit) - MQTT Objective-C client for iOS.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt_monitor[0m[38;5;12m (https://github.com/filipsPL/mqtt-monitor) - simple and lightweight console moniotor for mqtt topics, with eye-candies, in python 3.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mPaho[0m[38;5;12m (http://www.eclipse.org/paho/) - Open source client implementations (C/C++, Java, Python, Javascript, Go, C#).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mpubsubclient[0m[38;5;12m (https://github.com/knolleary/pubsubclient) - A client library for the Arduino Ethernet Shield that provides support for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mruby-mqtt[0m[38;5;12m (https://github.com/njh/ruby-mqtt) - Pure Ruby gem that implements the MQTT protocol.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mrumqtt[0m[38;5;12m (https://github.com/AtherEnergy/rumqtt) - A fast, lock free pure Rust MQTT client.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mtcl-mqtt[0m[38;5;12m (https://github.com/Tingenek/tcl-mqtt) - Small library to connect to a MQTT broker. Very, very basic.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mTMQTTClient[0m[38;5;12m (https://github.com/jamiei/Delphi-TMQTT2) - MQTT Client Library for Delphi.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mVert.x MQTT[0m[38;5;12m (https://github.com/vert-x3/vertx-mqtt) - Vert.x component that provides methods for connecting/disconnecting to a broker, publishing messages and subscribing to topics.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mwolfMQTT[0m[38;5;12m (https://www.wolfssl.com/products/wolfmqtt/) - A client implementation of the MQTT written in C for embedded use. It supports SSL/TLS via the wolfSSL library.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTTnet[0m[38;5;12m (https://github.com/chkr1011/MQTTnet) - MQTT client and broker implementations in .NET.[39m

[38;2;255;187;0m[4mScripting[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mlogic4mqtt[0m[38;5;12m (https://github.com/owagner/logic4mqtt) - Java based Logic and scripting engine for use with MQTT. Uses Java's general scripting interface, so scripts can be written in a multitude of languages like Javascript, Groovy etc.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-scripts[0m[38;5;12m (https://github.com/hobbyquaker/mqtt-scripts/) - Node.js based script runner.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mNode-RED[0m[38;5;12m (https://nodered.org/) - A visual tool for wiring the Internet of Things.[39m


[38;2;255;187;0m[4mInterfaces[0m


[38;2;255;187;0m[4mMakers[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1marduinoTemps2mqtt[0m[38;5;12m (https://github.com/matbor/arduinoTemps2mqtt) - Arduino sketch, grab One-wire Temperature's and publish to a MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mBasecamp[0m[38;5;12m (https://github.com/ct-Open-Source/Basecamp) - An Arduino library to ease the use of the ESP32 in IoT projects. See [39m[38;5;14m[1mc't Magazin 2'2018 (German)[0m[38;5;12m (https://www.heise.de/select/ct/2018/2/1515452111258448).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mdeskmate[0m[38;5;12m (https://github.com/rbaron/deskmate) - A hackable & portable MQTT-powered mini dashboard and control center.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMySensors[0m[38;5;12m (https://www.mysensors.org/) - Arduino NRF24L01 based sensor network with support for an MQTT gateway[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mpubsubclient[0m[38;5;12m (https://github.com/knolleary/pubsubclient) - A client library for the Arduino Ethernet Shield that provides support for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mRFM69-MQTT-client[0m[38;5;12m (https://github.com/computourist/RFM69-MQTT-client) - Arduino RFM69 based sensors and MQTT gateway.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mrpi2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/rpi2mqtt) - Connect a RaspberryPis GPIOs and 1-Wire Temperature Sensors to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mxbee2mqtt[0m[38;5;12m (https://github.com/xoseperez/xbee2mqtt) - XBee to MQTT gateway.[39m

[38;2;255;187;0m[4mESP[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mESP32-BLE2MQTT[0m[38;5;12m (https://github.com/shmuelzon/esp32-ble2mqtt) - BLE to MQTT bridge, exposes BLE GATT characteristics as MQTT topics for bidirectional communication.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mESP8266MQTTMesh[0m[38;5;12m (https://github.com/PhracturedBlue/ESP8266MQTTMesh) - MQTT over mesh WiFi integrated library for ESP8266[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mesp_mqtt[0m[38;5;12m (https://github.com/tuanpmt/esp_mqtt) - MQTT client library for ESP8266.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-ir-transceiver[0m[38;5;12m (https://github.com/piotrC4/mqtt-ir-transceiver) - ESP8266 based bidirectional gateway between MQTT and IR. Use with PlatformIO.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-with-micropython[0m[38;5;12m (https://docs.pycom.io/tutorials/networkprotocols/mqtt/) - Connect to MQTT with micropython and wipy/others (ESP32 inside)[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mnodemcu-gpiomqtt[0m[38;5;12m (https://github.com/hobbyquaker/nodemcu-gpiomqtt) - Lua script to connect ESP8266 GPIOs to MQTT.[39m


[38;2;255;187;0m[4mFirmwares for ESP based Devices [0m

[38;5;12mThere[39m[38;5;12m [39m[38;5;12mare[39m[38;5;12m [39m[38;5;12mmany[39m[38;5;12m [39m[38;5;12minexpensive[39m[38;5;12m [39m[38;5;12msmart[39m[38;5;12m [39m[38;5;12mhome[39m[38;5;12m [39m[38;5;12mWi-Fi[39m[38;5;12m [39m[38;5;12mdevices[39m[38;5;12m [39m[38;5;12mbased[39m[38;5;12m [39m[38;5;12mon[39m[38;5;12m [39m[38;5;12minexpensive[39m[38;5;12m [39m[38;5;12mESP8266[39m[38;5;12m [39m[38;5;12mchip[39m[38;5;12m [39m[38;5;12m_(see:[39m[38;5;12m [39m[38;5;14m[1m1[0m[38;5;12m [39m[38;5;12m(https://templates.blakadder.com/index.html),[39m[38;5;12m [39m[38;5;14m[1m2[0m[38;5;12m [39m[38;5;12m(https://github.com/xoseperez/espurna#supported-hardware),[39m[38;5;12m [39m[38;5;14m[1m3[0m[38;5;12m [39m
[38;5;12m(https://www.letscontrolit.com/wiki/index.php?title=ESP_Hardware))_.[39m[38;5;12m [39m[38;5;12mMost[39m[38;5;12m [39m[38;5;12mof[39m[38;5;12m [39m[38;5;12mthem[39m[38;5;12m [39m[38;5;12mcan[39m[38;5;12m [39m[38;5;12mbe[39m[38;5;12m [39m[38;5;12mreflashed[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mcustom[39m[38;5;12m [39m[38;5;12mfirmware.[39m
[38;5;12mHere are complete firmwares to turn them into MQTT-controlled smart home nodes:[39m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mESPEasy[0m[38;5;12m (https://www.letscontrolit.com/wiki/index.php?title=ESPEasy) - Turns ESP into a multifunction sensor device for  solutions with web-based configuration.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mESPHome[0m[38;5;12m (https://esphome.io/) - builds ESP8266/ESP32 firmware from concise YAML descriptions, uploads to and manages flashed devices.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mEspurna[0m[38;5;12m (https://github.com/xoseperez/espurna) -  firmware for ESP8266-based devices with rich web UI and ≈120 devices supported out of the box[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mOpenMQTTGateway[0m[38;5;12m [39m[38;5;12m(https://github.com/1technophile/OpenMQTTGateway)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mMQTT[39m[38;5;12m [39m[38;5;12mgateway[39m[38;5;12m [39m[38;5;12mfor[39m[38;5;12m [39m[38;5;12mESP8266,[39m[38;5;12m [39m[38;5;12mESP32,[39m[38;5;12m [39m[38;5;12mSonoff[39m[38;5;12m [39m[38;5;12mRF[39m[38;5;12m [39m[38;5;12mBridge[39m[38;5;12m [39m[38;5;12mor[39m[38;5;12m [39m[38;5;12mArduino[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mbidirectional[39m[38;5;12m [39m[38;5;12m433mhz/315mhz/868mhz,[39m[38;5;12m [39m[38;5;12mInfrared[39m[38;5;12m [39m[38;5;12mcommunications,[39m[38;5;12m [39m[38;5;12mBLE,[39m[38;5;12m [39m[38;5;12mbeacons[39m[38;5;12m [39m[38;5;12mdetection,[39m[38;5;12m [39m[38;5;12mmi[39m[38;5;12m [39m[38;5;12mflora,[39m[38;5;12m [39m[38;5;12mmi[39m[38;5;12m [39m
[38;5;12mjia,[39m[38;5;12m [39m[38;5;12mLYWSD02,[39m[38;5;12m [39m[38;5;12mLYWSD03MMC,[39m[38;5;12m [39m[38;5;12mMi[39m[38;5;12m [39m[38;5;12mScale[39m[38;5;12m [39m[38;5;12mcompatibility,[39m[38;5;12m [39m[38;5;12mSMS[39m[38;5;12m [39m[38;5;12m&[39m[38;5;12m [39m[38;5;12mLORA.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mSonoff-Tasmota[0m[38;5;12m (https://github.com/arendst/Tasmota) - Firmware for ESP8266 devices with web-based configuration. ≈500 devices supported (not only Sonoffs).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mWiFi-IoT[0m[38;5;12m (https://wifi-iot.com/p/wiki/) - ESP8266/ESP32 firmware builder. Partly in Russian. Free features are limited.[39m


[38;2;255;187;0m[4mIndustry[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mCODESYS-MQTT[0m[38;5;12m (https://github.com/stefandreyer/CODESYS-MQTT) - A MQTT client for CODESYS PLC[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mspicierModbus2mqtt[0m[38;5;12m (https://github.com/mbs38/spicierModbus2mqtt) - Modbus master which publishes register values via MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2opcua[0m[38;5;12m (https://github.com/nzfarmer1/mqtt2opcua) - Bi Directional MQTT to OPCUA Bridge.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mOPC Router[0m[38;5;12m (https://www.opc-router.com/4_1-mqtt-client-opc-router-plug-in-en/) - MQTT Gateway (publisher/subscriber) with various plug-ins (OPC UA Bridge, SQL Bridge, REST Bridge, SAP Bridge)[39m

[38;2;255;187;0m[4mTelephony, PBX[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1magi-mqtt[0m[38;5;12m (https://github.com/zeha/agi-mqtt) - Interface between Asterisk and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mfritz2mqtt[0m[38;5;12m (https://github.com/akentner/fritz2mqtt) - Connect FRITZ!Box to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1msip2mqtt[0m[38;5;12m (https://github.com/MartyTremblay/sip2mqtt) - A SIP monitoring script that publishes incoming calls with CallerID to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1msms2mqtt[0m[38;5;12m (https://github.com/Domochip/sms2mqtt) - Docker Gateway to send/receive SMS through MQTT using an USB GSM dongle (gammu).[39m


[38;2;255;187;0m[4mOperating System[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-os-status[0m[38;5;12m (https://github.com/oskarhagberg/mqtt-os-status) - Operating-system related data, published to an MQTT broker at fixed intervals.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttlauncher[0m[38;5;12m (https://github.com/jpmens/mqtt-launcher) - Execute shell commands triggered by published MQTT messages.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttpc[0m[38;5;12m (https://github.com/hobbyquaker/mqttpc) - Control processes via MQTT. Ability to send signals via MQTT and to publish stdout/stderr or pipe MQTT payloads into stdin.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttwatchdir[0m[38;5;12m (https://github.com/jpmens/mqtt-watchdir) - Recursively watch a directory for modifications and publish file content to an MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mpsmqtt[0m[38;5;12m (https://github.com/eschava/psmqtt) - Utility reporting system health and status via MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mWinThing[0m[38;5;12m (https://github.com/msiedlarek/winthing) - Remotely control Windows through MQTT.[39m


[38;2;255;187;0m[4mMonitoring[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mcheck-mqtt[0m[38;5;12m (https://github.com/jpmens/check-mqtt) - A Nagios/Icinga plugin for checking connectivity to an MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mnag2mqtt[0m[38;5;12m (https://github.com/DE-IBH/nag2mqtt) - Nagios event broker to MQTT gateway.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mnotify-by-mqtt[0m[38;5;12m (https://github.com/jpmens/notify-by-mqtt) - A Nagios/Icinga notification module which wraps data into JSON and fires it off to an MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2notifysend[0m[38;5;12m (https://github.com/David-Lor/MQTT2NotifySend) - Subscribe to a topic and show notifications from MQTT messages on Ubuntu & other notify-send compatible Linux distros.[39m


[38;2;255;187;0m[4mLocation tracking[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mOwnTracks[0m[38;5;12m (https://owntracks.org/) - Location tracking and geofencing for MQTT.[39m


[38;2;255;187;0m[4mLogging[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mgraylog-plugin-mqtt[0m[38;5;12m (https://github.com/graylog-labs/graylog-plugin-mqtt) - MQTT Input Plugin for Graylog.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1minflux4mqtt[0m[38;5;12m (https://github.com/hobbyquaker/influx4mqtt) - Subscribe to MQTT topics and insert into InfluxDB.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2elasticsearch[0m[38;5;12m (https://github.com/hobbyquaker/mqtt2elasticsearch) - Send MQTT messages to Elasticsearch.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2graphite[0m[38;5;12m (https://github.com/jpmens/mqtt2graphite) - Archived!  Instead use [39m[38;5;14m[1mmqttwarn[0m[38;5;12m (https://github.com/jpmens/mqttwarn) with [39m[38;5;14m[1mcarbon[0m[38;5;12m (https://github.com/jpmens/mqttwarn/blob/master/HANDBOOK.md#carbon) plugin.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttcollect[0m[38;5;12m (https://github.com/jpmens/mqttcollect) - A collectd "Exec" plugin for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtthandler[0m[38;5;12m (https://github.com/changyuheng/MQTTHandler) - A Python logging handler module for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2mongodb[0m[38;5;12m (https://github.com/David-Lor/MQTT2MongoDB) - Subscribe to MQTT topics and insert into MongoDB.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-firebase[0m[38;5;12m (https://www.npmjs.com/package/mqtt-firebase) - A CLI tool for subscribing to MQTT topics and dumping them to a firebase firestore DB.[39m


[38;2;255;187;0m[4mSmart Home Hardware Interfaces[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1maqara-mqtt[0m[38;5;12m (https://github.com/monster1025/aqara-mqtt) - Aqara (Xiaomi) Gateway to MQTT bridge.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1maqara2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/aqara2mqtt) - Attach [39m[38;5;14m[1mAqara[0m[38;5;12m (http://www.aqara.com.cn/us/index.html) Smart Hubs to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mcan2mqtt[0m[38;5;12m (https://github.com/c3re/can2mqtt) - CAN-Bus - MQTT Bridge (also works vice versa).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mcul2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/cul2mqtt) - Interface between [39m[38;5;14m[1mBusware CUL[0m[38;5;12m (http://shop.busware.de/product_info.php/cPath/1/products_id/29) (868MHz RF-Devices like ELV FS20, HMS, EM, ...) and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mdomiqtt[0m[38;5;12m (https://github.com/etobi/domiqtt) - Connects to a Domiq Base (LCN) and translate from and to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1meno2mqtt[0m[38;5;12m (https://github.com/owagner/eno2mqtt) - Interface between an Enocean USB300 (TCM310) adapter and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mEvohome2mqtt[0m[38;5;12m (https://github.com/svrooij/evohome2mqtt) - MQTT Interface for the Honeywell Evohome system.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mgardena2mqtt[0m[38;5;12m (https://github.com/Domochip/gardena2mqtt) - Docker Gateway to control GARDENA Smart system devices (Sileno mower, Irrigation Control, etc.) through MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhelios2mqtt[0m[38;5;12m (https://github.com/mreschka/helios2mqtt) - A daemon for syncing a helios easy controls system like my KWL EC 220D to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhm2mqtt.js[0m[38;5;12m (https://github.com/hobbyquaker/hm2mqtt.js) - Interface between EQ-3's Homematic line of smarthome devices and MQTT. Supports Homematic IP.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhomeeToMqtt[0m[38;5;12m (https://github.com/odig/homeeToMqtt) - Bidirectional Interface between homee and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHS100toMQTT[0m[38;5;12m (https://github.com/dersimn/HS100toMQTT) - Gateway between TPLink HS100/HS110 and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mipcam2mqtt[0m[38;5;12m (https://github.com/svrooij/ipcam2mqtt) - A small FTP server to receive movement images from ipcameras and turn them into MQTT alerts.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mknx-mqtt-bridge[0m[38;5;12m (https://github.com/pakerfeldt/knx-mqtt-bridge) - ridges KNX and MQTT using the knx.js library.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mknx2mqtt[0m[38;5;12m (https://github.com/owagner/knx2mqtt) - Interface between the KNX home automation standard and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmcsMQTT[0m[38;5;12m (https://shop.homeseer.com/products/mcsmqtt-software-plug-in-for-hs3) - Plug-in for HS3 (HomeSeer).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-dss-bridge[0m[38;5;12m (https://github.com/cgHome/mqtt-dss-bridge) - MQTT digitalSTROM-Server Bridge.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-unifi-protect-bridge[0m[38;5;12m (https://github.com/terafin/mqtt-unifi-protect-bridge) - Adding motion-status from UniFi Protect Cameras to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2homekit[0m[38;5;12m (https://github.com/forty2/mqtt2homekit) - Roughly the opposite of [39m[38;5;14m[1mhomekit2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/homekit2mqtt): Control your HomeKit-enabled devices with MQTT and without Siri or iPhone.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mnode-lox-mqtt-gateway[0m[38;5;12m (https://github.com/alladdin/node-lox-mqtt-gateway) - Gateway for Loxone™ mini server to communicate with MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1msmartthings-mqtt-bridge[0m[38;5;12m (https://github.com/stjohnjohnson/smartthings-mqtt-bridge) - Bridge between [39m[38;5;14m[1mSmartThings[0m[38;5;12m (https://www.smartthings.com/) and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mxiaomi2mqtt[0m[38;5;12m (https://github.com/svrooij/node-xiaomi2mqtt) - bridge between the Xiaomi Smart Home Gateway Aquara and a MQTT server.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mzigbee2mqtt[0m[38;5;12m (https://github.com/Koenkk/zigbee2mqtt) - Allows you to use your Zigbee devices without the vendors (Xiaomi/TRADFRI/Hue) bridge/gateway.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mzwavejs2mqtt[0m[38;5;12m (https://github.com/zwave-js/zwavejs2mqtt) - Zwave to Mqtt gateway and Control Panel Web UI.[39m


[38;2;255;187;0m[4mSmart Home Integration Software[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mcontrol-freak[0m[38;5;12m (https://github.com/catx23/control-freak) - IDE for IoT & friends. Built in MQTT support.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mDomoticz[0m[38;5;12m (https://www.domoticz.com/) - Domoticz beta supports MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mFHEM[0m[38;5;12m (http://fhem.de/fhem.html) has a [39m[38;5;14m[1mMQTT module[0m[38;5;12m (http://fhem.de/commandref.html#MQTT) since V5.6.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHome Assistant[0m[38;5;12m (https://www.home-assistant.io/) has a MQTT component.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHome.Pi[0m[38;5;12m (https://github.com/denschu/home.pi) is based on MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHomegear[0m[38;5;12m (https://homegear.eu/index.php/Main_Page) has build in MQTT support.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhomekit2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/homekit2mqtt) - Interface between [39m[38;5;14m[1mHAP-NodeJS[0m[38;5;12m (https://github.com/homebridge/HAP-NodeJS) and MQTT. Control MQTT connected devices with Siri or HomeKit Apps.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mioBroker[0m[38;5;12m (https://github.com/ioBroker) has a [39m[38;5;14m[1mMQTT adapter[0m[38;5;12m (https://github.com/ioBroker/ioBroker.mqtt).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mNode-RED[0m[38;5;12m (https://nodered.org/) - A visual tool for wiring the Internet of Things, has native MQTT Support.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mopenHAB[0m[38;5;12m (https://github.com/openhab) has a [39m[38;5;14m[1mMQTT binding[0m[38;5;12m (https://github.com/openhab/openhab1-addons/wiki/MQTT-Binding).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mpimatic[0m[38;5;12m (https://pimatic.org/) has a MQTT plugin.[39m


[38;2;255;187;0m[4mLighting[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mArilux_AL-LC0X[0m[38;5;12m (https://github.com/mertenats/Arilux_AL-LC0X) - This is an alternative firmware for Arilux LED controllers which uses MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mchromoflex2mqtt[0m[38;5;12m (https://github.com/owagner/chromoflex2mqtt) - Control Chromoflex USP3 RGB LED modules via MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mh801/mqtt[0m[38;5;12m (https://github.com/open-homeautomation/h801/tree/master/mqtt) - Alternative firmware for the H801 LED dimmer that uses MQTT as a control channel.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhue2mqtt.js[0m[38;5;12m (https://github.com/hobbyquaker/hue2mqtt.js) - Interface between the Philips Hue bridge and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT DMX Controller[0m[38;5;12m (https://github.com/hobbyquaker/mqtt-dmx-controller) - DMX Controller with MQTT support.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-dmx-sequencer[0m[38;5;12m [39m[38;5;12m(https://github.com/hobbyquaker/mqtt-dmx-sequencer)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mHeadless[39m[38;5;12m [39m[38;5;12mcounterpart[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;14m[1mMQTT[0m[38;5;14m[1m [0m[38;5;14m[1mDMX[0m[38;5;14m[1m [0m[38;5;14m[1mController[0m[38;5;12m [39m[38;5;12m(https://github.com/hobbyquaker/mqtt-dmx-sequencer)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12muse[39m[38;5;12m [39m[38;5;12mscenes[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12msequences[39m[38;5;12m [39m[38;5;12mexported[39m[38;5;12m [39m[38;5;12mfrom[39m[38;5;12m [39m[38;5;12mthe[39m[38;5;12m [39m[38;5;12mMQTT[39m[38;5;12m [39m[38;5;12mDMX[39m[38;5;12m [39m[38;5;12mController[39m[38;5;12m [39m
[38;5;12mand[39m[38;5;12m [39m[38;5;12mcontrol[39m[38;5;12m [39m[38;5;12mthem[39m[38;5;12m [39m[38;5;12mvia[39m[38;5;12m [39m[38;5;12mMQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1msunricher-wifi-mqtt[0m[38;5;12m (https://github.com/magcode/sunricher-wifi-mqtt) - control Sunricher LED devices using MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mTRADFRI2MQTT[0m[38;5;12m (https://github.com/hardillb/TRADFRI2MQTT) - MQTT Bridge for IKEA TRÅDFRI Light Gateway.[39m


[38;2;255;187;0m[4mHome Entertainment[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mairtunes2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/airtunes2mqtt) - MQTT controlled Multi-Room Audio with Airplay/Airtunes Devices.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mbravia2mqtt[0m[38;5;12m (https://github.com/forty2/bravia2mqtt) - Control your Sony Bravia TV with MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mbroadlink-mqtt[0m[38;5;12m (https://github.com/eschava/broadlink-mqtt) - MQTT client to control BroadLink RM devices.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mchromecast-mqtt-connector[0m[38;5;12m (https://github.com/nohum/chromecast-mqtt-connector) - Control your Google Chromecast devices using MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mharmony-api[0m[38;5;12m (https://github.com/maddox/harmony-api) - A simple server allowing you to query/control multiple local Harmony Home Hubs over HTTP or MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhtd2mqtt[0m[38;5;12m (https://github.com/TheOriginalAndrobot/htd2mqtt) - Bridge between an HTD Lync audio system and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mkodi2mqtt[0m[38;5;12m (https://github.com/owagner/kodi2mqtt) - Interface between a Kodi media center instance and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mlgtv2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/lgtv2mqtt) - Interface between LG WebOS Smart TVs and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mlirc2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/lirc2mqtt) - Send and receive infrared via [39m[38;5;14m[1mLIRC[0m[38;5;12m (www.lirc.org).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmopidy-mqtt[0m[38;5;12m (https://github.com/magcode/mopidy-mqtt) - MQTT features for Mopidy.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT-DashCast-Docker[0m[38;5;12m (https://github.com/mukowman/MQTT-DashCast-Docker) - MQTT Docker to launch DashCast session on Chromecast.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2atlonamatrix[0m[38;5;12m (https://github.com/forty2/mqtt2atlonamatrix) - Control Atlona HDMI matrix switches with MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2tivoremote[0m[38;5;12m (https://github.com/forty2/mqtt2tivoremote) - Make TiVo DVR remote control available through an MQTT smarthome style interface.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1monkyo2mqtt[0m[38;5;12m (https://github.com/owagner/onkyo2mqtt) - Interface between Onkyo AVR's EISCP network remote protocol and MQTT. Uses the onkyo-eiscp library.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1msonos2mqtt[0m[38;5;12m (https://github.com/svrooij/sonos2mqtt) - A bridge between Sonos and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mVLC MQTT Module[0m[38;5;12m (https://wiki.videolan.org/Documentation:Modules/mqtt/) - Control VLC via MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mxbmc2mqtt[0m[38;5;12m (https://github.com/gordonjcp/xbmc-mqtt) - A simple plugin for XBMC to listen for a particular topic on an MQTT broker, and display a popup message.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1myamaha-avr2mqtt[0m[38;5;12m (https://github.com/akentner/yamaha-avr2mqtt) - A simple adapter for connection Yamaha AVR to MQTT.[39m


[38;2;255;187;0m[4mSmart Metering[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mbcontrol2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/bcontrol2mqtt) - Publish measurements from TQ Energy Manager / [39m[38;5;14m[1mBusch-Jäger Energy Monitor[0m[38;5;12m (https://www.busch-jaeger.de/files/files_ONLINE/Brosch%c3%bcre_EnergyMonitor_druck.pdf) to MQTT.[39m


[38;2;255;187;0m[4mMessaging[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-irc-bot[0m[38;5;12m (https://github.com/dobermai/mqtt-irc-bot) - A MQTT to IRC / IRC to MQTT bridge or bot.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttwarn[0m[38;5;12m (https://github.com/jpmens/mqttwarn) - Subscribe to MQTT topics (with wildcards) and notify pluggable services.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mtwitter-to-mqtt[0m[38;5;12m (https://github.com/knolleary/twitter-to-mqtt) - A python daemon that uses the Twitter Streaming API to access tweets and republishes them to an MQTT topic.[39m


[38;2;255;187;0m[4mMisc[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mAlexaMqttBridge[0m[38;5;12m (https://github.com/mhdawson/AlexaMqttBridge) - Bridge between Amazon Alexa and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mbt-mqtt-gateway[0m[38;5;12m (https://github.com/zewelor/bt-mqtt-gateway) - Easily extensible Bluetooth to MQTT gateway, currently supports: EQ3 smart thermostat, Xiaomi Mi Scale, Linak Desk, MySensors and Xiaomi Mi Flora plant sensor.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mbuderus2mqtt[0m[38;5;12m (https://github.com/krambox/buderus2mqtt) - Bridge between Buderus KM200 internet gateway and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mchrome2mqtt[0m[38;5;12m (https://github.com/tbowmo/chrome2mqtt) - Python program to enable MQTT control endpoints for chromecasts (both audio and video).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mdashbutton2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/dashbutton2mqtt) - Publish Amazon Dash Button presses to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mflowerpower2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/flowerpower2mqtt) - Publish measurements from Parrot Flower Power plant sensors to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mgBridge[0m[38;5;12m [39m[38;5;12m(https://github.com/kservices/gBridge)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mgBridge[39m[38;5;12m [39m[38;5;12mallows[39m[38;5;12m [39m[38;5;12myou[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mcontrol[39m[38;5;12m [39m[38;5;12m(almost)[39m[38;5;12m [39m[38;5;12many[39m[38;5;12m [39m[38;5;12msmart[39m[38;5;12m [39m[38;5;12mhome[39m[38;5;12m [39m[38;5;12mdevice,[39m[38;5;12m [39m[38;5;12many[39m[38;5;12m [39m[38;5;12msmart[39m[38;5;12m [39m[38;5;12mhome[39m[38;5;12m [39m[38;5;12msoftware,[39m[38;5;12m [39m[38;5;12mwith[39m[38;5;12m [39m[38;5;12mGoogle[39m[38;5;12m [39m[38;5;12mAssistant.[39m[38;5;12m [39m[38;5;12mTherefore,[39m[38;5;12m [39m[38;5;12mit[39m[38;5;12m [39m[38;5;12mtransforms[39m[38;5;12m [39m[38;5;12mactions[39m[38;5;12m [39m[38;5;12mreceived[39m[38;5;12m [39m[38;5;12mfrom[39m[38;5;12m [39m[38;5;12mGoogle[39m[38;5;12m [39m[38;5;12mby[39m[38;5;12m [39m[38;5;12mvoice[39m[38;5;12m [39m[38;5;12mcommands[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m
[38;5;12mMQTT[39m[38;5;12m [39m[38;5;12mmessages.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhaiku2mqtt[0m[38;5;12m (https://github.com/forty2/haiku2mqtt) - A bridge between Haiku smart fans and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mhomely[0m[38;5;12m (https://github.com/baol/homely) - Collection of Go daemons for connecting Domoticz and other stuff.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mkobold2mqtt[0m[38;5;12m (https://github.com/krambox/kobold2mqtt) - Bridge between Vorwerk Kobold Vr200 internet gateway and MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mleaf-python-mqtt[0m[38;5;12m (https://github.com/glynhudson/leaf-python-mqtt) - Extract data from Nissan Leaf API and post to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmiflora-mqtt-daemon[0m[38;5;12m (https://github.com/ThomDietrich/miflora-mqtt-daemon) - Linux service to send Xiaomi Mi Flora plant sensor data to an MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT.Cool[0m[38;5;12m (https://mqtt.cool) - A web gateway that optimizes any MQTT broker when sending real-time data to web clients with automatic throttling.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2ble[0m[38;5;12m (https://github.com/hardillb/mqtt2ble) - A way to bridge MQTT topics to BLE Gatt characteristics.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttclpro[0m[38;5;12m (https://github.com/dc297/mqttclpro) - MQTT Client with tasker integration Android app.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqttDB[0m[38;5;12m (https://github.com/hobbyquaker/mqttDB) - A JSON store with MQTT interface.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-camera-streamer[0m[38;5;12m (https://github.com/robmarkcole/mqtt-camera-streamer) - Stream images from a connected camera over MQTT & view using Streamlit[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT Joystick Controller[0m[38;5;12m (https://github.com/Vincenzo-Petrolo/MQTT-Joystick-Controller) - Open Source Android app that lets you control everything with your smartphone. Download it from Google Play.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-transformer[0m[38;5;12m (https://github.com/tg44/mqtt-transformer) - A simple service which consumes, transforms and periodically republish json messages on MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mnode-mqtt-for-anki-overdrive[0m[38;5;12m (https://github.com/IBM-Cloud/node-mqtt-for-anki-overdrive) - Node.js Controller and MQTT API for Anki Overdrive.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mparrot-sample[0m[38;5;12m (https://github.com/IBM-Cloud/parrot-sample) - Sample code which uses MQTT to control a Parrot AR Drone.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mserial2mqtt[0m[38;5;12m (https://github.com/vortex314/serial2mqtt) - A Linux gateway to connect low-cost microcontrollers only with a serial port to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1msnowboy2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/snowboy2mqtt) - Publish MQTT Messages on Snowboy Hotword Detection.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mspeedtest2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/speedtest2mqtt) - Run speedtest-cli and publish results via MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1munifi2mqtt[0m[38;5;12m (https://github.com/hobbyquaker/unifi2mqtt) - Publish connected clients from Ubiquiti Unifi to MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mValetudo[0m[38;5;12m (https://github.com/Hypfer/Valetudo) - Xiaomi (Roborock) Vacuum Robots Firmware with MQTT and Webinterface.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mwlan-thermo-mqtt-addon[0m[38;5;12m (https://bitbucket.org/IOcastor/wlan-thermo-mqtt-addon/) - Addon for a popular DIY barbecue thermometer.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;12mTasker (Automation for Android) [39m[38;5;14m[1mMQTT Publisher Plugin[0m[38;5;12m (https://play.google.com/store/apps/details?id=net.nosybore.mqttpublishplugin).[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT2ETCD[0m[38;5;12m (https://github.com/David-Lor/MQTT2ETCD) - MQTT-ETCD gateway: PUT keys on ETCD through MQTT, and watch ETCD key changes on MQTT topics[39m


[38;2;255;187;0m[4mVisualization, Dashboards[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mCrouton[0m[38;5;12m (https://github.com/edfungus/Crouton) - A dashboard that taps into your IOT network, using only MQTT and JSON.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1md3-MQTT-Topic-Tree[0m[38;5;12m (https://github.com/hardillb/d3-MQTT-Topic-Tree) - A MQTT Topic Tree viewer using the d3 collapsible tree and MQTT over websockets.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHelloIoT[0m[38;5;12m (https://github.com/adrianromero/helloiot) - HelloIoT is a MQTT client and dashboard application.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mHOMR-REACT[0m[38;5;12m (https://github.com/klauserber/homr-react) - A configurable MQTT Visualization.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mIoT OnOff[0m[38;5;12m (https://www.iot-onoff.com/) - Configurable iOS/Android app.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mLinear MQTT Dashboard[0m[38;5;12m (https://github.com/ravendmaster/linear-mqtt-dashboard) - Easy, customizable control panel - MQTT-client.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMMM-mqtt[0m[38;5;12m (https://github.com/javiergayala/MMM-mqtt) - This is an extension for the MagicMirror². It provides the ability to subscribe to MQTT topics and display them.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT Dash[0m[38;5;12m (https://play.google.com/store/apps/details?id=net.routix.mqttdash&hl=de) - Android App: With the app you can create dashboards for your MQTT enabled IoT Smart Home devices and applications.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT-Hyperdash[0m[38;5;12m (https://github.com/kollokollo/MQTT-Hyperdash) - A universal independent MQTT Dashboard for linux/Raspberry Pi.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMQTT.Cool Test Client[0m[38;5;12m (https://testclient-cloud.mqtt.cool) - A web interface for testing interaction between MQTT.Cool and any MQTT broker.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-panel[0m[38;5;12m (https://github.com/fabaff/mqtt-panel) - A web interface for MQTT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-prometheus-message-exporter[0m[38;5;12m (https://github.com/tg44/mqtt-prometheus-message-exporter) - A small service which will convert mqtt messages to prometheus metrics.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-svg-dash[0m[38;5;12m (https://github.com/jpmens/mqtt-svg-dash) - Subscribe to MQTT, extract JSON from a message and make lights blink on an SVG page.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt2highcharts[0m[38;5;12m (https://github.com/matbor/mqtt2highcharts) - Plotting live numbered data from a subscribed MQTT topic using Highcharts.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mMYHELLOIOT[0m[38;5;12m (https://adrianromero.github.io/myhelloiot/) - MYHELLOIOT is a MQTT dashboard application inspired in my other MQTT project HelloIoT.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mnode-red-dashboard[0m[38;5;12m (https://github.com/node-red/node-red-dashboard) - A dashboard UI for Node-RED.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mPlotJuggler[0m[38;5;12m [39m[38;5;12m(https://github.com/facontidavide/PlotJuggler)[39m[38;5;12m [39m[38;5;12m-[39m[38;5;12m [39m[38;5;12mPlotJuggler[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mtool[39m[38;5;12m [39m[38;5;12mto[39m[38;5;12m [39m[38;5;12mvisualize[39m[38;5;12m [39m[38;5;12mtime[39m[38;5;12m [39m[38;5;12mseries[39m[38;5;12m [39m[38;5;12m(from[39m[38;5;12m [39m[38;5;12msources[39m[38;5;12m [39m[38;5;12msuch[39m[38;5;12m [39m[38;5;12mas:[39m[38;5;12m [39m[38;5;12mMQTT,[39m[38;5;12m [39m[38;5;12mWebsockets,[39m[38;5;12m [39m[38;5;12mZeroMQ,[39m[38;5;12m [39m[38;5;12mUDP,[39m[38;5;12m [39m[38;5;12metc.,[39m[38;5;12m [39m[38;5;12msupports[39m[38;5;12m [39m[38;5;12mdata[39m[38;5;12m [39m[38;5;12mformats[39m[38;5;12m [39m[38;5;12msuch[39m[38;5;12m [39m[38;5;12mas[39m[38;5;12m [39m[38;5;12mJSON,[39m[38;5;12m [39m[38;5;12mCBOR,[39m[38;5;12m [39m[38;5;12mBSON,[39m[38;5;12m [39m[38;5;12mMessage[39m[38;5;12m [39m[38;5;12mPack,[39m[38;5;12m [39m
[38;5;12metc.).[39m[38;5;12m [39m[38;5;12mIt[39m[38;5;12m [39m[38;5;12mis[39m[38;5;12m [39m[38;5;12ma[39m[38;5;12m [39m[38;5;12mfast,[39m[38;5;12m [39m[38;5;12mpowerful[39m[38;5;12m [39m[38;5;12mand[39m[38;5;12m [39m[38;5;12mintuitive[39m[38;5;12m [39m[38;5;12mcross-platform[39m[38;5;12m [39m[38;5;12mtool.[39m



[38;5;12mOther tools that can be used to create Visualization/Dashboards can be found under [39m[38;5;14m[1mPlatforms[0m[38;5;12m (#platforms) and [39m[38;5;14m[1mSmart Home Integration Software[0m[38;5;12m (#smart-home-integration-software).[39m


[38;2;255;187;0m[4mArchitecture, Convention[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mmqtt-smarthome[0m[38;5;12m (https://github.com/mqtt-smarthome/mqtt-smarthome) - Smart home automation with MQTT as the central message bus - Architectural proposal.[39m
[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mThe Homie Convention[0m[38;5;12m (https://github.com/homieiot/convention) - A lightweight MQTT convention for the IoT.[39m

[38;2;255;187;0m[4mSecurity, Encryption[0m

[48;5;12m[38;5;11m⟡[49m[39m[38;5;12m [39m[38;5;14m[1mTeserakt E4[0m[38;5;12m (https://teserakt.io/) - End-to-end encryption and key management for MQTT and other M2M protocols – Open-source and paid plans.[39m


[38;2;255;187;0m[4mContribute[0m

[38;5;12mContributions welcome! Read the [39m[38;5;14m[1mcontribution guidelines[0m[38;5;12m (contributing.md) first.[39m


[38;2;255;187;0m[4mLicense[0m

[38;5;14m[1m![0m[38;5;12mCC0[39m[38;5;14m[1m (https://i.creativecommons.org/p/zero/1.0/88x31.png)[0m[38;5;12m (https://creativecommons.org/publicdomain/zero/1.0/)[39m
