Metadata-Version: 2.1
Name: pymata-aio
Version: 2.35
Summary: A Python Protocol Abstraction Library For Arduino Firmata using Python asyncio
Home-page: https://github.com/MrYsLab/pymata-aio/wiki
Author: Alan Yorinks
Author-email: MisterYsLab@gmail.com
License: GNU Affero General Public License v3 or later (AGPLv3+)
Download-URL: https://github.com/MrYsLab/pymata-aio
Keywords: Firmata,Arduino,Protocol
Platform: UNKNOWN
Classifier: Development Status :: 5 - Production/Stable
Classifier: Environment :: Other Environment
Classifier: Intended Audience :: Developers
Classifier: Intended Audience :: Education
Classifier: License :: OSI Approved :: GNU Affero General Public License v3 or later (AGPLv3+)
Classifier: Operating System :: OS Independent
Classifier: Programming Language :: Python :: 3.5
Classifier: Programming Language :: Python :: 3 :: Only
Classifier: Topic :: Utilities
Classifier: Topic :: Education
Classifier: Topic :: Home Automation
Description-Content-Type: text/markdown
Requires-Dist: pyserial
Requires-Dist: websockets



pymata_aio is a high performance, non-blocking, Python asyncio client
for the Firmata Protocolthat supports the complete StandardFirmata
protocol.

Major features  
==============

* Python 3.5+ compatible.

* Choose From 3 Included APIs
     * pymata_core - a pure asyncio method call API.
     * pymata3 - A non-asyncio proxy for pymata_core
     * pymata_iot - A websocket based backed to control an Arduino over a Web page.

* Implements 100% of the StandardFirmata Protocol (StandardFirmata 2.5.3).

* Auto-detects Arduino COM ports.

* FirmataPlus (enhanced StandardFirmata sketch) included with distribution. It adds support for:
     * HC-SR04 Ultrasonic Distance Sensors using a single pin.
     * Stepper Motors.
     * Piezo Tone Generation.
     * 2 Pin Rotary Encoder Support.

* FirmataPlusRB (enhanced StandaradFirmata sketch to control a SparkFun Redbot. It adds support for:
     * Piezo Tone Generation.
     * Wheel encoders.
     * RedBot Accelerometer.

* Ability to automatically capture and time-stamp user specified analog and digital transient input events on a per-pin basis.
* All 3 APIs support callback as well as a polled interface.




