(footprint "R_Shunt_Ohmite_LVK20"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contacts shunt resistor, https://www.ohmite.com/assets/docs/res_lvk.pdf")
	(tags "4 contacts resistor smd")
	(property "Reference" "REF**"
		(at 0.025 -4.2 0)
		(layer "F.SilkS")
		(uuid "7126161d-6b54-411f-9887-7ae68a3e6d92")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Ohmite_LVK20"
		(at 0.05 4.325 0)
		(layer "F.Fab")
		(uuid "6a0f3322-774a-4fca-be31-d88d7ea57a74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "58ae2c11-2382-4567-8330-0e49785d111f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "af798b3f-753c-4f42-9a5b-3dd9c3eacdf1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.5 0.6)
		(end -1.5 -0.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "91425deb-f78a-4c0c-b161-7afebd033ed1")
	)
	(fp_line
		(start 0.15 -2.75)
		(end -0.15 -2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c187a939-be0a-4faf-b5f8-42d470c2985e")
	)
	(fp_line
		(start 0.15 2.75)
		(end -0.15 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9f4f888a-d99f-499d-bbbf-744a10f09e93")
	)
	(fp_line
		(start 1.5 -0.6)
		(end 1.5 0.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "98705423-d60f-46cb-b0e3-09484452648c")
	)
	(fp_line
		(start -2.05 -3.5)
		(end 2.05 -3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b3d16c07-2108-42eb-aae7-bdcc0f758d08")
	)
	(fp_line
		(start -2.05 3.5)
		(end -2.05 -3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d00873b4-f80f-41ac-9a9e-8c0b0b88c750")
	)
	(fp_line
		(start 2.05 -3.5)
		(end 2.05 3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ef2a2cac-5347-4abe-9651-1f679064ca7c")
	)
	(fp_line
		(start 2.05 3.5)
		(end -2.05 3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "20db513f-7307-4839-80ce-50f75de71976")
	)
	(fp_line
		(start -1.25 -2.5)
		(end 1.25 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8227ed00-93ec-40e3-bede-d3492b2147d6")
	)
	(fp_line
		(start -1.25 2.5)
		(end -1.25 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9c623acf-2306-4063-bff1-ec5e654cd4f4")
	)
	(fp_line
		(start 0 2.5)
		(end -1.25 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dcfc9340-ab2d-420f-96a2-215766fd46cb")
	)
	(fp_line
		(start 1.25 -2.5)
		(end 1.25 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "217c7f78-30bd-4a73-b3b9-df01bd19b437")
	)
	(fp_line
		(start 1.25 2.5)
		(end 0 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0d6c97a5-b1bf-41c6-b85c-1533526ec8cf")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "6a472fb4-7b94-49de-952c-993c0a85b71d")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
			)
		)
	)
	(pad "1" smd rect
		(at -1.025 -1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "9403a5f5-3032-4eac-9b91-7fd554a09f31")
	)
	(pad "2" smd rect
		(at 1.025 -1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "86b6d8dc-ff69-497f-b4f2-503cefeecc7d")
	)
	(pad "3" smd rect
		(at 1.025 1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "73edc423-e7cc-4d77-98fc-06a7898b09d4")
	)
	(pad "4" smd rect
		(at -1.025 1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b4d5020b-6787-4886-8d21-325e658bc8e4")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Ohmite_LVK20.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
