(footprint "R_Shunt_Vishay_WSR2_WSR3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Power Metal Strip Resistors 0.005 to 0.2, https://www.vishay.com/docs/30101/wsr.pdf")
	(tags "SMD Shunt Resistor")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
		(uuid "f4eb0cda-cd64-4ef9-9265-7d211dd67fa1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Vishay_WSR2_WSR3"
		(at 0 4.6 0)
		(layer "F.Fab")
		(uuid "83052caf-be33-49ff-997d-3dd21aa5fccf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "72e47c8e-04a0-4621-9c86-b92db68afa61")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b98e8c17-4d49-4283-b934-4e0f2b6c71c4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.78 -3.6)
		(end 5.78 -3.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c171ffa9-a7f8-4490-8977-2bd877daf32b")
	)
	(fp_line
		(start -5.78 3.6)
		(end 5.78 3.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5cae75e4-077a-4032-a8ad-86039724648d")
	)
	(fp_line
		(start -6.8 -3.74)
		(end -6.8 3.74)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "95d37aab-067f-40d2-846a-f89d602675e1")
	)
	(fp_line
		(start -6.8 -3.74)
		(end 6.8 -3.74)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4951ae3e-15fc-4445-85b2-42623ad1429d")
	)
	(fp_line
		(start -6.8 3.74)
		(end 6.8 3.74)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bcc6b6d7-ed3c-4e50-8163-f09f35fc3d88")
	)
	(fp_line
		(start 6.8 -3.74)
		(end 6.8 3.74)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f6508d5a-7efa-49f3-807d-b2cee5e0f134")
	)
	(fp_line
		(start -5.78 -3.49)
		(end -5.78 3.49)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f3dd4885-4386-484b-b16b-97a83aa0628b")
	)
	(fp_line
		(start -5.78 -3.49)
		(end 5.78 -3.49)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "15ede0cb-9a0b-4750-be49-2d8af8a691f3")
	)
	(fp_line
		(start -5.78 3.49)
		(end 5.78 3.49)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c2be4960-c6f3-49a9-9a4b-10d2377ac1a2")
	)
	(fp_line
		(start 5.78 -3.49)
		(end 5.78 3.49)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2f611df7-2672-40df-928c-5c73917f39a0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "fe59d19e-30c0-429e-9a2d-b001fe4bfe8b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -4.575 0)
		(size 3.94 5.84)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a8d74625-eb9d-490b-a662-e882a5c9ffc9")
	)
	(pad "2" smd rect
		(at 4.575 0)
		(size 3.94 5.84)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "4d648dde-9b35-43df-bd94-fe6853f5a82a")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSR2_WSR3.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
