(footprint "R_Shunt_Ohmite_LVK12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contact shunt resistor")
	(tags "shunt resistor 4 contacts")
	(property "Reference" "REF**"
		(at 0 -3.2 180)
		(layer "F.SilkS")
		(uuid "17e6e1ba-b97d-42b0-a314-6cbe61a06611")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Ohmite_LVK12"
		(at 0 3.4 0)
		(layer "F.Fab")
		(uuid "de7bb09e-3c28-465f-853f-b36d36989677")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "60bfbd54-198c-4d68-a5bc-0476b53286bd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8884c110-a3cd-4720-bbbf-390fee4927dc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1 0.4)
		(end -1 -0.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c700d361-8d9d-48ec-a838-acc6e5929f34")
	)
	(fp_line
		(start 1 -0.4)
		(end 1 0.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d1232d43-b53b-491c-b78d-f423687cc1c1")
	)
	(fp_line
		(start -1.5 -2.5)
		(end 1.5 -2.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "661922cb-3b5b-4e4a-9d48-b7109bf9ac1d")
	)
	(fp_line
		(start -1.5 2.5)
		(end -1.5 -2.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ec778308-51e3-43db-b0c2-85adf0d55e3d")
	)
	(fp_line
		(start 1.5 -2.5)
		(end 1.5 2.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "78e0f7b9-74b5-40b0-bb5a-ff60345a7431")
	)
	(fp_line
		(start 1.5 2.5)
		(end -1.5 2.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "89779130-bc97-4339-a149-3757742edec8")
	)
	(fp_line
		(start -0.8 -1.6)
		(end -0.8 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9e8f70fa-83ca-49bd-983e-c2c7ef5ef48b")
	)
	(fp_line
		(start -0.8 1.6)
		(end 0.8 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "07d95e83-b1a5-4a27-ae46-c23531fb2dd3")
	)
	(fp_line
		(start 0.8 -1.6)
		(end -0.8 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a5e6f86d-37c1-4153-af2c-ac441eeb8d64")
	)
	(fp_line
		(start 0.8 1.6)
		(end 0.8 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b26257fd-c70f-4800-bfcb-f1295367e8cc")
	)
	(fp_text user "${REFERENCE}"
		(at 0.1 0 90)
		(layer "F.Fab")
		(uuid "6c9a9589-20b7-4244-920c-c9a363b087ab")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(pad "1" smd rect
		(at -0.7 -1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "601f57ed-96f4-4eb7-9fbc-c38eddb97e95")
	)
	(pad "2" smd rect
		(at 0.7 -1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "3dbe8e76-f9ba-4922-bd62-17080af68e86")
	)
	(pad "3" smd rect
		(at 0.7 1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "46dac940-f796-45be-93a9-24304efb3c44")
	)
	(pad "4" smd rect
		(at -0.7 1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e839c15f-9834-4c27-a4c4-576e27d7236e")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Ohmite_LVK12.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
