(footprint "R_Array_Concave_4x0402"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -2.1 0)
		(layer "F.SilkS")
		(uuid "15873201-6f75-4e59-88bd-6885a23682d4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Concave_4x0402"
		(at 0 2.1 0)
		(layer "F.Fab")
		(uuid "821fb3a1-65e9-44b9-ae5e-87ea1d3ca34f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "66c8c093-5017-4061-9cd1-a5c0eb033ba7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "088f8c39-fb4c-422e-9e85-817b6e3e217e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.25 -1.14)
		(end -0.25 -1.14)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "521f8adf-f533-453b-80c3-3b017371e9a1")
	)
	(fp_line
		(start 0.25 1.14)
		(end -0.25 1.14)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b3ad0a4c-2934-4e96-a50a-364b8b050b70")
	)
	(fp_line
		(start -1 -1.25)
		(end -1 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1bd352c9-d9fc-4e3a-ae34-a6076f0ca2e6")
	)
	(fp_line
		(start -1 -1.25)
		(end 1 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "39355e7b-9f64-418b-a201-d407ad6403f4")
	)
	(fp_line
		(start 1 1.25)
		(end -1 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "588db268-eed3-4b20-8a9f-2ec1fe3c5249")
	)
	(fp_line
		(start 1 1.25)
		(end 1 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e3c0f187-1f32-43e3-a90e-339a996c29bd")
	)
	(fp_line
		(start -0.5 -1)
		(end 0.5 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c40d9823-b72e-4de5-8900-4be2afda65d3")
	)
	(fp_line
		(start -0.5 1)
		(end -0.5 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8067c342-ac03-42f9-8e72-de76868be0f7")
	)
	(fp_line
		(start 0.5 -1)
		(end 0.5 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b20dcf53-449f-4ed6-bf8a-776449e1b479")
	)
	(fp_line
		(start 0.5 1)
		(end -0.5 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "276d1f27-9b94-400c-905b-a7765056c96c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "feaeb7ac-ebfb-4672-a3fd-5026b74678eb")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -0.5 -0.75)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "74f55b47-ffd0-4804-bbe4-01b6acc1482c")
	)
	(pad "2" smd rect
		(at -0.5 -0.25)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "47ed728f-38fb-4ba8-ae26-3aa02f42649d")
	)
	(pad "3" smd rect
		(at -0.5 0.25)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "79a498a4-d351-4c26-9d9d-d61a9c7db9a1")
	)
	(pad "4" smd rect
		(at -0.5 0.75)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "29fdf553-6249-4f38-a361-00cfae716f49")
	)
	(pad "5" smd rect
		(at 0.5 0.75)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c81190da-b631-498b-abdc-eea32edccb58")
	)
	(pad "6" smd rect
		(at 0.5 0.25)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "45313535-6b92-4f02-a07b-f9c88ead0844")
	)
	(pad "7" smd rect
		(at 0.5 -0.25)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "73f23ba9-dcf7-4035-a9ce-90c86fe24ffc")
	)
	(pad "8" smd rect
		(at 0.5 -0.75)
		(size 0.5 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "aaee101d-5871-44d1-88d3-f677b9049f53")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Concave_4x0402.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
