(footprint "R_Cat16-4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMT resistor net, Bourns CAT16 series, 4 way")
	(tags "SMT resistor net Bourns CAT16 series 4 way")
	(property "Reference" "REF**"
		(at 0 -2.6 0)
		(layer "F.SilkS")
		(uuid "cb8d1e5e-cfa6-43d0-adc7-fa7965004757")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Cat16-4"
		(at 0 2.55 0)
		(layer "F.Fab")
		(uuid "fb3b2e0f-f73c-4291-af16-71de11ac6700")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "84a3bd30-0903-46bc-b64f-134c8c9f1c26")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "432ecc6e-fa7c-4a94-a5d5-6fae5ffd27af")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 1.1 -1.7)
		(end -1.1 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f0480aa5-e14b-4fd4-ac57-3dcbfe49b8c2")
	)
	(fp_line
		(start 1.1 1.7)
		(end -1.1 1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "05d6a13d-71d0-49db-90e2-06428dfc08db")
	)
	(fp_circle
		(center 0 0)
		(end -0.1 0)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill no)
		(layer "F.Adhes")
		(uuid "23caf80a-599d-4c12-8746-e300f1c32107")
	)
	(fp_line
		(start -1.39 -1.85)
		(end -1.39 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fe5366d7-3786-4c97-957a-98e19f0d7c34")
	)
	(fp_line
		(start -1.39 -1.85)
		(end 1.39 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d04826a7-1a92-4b29-924e-b40f350deb16")
	)
	(fp_line
		(start 1.39 1.85)
		(end -1.39 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0f8e6898-7cb9-4397-b6e6-e90744c4f357")
	)
	(fp_line
		(start 1.39 1.85)
		(end 1.39 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bf8ea53c-4a67-4bea-8b9c-db5d085d5be3")
	)
	(fp_line
		(start -0.8 -1.6)
		(end 0.8 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b34dd0ec-dc27-4439-8dfe-68338ee4ac5d")
	)
	(fp_line
		(start -0.8 1.6)
		(end -0.8 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dc48a1ac-16bd-46a8-b2ec-847dc865e61a")
	)
	(fp_line
		(start 0.8 -1.6)
		(end 0.8 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d575431d-d1d5-49d0-b468-403a83812826")
	)
	(fp_line
		(start 0.8 1.6)
		(end -0.8 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ae635850-0f35-4b48-81bc-17f74dd918b4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "1965ea1e-17ae-4257-8d98-cabafcf66b78")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -0.76 -1.2 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "f667b96c-877d-4ab1-96c2-891228ff8fb9")
	)
	(pad "2" smd rect
		(at -0.76 -0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ae270dff-b5b9-4dea-8b88-e5560195b64a")
	)
	(pad "3" smd rect
		(at -0.76 0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "4560570f-5089-4129-b4f0-86c07a968aeb")
	)
	(pad "4" smd rect
		(at -0.76 1.2 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "417c0223-9b8f-4ac0-a082-7615e83c2f44")
	)
	(pad "5" smd rect
		(at 0.76 1.2 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b93a3cbf-691e-42c6-85e9-f190d80384b4")
	)
	(pad "6" smd rect
		(at 0.76 0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a7dbb7f4-a4a8-40bd-966e-334bda9f0716")
	)
	(pad "7" smd rect
		(at 0.76 -0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5d0f862e-4c46-47b9-ba93-fcef75c4f664")
	)
	(pad "8" smd rect
		(at 0.76 -1.2 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "da33b4f2-b72e-4330-b7fb-cf412c419936")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
