(footprint "R_Shunt_Ohmite_LVK24"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contacts shunt resistor,https://www.ohmite.com/assets/docs/res_lvk.pdf")
	(tags "4 contacts resistor smd")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
		(uuid "db1a4c0b-a780-4ef7-acec-9b6b5d64d705")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Ohmite_LVK24"
		(at 0 5.325 0)
		(layer "F.Fab")
		(uuid "bc7aaf4f-5f57-44cc-8dd5-2c780ca14584")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8a73f20c-8414-40f8-beb7-16977b9cf46b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9d69a66-6f8f-40b3-9461-4d24592b1e99")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.75 0.9)
		(end -1.75 -0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1a6fc076-b637-40a5-8581-6dc34a948b55")
	)
	(fp_line
		(start 0.2 -3.35)
		(end -0.2 -3.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4a0c05dd-74d7-40e9-9d24-21f39dd32b1b")
	)
	(fp_line
		(start 0.2 3.35)
		(end -0.2 3.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e31bbf70-a8e8-43d5-99ba-c84ec2b6f4d2")
	)
	(fp_line
		(start 1.75 -0.9)
		(end 1.75 0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "27777506-7eb4-4af5-9773-1b2546346ea0")
	)
	(fp_line
		(start -2.45 -4.5)
		(end 2.45 -4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "91942984-59fd-4da4-86d8-c55421741d71")
	)
	(fp_line
		(start -2.45 4.5)
		(end -2.45 -4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4fdbff44-766f-49cf-877a-b6996e8ab37f")
	)
	(fp_line
		(start 2.45 -4.5)
		(end 2.45 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ca08365e-e4f8-4210-b518-b2107cc99dca")
	)
	(fp_line
		(start 2.45 4.5)
		(end -2.45 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "70bf9958-aad5-4478-98e1-00cbc8244bbc")
	)
	(fp_line
		(start -1.6 -3.2)
		(end 1.6 -3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "55e1a3ae-fa9b-4d1d-b9ef-abd848a3ac5a")
	)
	(fp_line
		(start -1.6 3.2)
		(end -1.6 -3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d1fa9ec4-6de1-4169-a2c9-6b76dc18147a")
	)
	(fp_line
		(start 0 3.2)
		(end -1.6 3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5d0670ad-5a21-4b18-91fb-b9ffdd8afdf0")
	)
	(fp_line
		(start 1.6 -3.2)
		(end 1.6 3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "29be0e3b-3f1c-45d3-93f4-d0510d096a0e")
	)
	(fp_line
		(start 1.6 3.2)
		(end 0 3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c5e16e80-7358-448e-ad0a-a0cf5b91d14e")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "39f940c8-8b20-4321-9d9b-05fe64c28b96")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -1.25 -2.625)
		(size 1.9 3.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "766d2828-9a40-4ae9-9f47-4ff237155fc6")
	)
	(pad "2" smd rect
		(at 1.25 -2.625)
		(size 1.9 3.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a8ab704f-ffb1-494c-a65f-ce44194b0c25")
	)
	(pad "3" smd rect
		(at 1.25 2.625)
		(size 1.9 3.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5110f476-5556-4f3a-958f-30d4d012ceb9")
	)
	(pad "4" smd rect
		(at -1.25 2.625)
		(size 1.9 3.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "356e7f02-ccfb-402d-85f6-3e089847c2a5")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Ohmite_LVK24.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
