(footprint "R_Array_Convex_2x0402"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Resistor Network, ROHM MNR02 (see mnr_g.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -1.75 0)
		(layer "F.SilkS")
		(uuid "66291a76-185d-48db-b650-948d00a9c4ff")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_2x0402"
		(at 0 1.8 0)
		(layer "F.Fab")
		(uuid "24ab06be-0816-4967-8778-c70220adbeba")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "75275cef-8939-48c2-9e4c-95468b01bd80")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "df5bde21-70f2-4bd3-908d-df07ff5fe791")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.25 -0.78)
		(end -0.25 -0.78)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "50f7c527-680f-4165-b1df-d1d949a93792")
	)
	(fp_line
		(start 0.25 0.78)
		(end -0.25 0.78)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a75c9854-4004-4236-ba2f-1fb7387b4d89")
	)
	(fp_line
		(start -1 -0.95)
		(end -1 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d99c0c96-8a6a-4cb9-adf9-3318df995e75")
	)
	(fp_line
		(start -1 -0.95)
		(end 1 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d936f7aa-ce52-46bd-b069-c13001509f7a")
	)
	(fp_line
		(start 1 0.95)
		(end -1 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "169535c3-42a6-4e1d-80e3-cb2c79f1f0c4")
	)
	(fp_line
		(start 1 0.95)
		(end 1 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9a3601af-4232-4851-8547-3c40422bd2ce")
	)
	(fp_line
		(start -0.5 -0.7)
		(end -0.5 0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e7225872-39f5-4998-8436-47ba3436b8e7")
	)
	(fp_line
		(start -0.5 0.7)
		(end 0.5 0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2b417bc3-fa08-4165-8306-7dcd18fa8e17")
	)
	(fp_line
		(start 0.5 -0.7)
		(end -0.5 -0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0d4a9ed3-ee0b-4682-8e5e-4a2416077cee")
	)
	(fp_line
		(start 0.5 0.7)
		(end 0.5 -0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f9c7a22d-eb6f-4395-a5f9-e67021c8a115")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.75 0)
		(layer "F.Fab")
		(uuid "0602aee3-f47d-4767-8779-3645a1b617e2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.5 -0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a84710ac-b50f-4ff6-9e6e-5e6257265146")
	)
	(pad "2" smd rect
		(at -0.5 0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b9adf9a6-7702-452a-80b5-d88fb0defc5b")
	)
	(pad "3" smd rect
		(at 0.5 0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "8e0c5c49-cc46-41e6-af9e-e33c57bdca9c")
	)
	(pad "4" smd rect
		(at 0.5 -0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "21e8861e-be44-4d78-a566-f2c4a3fb63a0")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_2x0402.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
