(footprint "R_Shunt_Ohmite_LVK25"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contacts shunt resistor,https://www.ohmite.com/assets/docs/res_lvk.pdf")
	(tags "4 contacts resistor smd")
	(property "Reference" "REF**"
		(at 0 -4.7 0)
		(layer "F.SilkS")
		(uuid "917a9854-3cce-4970-ac3e-36d6065248a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Ohmite_LVK25"
		(at 0.025 5.05 0)
		(layer "F.Fab")
		(uuid "e95acacf-96da-4c12-a70e-baa60b75f4e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "50fc211c-0cd1-4a24-b26a-785d01a4490f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4593b54f-93a4-4cad-8ad7-e890807e6615")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.8 0.4)
		(end -1.8 -0.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de4b30fb-45b0-49ed-8098-b6c7eac38d59")
	)
	(fp_line
		(start 1 -3.4)
		(end -1 -3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f55d418e-d38d-442d-9b76-d461ca636ae8")
	)
	(fp_line
		(start 1 3.4)
		(end -1 3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7c31ac5a-a62c-4349-a871-02d08f6f4e8d")
	)
	(fp_line
		(start 1.8 -0.4)
		(end 1.8 0.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "658e3a5f-06e6-4dce-a6d2-a297a09fdb28")
	)
	(fp_line
		(start -2.75 -4.05)
		(end 2.75 -4.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "34719262-3405-468a-bbeb-03f202db9c03")
	)
	(fp_line
		(start -2.75 4.05)
		(end -2.75 -4.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3ccefd16-5ac2-436a-9136-bfe370a18735")
	)
	(fp_line
		(start 2.75 -4.05)
		(end 2.75 4.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5a54ca5b-25a8-48c4-b164-6135e977a83e")
	)
	(fp_line
		(start 2.75 4.05)
		(end -2.75 4.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "38953463-c4a3-4e17-ad80-280d05cbdd42")
	)
	(fp_line
		(start -1.6 -3.2)
		(end 1.6 -3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7a860e9f-1b19-4af5-b1ac-58f0cc19e04a")
	)
	(fp_line
		(start -1.6 3.2)
		(end -1.6 -3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3950b11d-d974-40f5-bbdd-dbd907d7fce9")
	)
	(fp_line
		(start 0 3.2)
		(end -1.6 3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4b264e8d-b59f-4ee4-ab10-e3dac2a200df")
	)
	(fp_line
		(start 1.6 -3.2)
		(end 1.6 3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f2cf4b39-fdb1-46f9-a1e5-75e508553acf")
	)
	(fp_line
		(start 1.6 3.2)
		(end 0 3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "459a22fa-37fe-4872-8e66-022d93b5ef40")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "71aa6675-9dd1-4452-a780-1398bee2e804")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.2)
			)
		)
	)
	(pad "1" smd rect
		(at -1.8 -2.15)
		(size 1.4 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "d72ef79e-db9d-4137-8cfa-b43fd23ebbf6")
	)
	(pad "2" smd rect
		(at -1.8 2.15)
		(size 1.4 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a1a64c99-209c-40c3-90c2-096781a3084e")
	)
	(pad "3" smd rect
		(at 1.8 -2.15)
		(size 1.4 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "30994c99-464c-42b8-af0b-b2435d74da2a")
	)
	(pad "4" smd rect
		(at 1.8 2.15)
		(size 1.4 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "bd8600ea-0c11-4cff-a7a7-baf8d786f8a3")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Ohmite_LVK25.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
