(footprint "R_Cat16-2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMT resistor net, Bourns CAT16 series, 2 way")
	(tags "SMT resistor net Bourns CAT16 series 2 way")
	(property "Reference" "REF**"
		(at 0 -1.75 0)
		(layer "F.SilkS")
		(uuid "b4e04413-6c95-4141-9e66-7c769b920ec4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Cat16-2"
		(at 0 1.75 0)
		(layer "F.Fab")
		(uuid "68674cdb-2931-47d2-a136-c51c59749c20")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8c23f2b7-7d1a-42bc-bbc6-4881a3d15495")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e1063f46-abc1-40ca-a4e4-799348440e82")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 1.1 -0.9)
		(end -1.1 -0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a0717606-b045-45a4-a6d8-bc4618081b97")
	)
	(fp_line
		(start 1.1 0.9)
		(end -1.1 0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5d45c8b4-96cc-44d3-abb2-e0317f8afd30")
	)
	(fp_circle
		(center 0 0)
		(end -0.1 0)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill no)
		(layer "F.Adhes")
		(uuid "e97764e9-a19b-40c7-af9f-6aa6f31c2332")
	)
	(fp_line
		(start -1.39 -1.05)
		(end -1.39 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3870b3b9-38cd-4531-8718-b34528b9d73b")
	)
	(fp_line
		(start -1.39 -1.05)
		(end 1.39 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "89ed7c08-6484-4763-bde1-019dbdfaac71")
	)
	(fp_line
		(start 1.39 1.05)
		(end -1.39 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b0e98574-d1e4-4720-9a3b-8d6905409e2b")
	)
	(fp_line
		(start 1.39 1.05)
		(end 1.39 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8a23b953-afc3-42e4-a417-197e1f23f229")
	)
	(fp_line
		(start -0.8 -0.8)
		(end 0.8 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "25b253c2-de8d-4b55-87a0-8c1000356b67")
	)
	(fp_line
		(start -0.8 0.8)
		(end -0.8 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a6dc8c42-533e-4aaf-8a3c-71fbe5b88a8e")
	)
	(fp_line
		(start 0.8 -0.8)
		(end 0.8 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1a37ebc1-31d9-475d-84b9-a49969c2d886")
	)
	(fp_line
		(start 0.8 0.8)
		(end -0.8 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "78c24809-67c6-4526-80fa-2932f40975d4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.75 0)
		(layer "F.Fab")
		(uuid "55deb732-984f-4efd-a64d-7dedd3c80483")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.76 -0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "825449df-7ba1-4eed-8e2d-06bbfae939fd")
	)
	(pad "2" smd rect
		(at -0.76 0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b3461a14-9012-41be-865a-c3966415f039")
	)
	(pad "3" smd rect
		(at 0.76 0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "11d97768-0958-4342-a97f-76cf3a582a8c")
	)
	(pad "4" smd rect
		(at 0.76 -0.4 180)
		(size 0.76 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c1bf8d14-1037-42f8-a79b-097b2251e03d")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-2.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
