(footprint "R_1225_3264Metric_Pad1.47x6.45mm_HandSolder"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Resistor SMD 1225 (3264 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://www.koaspeer.com/pdfs/WK73S.pdf), generated with kicad-footprint-generator")
	(tags "resistor handsolder")
	(property "Reference" "REF**"
		(at 0 -4.18 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_1225_3264Metric_Pad1.47x6.45mm_HandSolder"
		(at 0 4.18 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.502064 -3.26)
		(end 0.502064 -3.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -0.502064 3.26)
		(end 0.502064 3.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -2.4 -3.48)
		(end 2.4 -3.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -2.4 3.48)
		(end -2.4 -3.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 2.4 -3.48)
		(end 2.4 3.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 2.4 3.48)
		(end -2.4 3.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -1.55 -3.15)
		(end 1.55 -3.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -1.55 3.15)
		(end -1.55 -3.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 1.55 -3.15)
		(end 1.55 3.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 1.55 3.15)
		(end -1.55 3.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 0.78 0.78)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.4125 0)
		(size 1.475 6.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.169492)
	)
	(pad "2" smd roundrect
		(at 1.4125 0)
		(size 1.475 6.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.169492)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1225_3264Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
