(footprint "R_Shunt_Isabellenhuette_BVR4026"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4-Wire Shunt, SMD 4026, https://www.isabellenhuette.de/fileadmin/Daten/Praezisionswiderstaende/Datenblaetter/BVR.PDF")
	(tags "kelvin-connection")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
		(uuid "af921c66-804f-4e11-990f-5b81b206ee94")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Isabellenhuette_BVR4026"
		(at 0 4.699 0)
		(layer "F.Fab")
		(uuid "95bef731-1750-46e4-bae7-2b988b5673ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fb4ce631-0144-42ac-9d2a-61f61012817e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d661561e-6748-48a0-9524-ad030e49b0be")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.2 2.2)
		(end -5.2 2.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b9b5c5ef-596e-42b3-b119-de4d7bc207ce")
	)
	(fp_line
		(start -2.5 -3.5)
		(end 2.5 -3.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8a69db6f-b1a4-4c36-9b61-b9461d169f24")
	)
	(fp_line
		(start -2.4 3.5)
		(end 2.4 3.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "99f12e82-bb7f-497e-93eb-411e5f8243fc")
	)
	(fp_line
		(start 5.2 2.2)
		(end 5.2 2.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b984126b-1d1d-428a-ae94-3d7fcb024cd8")
	)
	(fp_rect
		(start -5.55 -3.9)
		(end 5.55 3.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "eccb655f-cafe-4b4d-9ac7-992537bd997c")
	)
	(fp_rect
		(start -5.05 -3.3375)
		(end 5.05 3.3375)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "1ed5fdb2-e55d-4f50-8bb3-9a19aa3818bb")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "26847034-bba7-4f6a-8257-9179050aaccd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.025 -0.85)
		(size 2.55 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "8cfbe9f2-dbd4-46bc-86f3-4ea1d4698cc0")
	)
	(pad "2" smd roundrect
		(at -4.025 3.2)
		(size 2.55 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "2ab0f381-bcc1-4721-be70-36674bcfde2e")
	)
	(pad "3" smd roundrect
		(at 4.025 3.2)
		(size 2.55 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ed6c7d10-ffd8-44f1-a80d-1d630645df1c")
	)
	(pad "4" smd roundrect
		(at 4.025 -0.85)
		(size 2.55 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "77148445-fa79-41a0-96d0-a0d6c9545eee")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Isabellenhuette_BVR4026.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
