(footprint "R_0508_1220Metric_Pad1.12x2.15mm_HandSolder"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Resistor SMD 0508 (1220 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://www.koaspeer.com/pdfs/WK73S.pdf), generated with kicad-footprint-generator")
	(tags "resistor handsolder")
	(property "Reference" "REF**"
		(at 0 -2.03 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_0508_1220Metric_Pad1.12x2.15mm_HandSolder"
		(at 0 2.03 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.48 -1.33)
		(end 1.48 -1.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -1.48 1.33)
		(end -1.48 -1.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 1.48 -1.33)
		(end 1.48 1.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 1.48 1.33)
		(end -1.48 1.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -0.625 -1)
		(end 0.625 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -0.625 1)
		(end -0.625 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 0.625 -1)
		(end 0.625 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 0.625 1)
		(end -0.625 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 0.31 0.31)
				(thickness 0.05)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.6625 0)
		(size 1.125 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.222222)
	)
	(pad "2" smd roundrect
		(at 0.6625 0)
		(size 1.125 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.222222)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0508_1220Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
