(footprint "R_Array_Convex_4x1206"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
		(uuid "c03b7755-9837-468e-aede-1ec535caaa37")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_4x1206"
		(at 0 3.5 0)
		(layer "F.Fab")
		(uuid "9b460190-2cff-4922-a223-9c60c1725138")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "526b24ac-530f-4905-820e-bedd7211617a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "26622d45-d37d-4a97-b8bf-122d9ed19109")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 1.05 -2.67)
		(end -1.05 -2.67)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "08a7102c-6a90-4215-97d7-2c7691d676c2")
	)
	(fp_line
		(start 1.05 2.67)
		(end -1.05 2.67)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0288b546-eea0-4133-8602-9ebcc4de942b")
	)
	(fp_line
		(start -2.21 -2.85)
		(end -2.21 2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "809b751f-4ebf-4fad-95b8-f185cc52df6d")
	)
	(fp_line
		(start -2.21 -2.85)
		(end 2.2 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f41a0235-b0b4-4c11-b50c-4e6322edd504")
	)
	(fp_line
		(start 2.2 2.85)
		(end -2.21 2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2c3dddfc-2bef-4a95-adc7-0eea1d1d8966")
	)
	(fp_line
		(start 2.2 2.85)
		(end 2.2 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "82a6e323-87e2-4bcc-9607-b0934ae09b11")
	)
	(fp_line
		(start -1.6 -2.6)
		(end -1.6 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "089fe671-a005-4f46-9dcd-f553d4f61421")
	)
	(fp_line
		(start -1.6 2.6)
		(end 1.6 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a18e5240-9443-41b7-a28d-2d6e67bc66d6")
	)
	(fp_line
		(start 1.6 -2.6)
		(end -1.6 -2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "01560213-7be1-4227-b53c-c6d7a776707f")
	)
	(fp_line
		(start 1.6 2.6)
		(end 1.6 -2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b881cae7-c2bb-475a-be55-90d089cc7623")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "e460dad3-8e2a-450f-9d9e-0253ae136a15")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.105)
			)
		)
	)
	(pad "1" smd rect
		(at -1.5 -2)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "6556cf38-534a-4436-9f48-8e25a5b76679")
	)
	(pad "2" smd rect
		(at -1.5 -0.66)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "f46ee48a-d4aa-4410-9b56-f48d354ec72f")
	)
	(pad "3" smd rect
		(at -1.5 0.66)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c02a269f-fdc2-4d32-8e81-5cb76a044e60")
	)
	(pad "4" smd rect
		(at -1.5 2)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "d8ad4cf4-2450-4657-9892-c1e6b0d6f707")
	)
	(pad "5" smd rect
		(at 1.5 2)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ee9e3dce-9280-4eb2-b458-869fe1cb1ccf")
	)
	(pad "6" smd rect
		(at 1.5 0.66)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "20df2578-8f99-471f-b04b-b354c71e2bf6")
	)
	(pad "7" smd rect
		(at 1.5 -0.66)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "fcdc8e02-9a5b-43c6-bf28-b1558ff1ecc4")
	)
	(pad "8" smd rect
		(at 1.5 -2)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "dbbd954c-5ce2-4bac-80c6-9cb78ebd4406")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
