(footprint "R_Shunt_Vishay_WSK2512_6332Metric_T2.21mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 2.21mm, 1 to 4.9 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)")
	(tags "resistor shunt WSK2512")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(uuid "93a48ca8-a80b-4cd9-afef-01105691d0ae")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Vishay_WSK2512_6332Metric_T2.21mm"
		(at 0 2.65 0)
		(layer "F.Fab")
		(uuid "b6ede6d9-50d0-4709-9cc2-80da534b0abc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6282bfff-76df-436f-b8d1-2fc0c7b27e8d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "41e16b8e-ec08-4008-a761-185c2b298873")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.54 1.7)
		(end 0.66 1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b7d15f74-f34c-40a2-9ad3-7e8a9f312e34")
	)
	(fp_line
		(start -0.66 -1.7)
		(end 2.54 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e2137812-6be2-4558-af2e-d99c7794ef11")
	)
	(fp_line
		(start -4.38 -1.9)
		(end 4.38 -1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "15a38457-d632-4ad8-9e77-5f6366ca5bdd")
	)
	(fp_line
		(start -4.38 1.9)
		(end -4.38 -1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2ecf5387-0173-40c2-9b17-6d0e5f5083d7")
	)
	(fp_line
		(start 4.38 -1.9)
		(end 4.38 1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3c58fe9c-9ea7-49d8-a748-86840218d020")
	)
	(fp_line
		(start 4.38 1.9)
		(end -4.38 1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fe7ad3e3-7056-4ef6-9e22-5ed99f2205be")
	)
	(fp_line
		(start -3.175 -1.59)
		(end 3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0db2f8a9-1e32-45fb-a7f5-bb6c8baa4005")
	)
	(fp_line
		(start -3.175 0.32)
		(end -3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e11e8556-44a7-4718-9b91-ee784cd2860b")
	)
	(fp_line
		(start -3.175 0.32)
		(end -2.795 0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ded6761b-1336-401d-bd34-031e89bbaf43")
	)
	(fp_line
		(start -3.175 0.94)
		(end -3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ada46bd6-1208-4c67-915d-2a71c0de55a4")
	)
	(fp_line
		(start -3.175 0.94)
		(end -2.795 0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ebc8d535-51f7-4616-8ba8-0e9ccd0e5cc1")
	)
	(fp_line
		(start -2.795 0.94)
		(end -2.795 0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8819d9b4-dabc-4507-bef9-e87779c807b0")
	)
	(fp_line
		(start 2.79 -0.94)
		(end 3.17 -0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "865af5bc-d86f-4be5-a0a6-9616e717c68a")
	)
	(fp_line
		(start 2.79 -0.32)
		(end 2.79 -0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "98d6ceed-c217-4c43-aab9-8e34bb1e8ce5")
	)
	(fp_line
		(start 2.79 -0.32)
		(end 3.17 -0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d35b1f73-d189-4796-8d9d-959d79b41293")
	)
	(fp_line
		(start 3.175 -0.94)
		(end 3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a28a4b44-b50a-4147-9a62-1a6915e84c7e")
	)
	(fp_line
		(start 3.175 -0.32)
		(end 3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "452374ef-47dd-4610-9403-c44d7eecb8ab")
	)
	(fp_line
		(start 3.175 1.59)
		(end -3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "add51e31-67e7-431d-bb2c-bd6edc15a3aa")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "e8140674-6b6a-40c8-9196-940f0a28ab55")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.48 -0.635)
		(size 3.3 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "e258b0fe-8e0d-49de-bd7e-e950d87c741f")
	)
	(pad "2" smd roundrect
		(at -3.43 1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ffffda5f-ca36-4099-a27f-c07321eee25d")
	)
	(pad "3" smd roundrect
		(at 3.43 -1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "265af71f-d595-4075-b687-5a00868b476f")
	)
	(pad "4" smd roundrect
		(at 2.48 0.635)
		(size 3.3 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "1e65cb55-e8ed-4959-9134-2c60ba8b0add")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSK2512_6332Metric_T2.21mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
