(footprint "R_Array_Convex_2x0603"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -1.75 0)
		(layer "F.SilkS")
		(uuid "29364b5b-0a7e-4518-b9dc-12c1e9b06b53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_2x0603"
		(at 0 2.1 0)
		(layer "F.Fab")
		(uuid "8b28b6fc-6722-4df8-898b-0e0319bf3fea")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3aa864b8-0d47-4c52-ab9a-cc00e876c296")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d04f7e2d-cb43-4591-9b77-d8a796a6de66")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.5 -0.97)
		(end -0.5 -0.97)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "968aa70e-01e6-4bbd-a121-6b8ba41d7a04")
	)
	(fp_line
		(start 0.5 0.97)
		(end -0.5 0.97)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5a3822f5-18aa-417d-b09a-559b7cfc9b45")
	)
	(fp_line
		(start -1.55 -1.05)
		(end -1.55 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5d03f7db-8024-4edc-8fe7-eec4b21b029c")
	)
	(fp_line
		(start -1.55 -1.05)
		(end 1.55 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ee0d94ad-5eb9-44ef-961a-a36a5e42f6b6")
	)
	(fp_line
		(start 1.55 1.05)
		(end -1.55 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f59c8d75-dfc7-4e8c-8488-6c89b152c8d9")
	)
	(fp_line
		(start 1.55 1.05)
		(end 1.55 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "423f6eef-a331-4e25-a8c8-73bec906ec08")
	)
	(fp_line
		(start -0.8 -0.8)
		(end 0.8 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "76e440ff-35fc-4c42-897f-407276c95760")
	)
	(fp_line
		(start -0.8 0.8)
		(end -0.8 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e2cfa6dc-11ed-44f5-8344-6d5aca9b10df")
	)
	(fp_line
		(start 0.8 -0.8)
		(end 0.8 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "06d6ea0b-f432-4883-aabe-1c71353af826")
	)
	(fp_line
		(start 0.8 0.8)
		(end -0.8 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b20a0e4-72b1-4a1f-9a1e-aeb6fb78307b")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.75 0)
		(layer "F.Fab")
		(uuid "1e4d150c-9d4b-4723-8297-0b16821505b3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.9 -0.5)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "081d452b-f939-4b20-99a4-85d937c1b42e")
	)
	(pad "2" smd rect
		(at -0.9 0.5)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a79d70fe-ddc9-4851-b7aa-9494bc600622")
	)
	(pad "3" smd rect
		(at 0.9 0.5)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "0cdec7c0-1aae-4d0b-9aba-ce052d7059c4")
	)
	(pad "4" smd rect
		(at 0.9 -0.5)
		(size 0.8 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "aad2f3c7-4585-4018-a26a-3435cff4e27c")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
