(footprint "R_MicroMELF_MMU-0102"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, MicroMELF, MMU-0102, http://www.vishay.com/docs/28713/melfprof.pdf")
	(tags "MicroMELF Resistor")
	(property "Reference" "REF**"
		(at 0 -1.45 0)
		(layer "F.SilkS")
		(uuid "5875775a-4d97-4b46-9118-c9b1249c0f82")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_MicroMELF_MMU-0102"
		(at 0 1.55 0)
		(layer "F.Fab")
		(uuid "8b1f6dab-7d39-4b50-8ca6-1c7d040425d4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "08c0e5b8-1bc8-420a-91f0-1a6f3bc7daf5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c6a0dc80-8c2b-445b-b632-3c1bd4536b9e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.2 -0.7)
		(end 0.2 -0.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "490bb611-8695-4c49-867d-535273cfe62f")
	)
	(fp_line
		(start 0.2 0.7)
		(end -0.2 0.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a2191530-b4c2-4fd2-8004-170efa93d0bf")
	)
	(fp_line
		(start -1.8 -1)
		(end -1.8 1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6fa035d1-2201-4e55-a699-b2b3d15913e5")
	)
	(fp_line
		(start -1.8 -1)
		(end 1.8 -1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8415205c-393a-4071-ad6a-bb76f2fa2d15")
	)
	(fp_line
		(start 1.8 1)
		(end -1.8 1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "83ce4ca8-4e84-4c24-9e39-1d0d0f90c752")
	)
	(fp_line
		(start 1.8 1)
		(end 1.8 -1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f8fcd19b-80b9-4a98-925d-995e8dfa60e6")
	)
	(fp_line
		(start -1.1 -0.55)
		(end 1.1 -0.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f59fd069-2dba-4705-9c83-28b390885fa6")
	)
	(fp_line
		(start -1.1 0.55)
		(end -1.1 -0.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b3a12ba6-308b-4fd9-bd99-b411224fbd1f")
	)
	(fp_line
		(start -0.6 -0.55)
		(end -0.6 0.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fdd71790-d2fb-4e15-96d7-1557f0850dc7")
	)
	(fp_line
		(start 0.6 -0.55)
		(end 0.6 0.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "81c160c0-775f-4585-86a4-ee7500e5b04e")
	)
	(fp_line
		(start 1.1 -0.55)
		(end 1.1 0.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2c36ea45-ffc6-451d-988f-777a31c9cdb0")
	)
	(fp_line
		(start 1.1 0.55)
		(end -1.1 0.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0f39bde2-fee5-4489-b662-db96a3afb751")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.45 0)
		(layer "F.Fab")
		(uuid "e501a48f-785f-403e-b73c-fa309bdb98a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.95 0)
		(size 1.2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c43f1c71-d317-477c-b112-f522a3fa3228")
	)
	(pad "2" smd rect
		(at 0.95 0)
		(size 1.2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b449e48e-d2e2-4652-8ef9-28d0c134ce64")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MicroMELF_MMU-0102.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
