(footprint "R_Array_Convex_4x0612"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
		(uuid "c0e6ce31-c7fc-43f3-a5a7-dab2807046a1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_4x0612"
		(at 0 2.8 0)
		(layer "F.Fab")
		(uuid "a73b0a85-8e21-4e8c-b72c-b6e4abb86d2e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3b4f36b1-0324-415e-b98e-bbc71b4e0e68")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d9a43e81-99b0-4179-96c2-d34395e84756")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.5 -1.68)
		(end -0.5 -1.68)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8f3d21e6-b2a8-40de-8b88-f0d0924c9817")
	)
	(fp_line
		(start 0.5 1.68)
		(end -0.5 1.68)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "faa1a9c7-c382-4b97-a2bd-819076b2a5b3")
	)
	(fp_line
		(start -1.3 -1.85)
		(end -1.3 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f9a94600-1d48-4097-b09c-3f1dcaaa3838")
	)
	(fp_line
		(start -1.3 -1.85)
		(end 1.3 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a1df35e9-5837-4844-b4b6-93ecc9399342")
	)
	(fp_line
		(start 1.3 1.85)
		(end -1.3 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5b02c665-d873-4f56-af5f-8f0543df366b")
	)
	(fp_line
		(start 1.3 1.85)
		(end 1.3 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "61d365bc-910b-47b6-93f0-143233f688c1")
	)
	(fp_line
		(start -0.8 -1.6)
		(end 0.8 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b61d90ed-b48f-4d27-95e9-e132a0fbad60")
	)
	(fp_line
		(start -0.8 1.6)
		(end -0.8 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a4494b8-b35f-41e1-a1b9-323717ba0beb")
	)
	(fp_line
		(start 0.8 -1.6)
		(end 0.8 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "07a435a2-ce22-4a2d-9cd5-e0672d39d342")
	)
	(fp_line
		(start 0.8 1.6)
		(end -0.8 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "25696956-baff-4ed5-8a55-4083f0603951")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "8fcba2c7-188a-4bdf-8921-dc009331c70c")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -0.7 -1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "1d53dedd-0556-4ddf-a17f-eff57efc4f1a")
	)
	(pad "2" smd rect
		(at -0.7 -0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "68c64c09-30df-426d-b28d-4d746c97e39c")
	)
	(pad "3" smd rect
		(at -0.7 0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c8324caf-3822-4fba-9bab-2442613156e9")
	)
	(pad "4" smd rect
		(at -0.7 1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "55dfebaa-bf37-425b-aca6-ff0bd827b5f5")
	)
	(pad "5" smd rect
		(at 0.7 1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "d3efa5b9-34e4-4a88-9ef0-6015ff3f4ceb")
	)
	(pad "6" smd rect
		(at 0.7 0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5b8b7f9d-24f9-40f9-9dee-09505c37d739")
	)
	(pad "7" smd rect
		(at 0.7 -0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "1e3e1c34-60d7-495e-9407-95fe9eeb0b32")
	)
	(pad "8" smd rect
		(at 0.7 -1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "54046ef0-23bc-4098-8d4a-a68c953a1b44")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
