(footprint "R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "resistor handsolder")
	(property "Reference" "REF**"
		(at 0 -2.63 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(at 0 2.63 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.177064 -1.71)
		(end 2.177064 -1.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -2.177064 1.71)
		(end 2.177064 1.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4 -1.93)
		(end 4 -1.93)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4 1.93)
		(end -4 -1.93)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 4 -1.93)
		(end 4 1.93)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 4 1.93)
		(end -4 1.93)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -3.15 -1.6)
		(end 3.15 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -3.15 1.6)
		(end -3.15 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 3.15 -1.6)
		(end 3.15 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 3.15 1.6)
		(end -3.15 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.05 0)
		(size 1.4 3.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.178571)
	)
	(pad "2" smd roundrect
		(at 3.05 0)
		(size 1.4 3.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.178571)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
