(footprint "R_Array_Convex_5x0603"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Resistor Network, ROHM MNR15 (see mnr_g.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
		(uuid "59bb3e04-77d5-4f71-88e5-72ca5811bcc1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_5x0603"
		(at 0 2.8 0)
		(layer "F.Fab")
		(uuid "955255fd-a0dc-46f8-b039-a8bfa10ee3d3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f28eea11-3876-4011-900b-d0ef831e24e1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5294a04a-78dd-4c99-b194-2733bed04fe5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.53 -1.82)
		(end -0.53 -1.82)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "61bbc03e-8623-45ba-94ad-3b51a3ca9ecc")
	)
	(fp_line
		(start 0.53 1.82)
		(end -0.53 1.82)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "316274db-f292-4371-90a6-ac7e41cce4c2")
	)
	(fp_line
		(start -1.55 -1.95)
		(end -1.55 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c1944fcc-2d27-47e7-8893-3979fd0d7445")
	)
	(fp_line
		(start -1.55 -1.95)
		(end 1.55 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "70fd3cfc-0428-4132-82bc-f8acec815a0b")
	)
	(fp_line
		(start 1.55 1.95)
		(end -1.55 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cdab86d4-fac1-4ba3-b8bb-d0c3d90c41b9")
	)
	(fp_line
		(start 1.55 1.95)
		(end 1.55 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ccae9087-c750-4507-ae0e-d8850ff85f90")
	)
	(fp_line
		(start -0.8 -1.7)
		(end -0.8 1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4e3ce04d-6923-4ec4-95be-ce6dd7f7c458")
	)
	(fp_line
		(start -0.8 1.7)
		(end 0.8 1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2c64d3c7-1f26-414b-b9ea-4eed58997093")
	)
	(fp_line
		(start 0.8 -1.7)
		(end -0.8 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4a4a1f21-eabc-438a-a8cd-3c8af288f33c")
	)
	(fp_line
		(start 0.8 1.7)
		(end 0.8 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8d6796c4-1bb3-4e35-bbeb-717d3c9d0c70")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "362dbca5-7ba2-47cd-8795-9ae75a9cdc24")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -0.9 -1.36)
		(size 0.8 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e79d575c-9ea5-450d-88a8-db47062620a3")
	)
	(pad "2" smd rect
		(at -0.9 -0.64)
		(size 0.8 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "0c9a2066-fb79-4068-9f04-fa70a4552fcb")
	)
	(pad "3" smd rect
		(at -0.9 0)
		(size 0.8 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "4287679a-d302-4c45-930c-ad624d6b1e13")
	)
	(pad "4" smd rect
		(at -0.9 0.64)
		(size 0.8 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c0834c6c-a9b0-43df-b39e-558ed695f9f1")
	)
	(pad "5" smd rect
		(at -0.9 1.36)
		(size 0.8 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "242db984-f36c-4d07-be8c-5b42f42e67e7")
	)
	(pad "6" smd rect
		(at 0.9 1.36)
		(size 0.8 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "1caff16a-0a79-4ea0-a026-0d56987a997c")
	)
	(pad "7" smd rect
		(at 0.9 0.64)
		(size 0.8 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "bbfb7e5c-56fe-4441-98f1-4050bc2cf7a1")
	)
	(pad "8" smd rect
		(at 0.9 0)
		(size 0.8 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e0ca962b-e740-41aa-be6d-b3fe9f6cf2df")
	)
	(pad "9" smd rect
		(at 0.9 -0.64)
		(size 0.8 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b2a0242e-3b71-4c8b-95a5-6bf7a970091d")
	)
	(pad "10" smd rect
		(at 0.9 -1.36)
		(size 0.8 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "81ff93f6-55ff-4874-bf7f-89555ba4bcba")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_5x0603.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
