(footprint "C_3640_9110Metric_Pad2.10x10.45mm_HandSolder"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Capacitor SMD 3640 (9110 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
	(tags "capacitor handsolder")
	(property "Reference" "REF**"
		(at 0 -6.18 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_3640_9110Metric_Pad2.10x10.45mm_HandSolder"
		(at 0 6.18 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.922369 -5.21)
		(end 2.922369 -5.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -2.922369 5.21)
		(end 2.922369 5.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -5.48 -5.48)
		(end 5.48 -5.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.48 5.48)
		(end -5.48 -5.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 5.48 -5.48)
		(end 5.48 5.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 5.48 5.48)
		(end -5.48 5.48)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.57 -5.1)
		(end 4.57 -5.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.57 5.1)
		(end -4.57 -5.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 4.57 -5.1)
		(end 4.57 5.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 4.57 5.1)
		(end -4.57 5.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.175 0)
		(size 2.1 10.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.119048)
	)
	(pad "2" smd roundrect
		(at 4.175 0)
		(size 2.1 10.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.119048)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_3640_9110Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
