(footprint "R_Shunt_Vishay_WSR2_WSR3_KelvinConnection"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Power Metal Strip Resistors 0.005 to 0.2, https://www.vishay.com/docs/30101/wsr.pdf")
	(tags "SMD Shunt Resistor")
	(property "Reference" "REF**"
		(at 0 -4.7 0)
		(layer "F.SilkS")
		(uuid "c0faec96-c289-436a-b91f-a05782314efe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Vishay_WSR2_WSR3_KelvinConnection"
		(at 0 4.5 0)
		(layer "F.Fab")
		(uuid "52ee9948-15bc-4169-ae5f-38e8e3438dd7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "56dbbaf5-1fc6-4afd-8f9a-e93cccb05118")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "62a2389f-7123-4cba-89a7-feb54fb2286a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.78 -3.89)
		(end 5.78 -3.89)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b69d417d-7b81-40e1-9554-49f72af6689f")
	)
	(fp_line
		(start -5.78 3.31)
		(end 5.78 3.31)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3da7f859-1d88-4445-a27f-c8545044c68a")
	)
	(fp_line
		(start -6.8 -4.03)
		(end -6.8 3.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "adf5f96f-4172-40bd-8504-3b3b44a75d2f")
	)
	(fp_line
		(start -6.8 -4.03)
		(end 6.8 -4.03)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5b8d265a-d3c4-45ef-bf7b-19df7fc7c781")
	)
	(fp_line
		(start -6.8 3.45)
		(end 6.8 3.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "85bcda15-46d8-4801-9107-0c765d3607b6")
	)
	(fp_line
		(start 6.8 -4.03)
		(end 6.8 3.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c2c38456-0a21-4c96-9d62-1da8871e04c3")
	)
	(fp_line
		(start -5.78 -3.78)
		(end -5.78 3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "44fc2207-d52e-4718-8986-936e5c6b3d89")
	)
	(fp_line
		(start -5.78 -3.78)
		(end 5.78 -3.78)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4cfcd695-d59f-4191-b9a4-57dce01fea95")
	)
	(fp_line
		(start -5.78 3.2)
		(end 5.78 3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1dd4c49c-879b-4b08-b53c-bdd6c1614eb9")
	)
	(fp_line
		(start 5.78 -3.78)
		(end 5.78 3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "959a9877-fc95-4efb-a618-c0084353bb48")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "9336336a-d5cb-4caa-81f1-721f11be7a0b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -6.29 2.91)
		(size 0.51 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "43c359fb-059e-4544-aa52-b399a73628a6")
	)
	(pad "1" smd rect
		(at -4.575 -0.29)
		(size 3.94 5.84)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ef8357c8-0cee-47c1-a8fe-d86a933cb8ea")
	)
	(pad "2" smd rect
		(at 4.575 -0.29)
		(size 3.94 5.84)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "9bf14b0e-694d-4ce3-a6b2-4d839c184971")
	)
	(pad "2" smd rect
		(at 6.29 2.91)
		(size 0.51 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c5335fda-1e6f-4cf9-ae26-bcaeb66713b1")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSR2_WSR3.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
