(footprint "R_Array_Convex_8x0602"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
		(uuid "5946dafe-4bd3-4af7-a072-0ddef79c4fce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_8x0602"
		(at 0 3 0)
		(layer "F.Fab")
		(uuid "6fd50d1d-06d1-45b8-885c-0f3692fd9d0a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fb4014be-9dc7-400a-a132-f1dec0ec61d5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "96018623-bb02-4226-b152-0b30d771ea58")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.5 -2.12)
		(end -0.5 -2.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4360edc9-3d45-4fd2-b973-121dbacfd75a")
	)
	(fp_line
		(start 0.5 2.12)
		(end -0.5 2.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "133a1d69-a0ca-46d4-9f18-39c89a0bb917")
	)
	(fp_line
		(start -1.55 -2.25)
		(end -1.55 2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b8eeb090-deb6-4db6-9f26-f8cf1ea2f550")
	)
	(fp_line
		(start -1.55 -2.25)
		(end 1.55 -2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0ce145e7-6920-4401-afcf-c09592d659d1")
	)
	(fp_line
		(start 1.55 2.25)
		(end -1.55 2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f0d81295-9cf5-41f8-8f0c-be899a29539b")
	)
	(fp_line
		(start 1.55 2.25)
		(end 1.55 -2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6ba35591-8f8c-4360-bc91-a509d2fb5f66")
	)
	(fp_line
		(start -0.8 -2)
		(end -0.8 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0e69483b-100b-4a94-953a-a00ef920b0f0")
	)
	(fp_line
		(start -0.8 2)
		(end 0.8 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5722acb4-8793-4799-a358-6fb01cec3be5")
	)
	(fp_line
		(start 0.8 -2)
		(end -0.8 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "39d65c62-0934-4eeb-bb33-ff8b1a24bb52")
	)
	(fp_line
		(start 0.8 2)
		(end 0.8 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0ccc3e72-d89d-4bca-9a91-b972a7fae292")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "ab8514ce-6154-47dd-90e7-11705524c1c0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.9 -1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "483d6300-5f2e-428a-9758-d2e5c3ffd321")
	)
	(pad "2" smd rect
		(at -0.9 -1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c134004a-beeb-48a7-be32-33b92ceddda7")
	)
	(pad "3" smd rect
		(at -0.9 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "2d5fe6eb-14de-4f58-91ab-3524c55ab4cd")
	)
	(pad "4" smd rect
		(at -0.9 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "f20067e5-ba62-4b76-a87a-915b0d1904f6")
	)
	(pad "5" smd rect
		(at -0.9 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "83127947-a197-4bdf-be3a-8521db83e204")
	)
	(pad "6" smd rect
		(at -0.9 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b63eb887-c6eb-40d5-8eb2-3b3a9b5d3fcf")
	)
	(pad "7" smd rect
		(at -0.9 1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "b5612e46-1c55-48ad-8bf1-6070ba3b5657")
	)
	(pad "8" smd rect
		(at -0.9 1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e0682fd6-9389-4e56-b2b8-d220fbd434a4")
	)
	(pad "9" smd rect
		(at 0.9 1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "62a0f29f-e49b-4df8-a8a2-0f806ccda403")
	)
	(pad "10" smd rect
		(at 0.9 1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "233dde1c-691b-439c-a9f3-7df06f38836e")
	)
	(pad "11" smd rect
		(at 0.9 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "1a2e695a-0774-4315-a926-4cd42c820c2d")
	)
	(pad "12" smd rect
		(at 0.9 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "cbb8eb59-9cce-433a-97cb-5591b18d8cad")
	)
	(pad "13" smd rect
		(at 0.9 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "796125bf-fa5a-4752-9de9-92ba432cc21b")
	)
	(pad "14" smd rect
		(at 0.9 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "f6bdf214-8731-460e-8242-ebbdc4197df3")
	)
	(pad "15" smd rect
		(at 0.9 -1.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c7ef2b7d-6f40-4d3d-8206-60ddcfef0f0b")
	)
	(pad "16" smd rect
		(at 0.9 -1.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "88b17864-b09c-40f7-b4d4-7ce8beae2d24")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_8x0602.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
