(footprint "R_1812_4532Metric"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
	(tags "resistor")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_1812_4532Metric"
		(at 0 2.65 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.386252 -1.71)
		(end 1.386252 -1.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -1.386252 1.71)
		(end 1.386252 1.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -2.95 -1.95)
		(end 2.95 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -2.95 1.95)
		(end -2.95 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 2.95 -1.95)
		(end 2.95 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 2.95 1.95)
		(end -2.95 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -2.25 -1.6)
		(end 2.25 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -2.25 1.6)
		(end -2.25 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 2.25 -1.6)
		(end 2.25 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 2.25 1.6)
		(end -2.25 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.1375 0)
		(size 1.125 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.222222)
	)
	(pad "2" smd roundrect
		(at 2.1375 0)
		(size 1.125 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.222222)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
