(footprint "R_Array_Convex_2x1206"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Resistor Network, ROHM MNR32 (see mnr_g.pdf)")
	(tags "resistor array")
	(property "Reference" "REF**"
		(at 0 -2.3 0)
		(layer "F.SilkS")
		(uuid "29737dcd-0721-4aaa-a00c-6f67d3d0aee6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Array_Convex_2x1206"
		(at 0 2.3 0)
		(layer "F.Fab")
		(uuid "a3c67f80-26a3-41a0-ab6b-072791015d10")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "33b4437a-8dce-4e88-a48e-5b5b7660d167")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d08bc67-5c1d-48cc-8105-101b55b88341")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 1.05 -1.38)
		(end -1.05 -1.38)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f0242d0c-0931-43c6-9768-3c2573e7925c")
	)
	(fp_line
		(start 1.05 1.38)
		(end -1.05 1.38)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d1c32b0d-10d9-4cdb-b8f6-459526dd3506")
	)
	(fp_line
		(start -2.21 -1.55)
		(end -2.21 1.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e35aeff1-9db2-4c8d-9ca8-75064fabb1e7")
	)
	(fp_line
		(start -2.21 -1.55)
		(end 2.2 -1.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a3636b3e-3a7e-43e1-9a86-8c63831ba6e4")
	)
	(fp_line
		(start 2.2 1.55)
		(end -2.21 1.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e3e240ef-f0de-40b5-bb2b-2007276038ea")
	)
	(fp_line
		(start 2.2 1.55)
		(end 2.2 -1.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "73c21270-e5da-4344-9c00-729e4de23e85")
	)
	(fp_line
		(start -1.55 -1.3)
		(end 1.6 -1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "70d57454-3a21-4e95-89f5-4305c74cfc85")
	)
	(fp_line
		(start -1.55 1.3)
		(end -1.55 -1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "956dc54e-480b-4a95-9247-23f8d26ff08c")
	)
	(fp_line
		(start 1.6 -1.3)
		(end 1.6 1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aa7f70b0-88d8-4df3-a674-894294e14848")
	)
	(fp_line
		(start 1.6 1.3)
		(end -1.55 1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1f59a499-a9ee-4644-9659-b58c79f7c485")
	)
	(fp_text user "${REFERENCE}"
		(at 0.025 0 0)
		(layer "F.Fab")
		(uuid "150b216f-0c3f-4362-8762-4d82d003e0da")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.105)
			)
		)
	)
	(pad "1" smd rect
		(at -1.5 -0.7)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "d24a5138-e39c-474a-991b-a37936babdc9")
	)
	(pad "2" smd rect
		(at -1.5 0.7)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "764557e3-fd91-4821-9645-e0906248b9e1")
	)
	(pad "3" smd rect
		(at 1.5 0.7)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c37a94c3-1cc7-4193-b8c7-a1772ff77284")
	)
	(pad "4" smd rect
		(at 1.5 -0.7)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a2ca37e1-9b13-4810-a1f9-f9201328cd42")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_2x1206.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
