(footprint "R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 1.19mm, 5 to 200 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)")
	(tags "resistor shunt WSK2512")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(uuid "e64357ee-67ea-437d-842c-edd4e9b0e817")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm"
		(at 0 2.65 0)
		(layer "F.Fab")
		(uuid "6d43eee8-d677-4710-a5b6-ed0a393d7e86")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "43a355dd-2659-4979-ba88-a760956ad562")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "95c003da-70d8-48a1-b453-e1224c97f655")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.5 1.7)
		(end 1.67 1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "686b0a9f-f303-4b9c-97bc-13b268071b2a")
	)
	(fp_line
		(start -1.67 -1.7)
		(end 2.53 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8ff3cd0c-2e69-49a7-948e-62e2af1cdeaf")
	)
	(fp_line
		(start -4.38 -1.9)
		(end 4.38 -1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "97453d6f-90a6-4d0b-9533-4b9de0e70d67")
	)
	(fp_line
		(start -4.38 1.9)
		(end -4.38 -1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8d751a64-d963-4d3e-b652-c6367d221a4c")
	)
	(fp_line
		(start 4.38 -1.9)
		(end 4.38 1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5fc8cbbe-390d-45f2-b9e2-001b3b36ad53")
	)
	(fp_line
		(start 4.38 1.9)
		(end -4.38 1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "85ea9322-734e-4f57-b7f4-e08d8559c109")
	)
	(fp_line
		(start -3.175 -1.59)
		(end 3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a616017c-8c30-4c24-8988-6ebc65a5a14c")
	)
	(fp_line
		(start -3.175 0.32)
		(end -3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "007035a4-df14-4627-b9dd-16c0816e9fc4")
	)
	(fp_line
		(start -3.175 0.32)
		(end -2.795 0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7a92ebc4-86fb-494b-8925-1512bf4598dd")
	)
	(fp_line
		(start -3.175 0.94)
		(end -3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8d1ed9db-8b9e-4c9a-b026-a147d8ba5a89")
	)
	(fp_line
		(start -3.175 0.94)
		(end -2.795 0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3238b0a3-1bbc-4ecd-9eca-d39a4563f46a")
	)
	(fp_line
		(start -2.795 0.94)
		(end -2.795 0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "56e7214e-7e65-4896-9919-6dfa6ad242a1")
	)
	(fp_line
		(start 2.79 -0.94)
		(end 3.17 -0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bf2fd8b5-dc07-4d36-93f4-c05d760e4ae8")
	)
	(fp_line
		(start 2.79 -0.32)
		(end 2.79 -0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2732ea3b-0a68-4014-9f1f-147b192cb827")
	)
	(fp_line
		(start 2.79 -0.32)
		(end 3.17 -0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7597632e-0fab-4537-9ef5-3d955ee8fe04")
	)
	(fp_line
		(start 3.175 -0.94)
		(end 3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "be78e59b-9296-4843-849b-9aeaddf3ec90")
	)
	(fp_line
		(start 3.175 -0.32)
		(end 3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f0529fdf-6a96-4afa-ae66-3987676f8cc1")
	)
	(fp_line
		(start 3.175 1.59)
		(end -3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5494f1f1-9934-4901-ae11-4f45356840a6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7af73258-6848-4c90-ada6-9916b21e0d54")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.985 -0.635)
		(size 2.29 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "7d665233-6376-4fd3-9d23-184556b0630c")
	)
	(pad "2" smd roundrect
		(at -3.43 1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "a060266a-0c38-4364-b2df-6f7cf4c69f0d")
	)
	(pad "3" smd roundrect
		(at 3.43 -1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a1e31646-49e8-4836-bd67-1b6bed652414")
	)
	(pad "4" smd roundrect
		(at 2.985 0.635)
		(size 2.29 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "3f532dd2-fd5a-4fe7-9636-aa84f769e3b2")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
