(export (version D)
  (design
    (source /home/johannes/git/flippr-circuit/circuit/mainboard/mainboard.sch)
    (date "Do 09 Mai 2019 22:39:46 CEST")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title MainBoard)
        (company FlippR_ChillR)
        (rev V_01)
        (date 2019-01-25)
        (source mainboard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref RPi1)
      (value Raspberry_Pi_2_3)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical)
      (datasheet https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (libsource (lib Connector) (part Raspberry_Pi_2_3) (description "expansion header for Raspberry Pi 2 & 3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A3BB2))
    (comp (ref Column1)
      (value CD4051B)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet http://www.ti.com/lit/ds/symlink/cd4052b.pdf)
      (libsource (lib Analog_Switch) (part CD4051B) (description "CMOS single 8-channel analog multiplexer demultiplexer, TSSOP-16/DIP-16/SOIC-16"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A3DE5))
    (comp (ref Row1)
      (value CD4051B)
      (footprint Package_DIP:DIP-16_W7.62mm_LongPads)
      (datasheet http://www.ti.com/lit/ds/symlink/cd4052b.pdf)
      (libsource (lib Analog_Switch) (part CD4051B) (description "CMOS single 8-channel analog multiplexer demultiplexer, TSSOP-16/DIP-16/SOIC-16"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A3E27))
    (comp (ref Display_2)
      (value 74HC245)
      (footprint Package_DIP:DIP-20_W7.62mm_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A3F61))
    (comp (ref Display_Conn1)
      (value Conn_02x10_Odd_Even)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x10_Odd_Even) (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A4311))
    (comp (ref Input_CN1)
      (value Conn_01x20)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x20) (description "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A74B9))
    (comp (ref Input_CN2)
      (value Conn_01x20)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x20) (description "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A7563))
    (comp (ref R2)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B349D))
    (comp (ref R4)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B3760))
    (comp (ref R6)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B378A))
    (comp (ref R8)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B37BA))
    (comp (ref R10)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B37E8))
    (comp (ref R1)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B3818))
    (comp (ref R13)
      (value 4,7K)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4B3890))
    (comp (ref R3)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4F4ADA))
    (comp (ref R5)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4F4B8E))
    (comp (ref R7)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4F4BD2))
    (comp (ref R9)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4F4C14))
    (comp (ref R11)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4F4C50))
    (comp (ref R12)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4F4C8E))
    (comp (ref R14)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C50A6D8))
    (comp (ref R15)
      (value 3.3)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C50A71A))
    (comp (ref HV_Conn1)
      (value Conn_01x04_Male)
      (footprint Connector:Dicker170V_Conn)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C566356))
    (comp (ref C1)
      (value C_Small)
      (footprint Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C658A9E))
    (comp (ref Display_1)
      (value 74HC245)
      (footprint Package_DIP:DIP-20_W7.62mm_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A3EFF))
    (comp (ref C2)
      (value C_Small)
      (footprint Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68B326))
    (comp (ref C4)
      (value C_Small)
      (footprint Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68BCD2))
    (comp (ref C3)
      (value C_Small)
      (footprint Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68C137))
    (comp (ref Soundboard_Connector1)
      (value Conn_02x05_Counter_Clockwise)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Counter_Clockwise) (description "Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDA94CF))
    (comp (ref Driverboard_Connector1)
      (value Conn_02x05_Counter_Clockwise)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Counter_Clockwise) (description "Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE40B14))
    (comp (ref Extensionboard_Connector1)
      (value Conn_02x05_Counter_Clockwise)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Counter_Clockwise) (description "Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE87E7B)))
  (libparts
    (libpart (lib 74xx) (part 74LS245)
      (aliases
        (alias 74HC245))
      (description "Octal BUS Transceivers, 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS245)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib Analog_Switch) (part CD4051B)
      (description "CMOS single 8-channel analog multiplexer demultiplexer, TSSOP-16/DIP-16/SOIC-16")
      (docs http://www.ti.com/lit/ds/symlink/cd4052b.pdf)
      (footprints
        (fp TSSOP*4.4x5mm*P0.65mm*)
        (fp DIP*W7.62*)
        (fp SOIC*3.9x9.9mm*P1.27mm*)
        (fp SO*5.3x10.2mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) CD4051B))
      (pins
        (pin (num 1) (name X4) (type BiDi))
        (pin (num 2) (name X6) (type BiDi))
        (pin (num 3) (name X) (type BiDi))
        (pin (num 4) (name X7) (type BiDi))
        (pin (num 5) (name X5) (type BiDi))
        (pin (num 6) (name INH) (type input))
        (pin (num 7) (name VEE) (type power_in))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name C) (type input))
        (pin (num 10) (name B) (type input))
        (pin (num 11) (name A) (type input))
        (pin (num 12) (name X3) (type BiDi))
        (pin (num 13) (name X0) (type BiDi))
        (pin (num 14) (name X1) (type BiDi))
        (pin (num 15) (name X2) (type BiDi))
        (pin (num 16) (name VDD) (type power_in))))
    (libpart (lib Connector) (part Conn_01x04_Male)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector) (part Raspberry_Pi_2_3)
      (description "expansion header for Raspberry Pi 2 & 3")
      (docs https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (footprints
        (fp PinHeader*2x20*P2.54mm*Vertical*)
        (fp PinSocket*2x20*P2.54mm*Vertical*))
      (fields
        (field (name Reference) J)
        (field (name Value) Raspberry_Pi_2_3))
      (pins
        (pin (num 1) (name 3V3) (type power_in))
        (pin (num 2) (name 5V) (type power_in))
        (pin (num 3) (name SDA/GPIO2) (type BiDi))
        (pin (num 4) (name 5V) (type power_in))
        (pin (num 5) (name SCL/GPIO3) (type BiDi))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name GCLK0/GPIO4) (type BiDi))
        (pin (num 8) (name GPIO14/TXD) (type BiDi))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name GPIO15/RXD) (type BiDi))
        (pin (num 11) (name GPIO17) (type BiDi))
        (pin (num 12) (name GPIO18/PWM0) (type BiDi))
        (pin (num 13) (name GPIO27) (type BiDi))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name GPIO22) (type BiDi))
        (pin (num 16) (name GPIO23) (type BiDi))
        (pin (num 17) (name 3V3) (type power_in))
        (pin (num 18) (name GPIO24) (type BiDi))
        (pin (num 19) (name MOSI0/GPIO10) (type BiDi))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name MISO0/GPIO9) (type BiDi))
        (pin (num 22) (name GPIO25) (type BiDi))
        (pin (num 23) (name SCLK0/GPIO11) (type BiDi))
        (pin (num 24) (name ~CE0~/GPIO8) (type BiDi))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name ~CE1~/GPIO7) (type BiDi))
        (pin (num 27) (name ID_SD/GPIO0) (type BiDi))
        (pin (num 28) (name ID_SC/GPIO1) (type BiDi))
        (pin (num 29) (name GCLK1/GPIO5) (type BiDi))
        (pin (num 30) (name GND) (type power_in))
        (pin (num 31) (name GCLK2/GPIO6) (type BiDi))
        (pin (num 32) (name PWM0/GPIO12) (type BiDi))
        (pin (num 33) (name PWM1/GPIO13) (type BiDi))
        (pin (num 34) (name GND) (type power_in))
        (pin (num 35) (name GPIO19/MISO1) (type BiDi))
        (pin (num 36) (name GPIO16) (type BiDi))
        (pin (num 37) (name GPIO26) (type BiDi))
        (pin (num 38) (name GPIO20/MOSI1) (type BiDi))
        (pin (num 39) (name GND) (type power_in))
        (pin (num 40) (name GPIO21/SCLK1) (type BiDi))))
    (libpart (lib Connector_Generic) (part Conn_01x20)
      (description "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x20))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x05_Counter_Clockwise)
      (description "Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x05_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x10_Odd_Even)
      (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x10_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical Analog_Switch)
      (uri /usr/share/kicad/library/Analog_Switch.lib))
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib)))
  (nets
    (net (code 1) (name "Net-(Display_1-Pad16)")
      (node (ref Display_Conn1) (pin 11))
      (node (ref Display_1) (pin 16)))
    (net (code 2) (name GND)
      (node (ref HV_Conn1) (pin 2))
      (node (ref Soundboard_Connector1) (pin 6))
      (node (ref C2) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref Display_Conn1) (pin 17))
      (node (ref Display_Conn1) (pin 18))
      (node (ref Display_2) (pin 19))
      (node (ref RPi1) (pin 30))
      (node (ref RPi1) (pin 34))
      (node (ref RPi1) (pin 39))
      (node (ref Driverboard_Connector1) (pin 6))
      (node (ref Extensionboard_Connector1) (pin 6))
      (node (ref C1) (pin 2))
      (node (ref Display_1) (pin 10))
      (node (ref Display_1) (pin 19))
      (node (ref RPi1) (pin 6))
      (node (ref R2) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref Column1) (pin 8))
      (node (ref RPi1) (pin 9))
      (node (ref RPi1) (pin 14))
      (node (ref RPi1) (pin 20))
      (node (ref RPi1) (pin 25))
      (node (ref Row1) (pin 7))
      (node (ref Row1) (pin 3))
      (node (ref Row1) (pin 6))
      (node (ref Row1) (pin 8))
      (node (ref Display_2) (pin 10))
      (node (ref Column1) (pin 6))
      (node (ref Column1) (pin 7)))
    (net (code 3) (name "Net-(Display_1-Pad18)")
      (node (ref Display_1) (pin 18))
      (node (ref Display_Conn1) (pin 9)))
    (net (code 4) (name "Net-(Display_1-Pad17)")
      (node (ref Display_Conn1) (pin 12))
      (node (ref Display_1) (pin 17)))
    (net (code 5) (name "Net-(Display_1-Pad15)")
      (node (ref Display_1) (pin 15))
      (node (ref Display_Conn1) (pin 14)))
    (net (code 6) (name "Net-(Display_1-Pad14)")
      (node (ref Display_1) (pin 14))
      (node (ref Display_Conn1) (pin 13)))
    (net (code 7) (name "Net-(Display_1-Pad13)")
      (node (ref Display_1) (pin 13))
      (node (ref Display_Conn1) (pin 16)))
    (net (code 8) (name /~LT)
      (node (ref Display_2) (pin 9))
      (node (ref RPi1) (pin 37)))
    (net (code 9) (name "Net-(Display_2-Pad11)")
      (node (ref Display_Conn1) (pin 5))
      (node (ref Display_2) (pin 11)))
    (net (code 10) (name "Net-(Display_2-Pad15)")
      (node (ref Display_2) (pin 15))
      (node (ref Display_Conn1) (pin 1)))
    (net (code 11) (name "Net-(Display_2-Pad14)")
      (node (ref Display_Conn1) (pin 4))
      (node (ref Display_2) (pin 14)))
    (net (code 12) (name "Net-(Display_2-Pad13)")
      (node (ref Display_Conn1) (pin 3))
      (node (ref Display_2) (pin 13)))
    (net (code 13) (name "Net-(Display_2-Pad12)")
      (node (ref Display_Conn1) (pin 6))
      (node (ref Display_2) (pin 12)))
    (net (code 14) (name /~D3)
      (node (ref RPi1) (pin 35))
      (node (ref Display_2) (pin 8)))
    (net (code 15) (name /~D2)
      (node (ref RPi1) (pin 33))
      (node (ref Display_2) (pin 7)))
    (net (code 16) (name /~D1)
      (node (ref Display_2) (pin 6))
      (node (ref RPi1) (pin 31)))
    (net (code 17) (name /~D0)
      (node (ref Display_2) (pin 5))
      (node (ref RPi1) (pin 29)))
    (net (code 18) (name /~A2)
      (node (ref RPi1) (pin 15))
      (node (ref Display_2) (pin 4)))
    (net (code 19) (name /~A1)
      (node (ref RPi1) (pin 13))
      (node (ref Display_2) (pin 3)))
    (net (code 20) (name /~A0)
      (node (ref RPi1) (pin 11))
      (node (ref Display_2) (pin 2)))
    (net (code 21) (name "Net-(Display_1-Pad12)")
      (node (ref Display_1) (pin 12))
      (node (ref Display_Conn1) (pin 2)))
    (net (code 22) (name /~S1)
      (node (ref Display_1) (pin 2))
      (node (ref RPi1) (pin 26)))
    (net (code 23) (name /~S2)
      (node (ref Display_1) (pin 3))
      (node (ref RPi1) (pin 38)))
    (net (code 24) (name /~S3)
      (node (ref RPi1) (pin 32))
      (node (ref Display_1) (pin 4)))
    (net (code 25) (name /~S4)
      (node (ref Display_1) (pin 5))
      (node (ref RPi1) (pin 36)))
    (net (code 26) (name /~S5)
      (node (ref RPi1) (pin 7))
      (node (ref Display_1) (pin 6)))
    (net (code 27) (name /~S6)
      (node (ref Display_1) (pin 7))
      (node (ref RPi1) (pin 23)))
    (net (code 28) (name /~RUN)
      (node (ref RPi1) (pin 40))
      (node (ref Display_1) (pin 8)))
    (net (code 29) (name "Net-(Display_2-Pad18)")
      (node (ref Display_Conn1) (pin 8))
      (node (ref Display_2) (pin 18)))
    (net (code 30) (name "Net-(Display_2-Pad17)")
      (node (ref Display_Conn1) (pin 7))
      (node (ref Display_2) (pin 17)))
    (net (code 31) (name "Net-(Display_2-Pad16)")
      (node (ref Display_Conn1) (pin 10))
      (node (ref Display_2) (pin 16)))
    (net (code 32) (name +3V3)
      (node (ref Column1) (pin 16))
      (node (ref C3) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref Driverboard_Connector1) (pin 1))
      (node (ref R15) (pin 2))
      (node (ref RPi1) (pin 1))
      (node (ref Extensionboard_Connector1) (pin 1))
      (node (ref RPi1) (pin 17))
      (node (ref Row1) (pin 16))
      (node (ref R9) (pin 2))
      (node (ref Soundboard_Connector1) (pin 1)))
    (net (code 33) (name +5V)
      (node (ref Soundboard_Connector1) (pin 10))
      (node (ref Display_2) (pin 20))
      (node (ref RPi1) (pin 4))
      (node (ref RPi1) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref Driverboard_Connector1) (pin 10))
      (node (ref Extensionboard_Connector1) (pin 10))
      (node (ref Display_1) (pin 1))
      (node (ref Display_2) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref Display_1) (pin 20)))
    (net (code 34) (name "Net-(Driverboard_Connector1-Pad7)")
      (node (ref Driverboard_Connector1) (pin 7)))
    (net (code 35) (name "Net-(Driverboard_Connector1-Pad8)")
      (node (ref Driverboard_Connector1) (pin 8)))
    (net (code 36) (name "Net-(Driverboard_Connector1-Pad9)")
      (node (ref Soundboard_Connector1) (pin 9))
      (node (ref RPi1) (pin 5))
      (node (ref Extensionboard_Connector1) (pin 9))
      (node (ref Driverboard_Connector1) (pin 9)))
    (net (code 37) (name "Net-(Driverboard_Connector1-Pad3)")
      (node (ref Driverboard_Connector1) (pin 3))
      (node (ref Soundboard_Connector1) (pin 3))
      (node (ref RPi1) (pin 21))
      (node (ref Extensionboard_Connector1) (pin 3)))
    (net (code 38) (name /5.6V)
      (node (ref Soundboard_Connector1) (pin 5))
      (node (ref HV_Conn1) (pin 4))
      (node (ref Driverboard_Connector1) (pin 5))
      (node (ref Extensionboard_Connector1) (pin 5)))
    (net (code 39) (name "Net-(Driverboard_Connector1-Pad4)")
      (node (ref Driverboard_Connector1) (pin 4))
      (node (ref Soundboard_Connector1) (pin 4))
      (node (ref RPi1) (pin 19))
      (node (ref Extensionboard_Connector1) (pin 4)))
    (net (code 40) (name "Net-(Extensionboard_Connector1-Pad8)")
      (node (ref Extensionboard_Connector1) (pin 8)))
    (net (code 41) (name "Net-(Driverboard_Connector1-Pad2)")
      (node (ref Soundboard_Connector1) (pin 2))
      (node (ref RPi1) (pin 3))
      (node (ref Extensionboard_Connector1) (pin 2))
      (node (ref Driverboard_Connector1) (pin 2)))
    (net (code 42) (name "Net-(Extensionboard_Connector1-Pad7)")
      (node (ref Extensionboard_Connector1) (pin 7)))
    (net (code 43) (name "Net-(Display_1-Pad11)")
      (node (ref Display_1) (pin 11)))
    (net (code 44) (name "Net-(Display_Conn1-Pad19)")
      (node (ref HV_Conn1) (pin 1))
      (node (ref Display_Conn1) (pin 19)))
    (net (code 45) (name /PowerFailure)
      (node (ref HV_Conn1) (pin 3)))
    (net (code 46) (name "Net-(Soundboard_Connector1-Pad7)")
      (node (ref Soundboard_Connector1) (pin 7)))
    (net (code 47) (name "Net-(Soundboard_Connector1-Pad8)")
      (node (ref Soundboard_Connector1) (pin 8)))
    (net (code 48) (name "Net-(Display_1-Pad9)")
      (node (ref Display_1) (pin 9)))
    (net (code 49) (name "Net-(Display_Conn1-Pad20)")
      (node (ref Display_Conn1) (pin 20)))
    (net (code 50) (name "Net-(Input_CN1-Pad1)")
      (node (ref Input_CN1) (pin 1)))
    (net (code 51) (name "Net-(Input_CN1-Pad10)")
      (node (ref Input_CN1) (pin 10)))
    (net (code 52) (name "Net-(Input_CN1-Pad11)")
      (node (ref Input_CN1) (pin 11)))
    (net (code 53) (name "Net-(Input_CN1-Pad12)")
      (node (ref Input_CN1) (pin 12)))
    (net (code 54) (name "Net-(Input_CN1-Pad13)")
      (node (ref Input_CN1) (pin 13)))
    (net (code 55) (name "Net-(Input_CN1-Pad14)")
      (node (ref Input_CN1) (pin 14)))
    (net (code 56) (name "Net-(Input_CN1-Pad15)")
      (node (ref Input_CN1) (pin 15)))
    (net (code 57) (name "Net-(Input_CN1-Pad16)")
      (node (ref Input_CN1) (pin 16)))
    (net (code 58) (name "Net-(Display_Conn1-Pad15)")
      (node (ref Display_Conn1) (pin 15)))
    (net (code 59) (name "Net-(Input_CN2-Pad18)")
      (node (ref Input_CN2) (pin 18)))
    (net (code 60) (name "Net-(Input_CN2-Pad19)")
      (node (ref Input_CN2) (pin 19)))
    (net (code 61) (name "Net-(Input_CN2-Pad2)")
      (node (ref Input_CN2) (pin 2)))
    (net (code 62) (name "Net-(Input_CN2-Pad20)")
      (node (ref Input_CN2) (pin 20)))
    (net (code 63) (name "Net-(Input_CN2-Pad8)")
      (node (ref Input_CN2) (pin 8)))
    (net (code 64) (name "Net-(Input_CN2-Pad9)")
      (node (ref Input_CN2) (pin 9)))
    (net (code 65) (name "Net-(Input_CN1-Pad17)")
      (node (ref Input_CN1) (pin 17)))
    (net (code 66) (name "Net-(Input_CN1-Pad18)")
      (node (ref Input_CN1) (pin 18)))
    (net (code 67) (name "Net-(Input_CN1-Pad19)")
      (node (ref Input_CN1) (pin 19)))
    (net (code 68) (name "Net-(Input_CN1-Pad2)")
      (node (ref Input_CN1) (pin 2)))
    (net (code 69) (name "Net-(Input_CN1-Pad20)")
      (node (ref Input_CN1) (pin 20)))
    (net (code 70) (name "Net-(Input_CN1-Pad3)")
      (node (ref Input_CN1) (pin 3)))
    (net (code 71) (name "Net-(Input_CN1-Pad4)")
      (node (ref Input_CN1) (pin 4)))
    (net (code 72) (name "Net-(Input_CN1-Pad5)")
      (node (ref Input_CN1) (pin 5)))
    (net (code 73) (name "Net-(Input_CN1-Pad8)")
      (node (ref Input_CN1) (pin 8)))
    (net (code 74) (name "Net-(Input_CN1-Pad9)")
      (node (ref Input_CN1) (pin 9)))
    (net (code 75) (name "Net-(Input_CN2-Pad1)")
      (node (ref Input_CN2) (pin 1)))
    (net (code 76) (name "Net-(Column1-Pad15)")
      (node (ref Input_CN2) (pin 12))
      (node (ref Column1) (pin 15))
      (node (ref R12) (pin 1)))
    (net (code 77) (name "Net-(Column1-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref Input_CN2) (pin 14))
      (node (ref Column1) (pin 1)))
    (net (code 78) (name "Net-(RPi1-Pad28)")
      (node (ref RPi1) (pin 28)))
    (net (code 79) (name "Net-(RPi1-Pad27)")
      (node (ref RPi1) (pin 27)))
    (net (code 80) (name "Net-(Row1-Pad4)")
      (node (ref Row1) (pin 4)))
    (net (code 81) (name "Net-(RPi1-Pad12)")
      (node (ref RPi1) (pin 12))
      (node (ref Row1) (pin 9)))
    (net (code 82) (name "Net-(Column1-Pad4)")
      (node (ref R3) (pin 1))
      (node (ref Column1) (pin 4))
      (node (ref Input_CN2) (pin 17)))
    (net (code 83) (name "Net-(Column1-Pad10)")
      (node (ref RPi1) (pin 18))
      (node (ref Column1) (pin 10)))
    (net (code 84) (name "Net-(Column1-Pad11)")
      (node (ref Column1) (pin 11))
      (node (ref RPi1) (pin 16)))
    (net (code 85) (name "Net-(Column1-Pad12)")
      (node (ref R11) (pin 1))
      (node (ref Input_CN2) (pin 13))
      (node (ref Column1) (pin 12)))
    (net (code 86) (name "Net-(Column1-Pad13)")
      (node (ref Column1) (pin 13))
      (node (ref R15) (pin 1))
      (node (ref Input_CN2) (pin 10)))
    (net (code 87) (name "Net-(Column1-Pad14)")
      (node (ref R14) (pin 1))
      (node (ref Input_CN2) (pin 11))
      (node (ref Column1) (pin 14)))
    (net (code 88) (name "Net-(Column1-Pad3)")
      (node (ref Column1) (pin 3))
      (node (ref RPi1) (pin 24)))
    (net (code 89) (name "Net-(Column1-Pad9)")
      (node (ref Column1) (pin 9))
      (node (ref RPi1) (pin 22)))
    (net (code 90) (name "Net-(RPi1-Pad10)")
      (node (ref RPi1) (pin 10))
      (node (ref Row1) (pin 10)))
    (net (code 91) (name "Net-(RPi1-Pad8)")
      (node (ref RPi1) (pin 8))
      (node (ref Row1) (pin 11)))
    (net (code 92) (name /Row_5)
      (node (ref Input_CN2) (pin 6))
      (node (ref Row1) (pin 5))
      (node (ref Row1) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref Input_CN2) (pin 7))
      (node (ref R4) (pin 2)))
    (net (code 93) (name "Net-(Column1-Pad2)")
      (node (ref R5) (pin 1))
      (node (ref Input_CN2) (pin 16))
      (node (ref Column1) (pin 2)))
    (net (code 94) (name "Net-(Column1-Pad5)")
      (node (ref Input_CN2) (pin 15))
      (node (ref Column1) (pin 5))
      (node (ref R7) (pin 1)))
    (net (code 95) (name /Row_0)
      (node (ref Input_CN1) (pin 6))
      (node (ref R1) (pin 1))
      (node (ref Row1) (pin 13)))
    (net (code 96) (name /Row_1)
      (node (ref R13) (pin 1))
      (node (ref Row1) (pin 14))
      (node (ref Input_CN1) (pin 7)))
    (net (code 97) (name /Row_3)
      (node (ref R8) (pin 2))
      (node (ref Input_CN2) (pin 4))
      (node (ref Row1) (pin 12)))
    (net (code 98) (name /Row_2)
      (node (ref Input_CN2) (pin 3))
      (node (ref R10) (pin 2))
      (node (ref Row1) (pin 15)))
    (net (code 99) (name /Row_4)
      (node (ref R6) (pin 2))
      (node (ref Row1) (pin 1))
      (node (ref Input_CN2) (pin 5)))))