(export (version D)
  (design
    (source /home/johannes/git/flippr-circuit/circuit/driverboard/driverboard/driverboard.sch)
    (date "Do 09 Mai 2019 23:29:09 CEST")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source driverboard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value MCP23017_SP)
      (footprint Package_DIP:DIP-28_W7.62mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf)
      (libsource (lib Interface_Expansion) (part MCP23017_SP) (description "16-bit I/O expander, I2C, interrupts, w pull-ups, SPDIP-28"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A2167))
    (comp (ref Driverboard_Connector1)
      (value Conn_02x10_Odd_Even)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x10_Odd_Even) (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A3D78))
    (comp (ref HC_1)
      (value 74HC245)
      (footprint 74HCT245N:DIP254P762X420-20)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A240D))
    (comp (ref C2)
      (value C_Small)
      (footprint Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68DF77))
    (comp (ref C1)
      (value C_Small)
      (footprint Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68E091))
    (comp (ref HC_2)
      (value 74HC245)
      (footprint 74HCT245N:DIP254P762X420-20)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD45ABE))
    (comp (ref C3)
      (value C_Small)
      (footprint Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD45AC5))
    (comp (ref HC_3)
      (value 74HC245)
      (footprint 74HCT245N:DIP254P762X420-20)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD45CEC))
    (comp (ref C4)
      (value C_Small)
      (footprint Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD45CF3))
    (comp (ref Mainboard_Connector1)
      (value Conn_02x05_Counter_Clockwise)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Counter_Clockwise) (description "Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD46E67))
    (comp (ref Delay_NE555)
      (value NE555)
      (footprint Package_DIP:DIP-8_W10.16mm_LongPads)
      (datasheet http://www.ti.com/lit/ds/symlink/ne555.pdf)
      (libsource (lib Timer) (part NE555) (description "Precision Timers, DIP-8/SOIC-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD6FEE1))
    (comp (ref C47uF1)
      (value CP)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P3.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD789F8))
    (comp (ref R47k1)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P7.62mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD78D10))
    (comp (ref C10nF1)
      (value C)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P3.50mm)
      (datasheet ~)
      (libsource (lib pspice) (part C) (description "Capacitor symbol for simulation only"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD7C018))
    (comp (ref Q1)
      (value Q_PNP_BCE)
      (footprint Package_TO_SOT_THT:TO-92)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_BCE) (description "PNP transistor, base/collector/emitter"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD7C464))
    (comp (ref SW1)
      (value SW_DIP_x03)
      (footprint Button_Switch_THT:SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm)
      (libsource (lib Switch) (part SW_DIP_x03) (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD866BB))
    (comp (ref R4.7k1)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD987BA))
    (comp (ref R4.7k2)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD9881F))
    (comp (ref R4.7k3)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD9885D)))
  (libparts
    (libpart (lib 74xx) (part 74LS245)
      (aliases
        (alias 74HC245))
      (description "Octal BUS Transceivers, 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS245)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib Connector_Generic) (part Conn_02x05_Counter_Clockwise)
      (description "Generic connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x05_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x10_Odd_Even)
      (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x10_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Q_PNP_BCE)
      (description "PNP transistor, base/collector/emitter")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PNP_BCE))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name C) (type passive))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Interface_Expansion) (part MCP23017_SP)
      (description "16-bit I/O expander, I2C, interrupts, w pull-ups, SPDIP-28")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP23017_SP)
        (field (name Footprint) Package_DIP:DIP-28_W7.62mm))
      (pins
        (pin (num 1) (name GPB0) (type BiDi))
        (pin (num 2) (name GPB1) (type BiDi))
        (pin (num 3) (name GPB2) (type BiDi))
        (pin (num 4) (name GPB3) (type BiDi))
        (pin (num 5) (name GPB4) (type BiDi))
        (pin (num 6) (name GPB5) (type BiDi))
        (pin (num 7) (name GPB6) (type BiDi))
        (pin (num 8) (name GPB7) (type BiDi))
        (pin (num 9) (name VDD) (type power_in))
        (pin (num 10) (name VSS) (type power_in))
        (pin (num 11) (name NC) (type NotConnected))
        (pin (num 12) (name SCK) (type input))
        (pin (num 13) (name SDA) (type BiDi))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name A0) (type input))
        (pin (num 16) (name A1) (type input))
        (pin (num 17) (name A2) (type input))
        (pin (num 18) (name ~RESET~) (type input))
        (pin (num 19) (name INTB) (type 3state))
        (pin (num 20) (name INTA) (type 3state))
        (pin (num 21) (name GPA0) (type BiDi))
        (pin (num 22) (name GPA1) (type BiDi))
        (pin (num 23) (name GPA2) (type BiDi))
        (pin (num 24) (name GPA3) (type BiDi))
        (pin (num 25) (name GPA4) (type BiDi))
        (pin (num 26) (name GPA5) (type BiDi))
        (pin (num 27) (name GPA6) (type BiDi))
        (pin (num 28) (name GPA7) (type BiDi))))
    (libpart (lib Switch) (part SW_DIP_x03)
      (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x3*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x03))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib Timer) (part LM555)
      (aliases
        (alias ICM7555)
        (alias LMC555xM)
        (alias LMC555xMM)
        (alias LMC555xN)
        (alias MC1455)
        (alias TLC555CD)
        (alias TLC555CP)
        (alias TLC555CPS)
        (alias NA555)
        (alias NE555)
        (alias SE555)
        (alias SA555))
      (description "Timer, DIP-8/SOIC-8/SSOP-8")
      (docs http://www.ti.com/lit/ds/symlink/lm555.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*3x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM555))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name TR) (type input))
        (pin (num 3) (name Q) (type output))
        (pin (num 4) (name R) (type input))
        (pin (num 5) (name CV) (type input))
        (pin (num 6) (name THR) (type input))
        (pin (num 7) (name DIS) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib pspice) (part CAP)
      (aliases
        (alias C))
      (description "Capacitor symbol for simulation only")
      (docs ~)
      (fields
        (field (name Reference) C)
        (field (name Value) CAP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Interface_Expansion)
      (uri /usr/share/kicad/library/Interface_Expansion.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical Timer)
      (uri /usr/share/kicad/library/Timer.lib))
    (library (logical pspice)
      (uri /usr/share/kicad/library/pspice.lib)))
  (nets
    (net (code 1) (name "Net-(Driverboard_Connector1-Pad9)")
      (node (ref HC_1) (pin 14))
      (node (ref Driverboard_Connector1) (pin 9)))
    (net (code 2) (name "Net-(Driverboard_Connector1-Pad7)")
      (node (ref HC_1) (pin 15))
      (node (ref Driverboard_Connector1) (pin 7)))
    (net (code 3) (name "Net-(Driverboard_Connector1-Pad5)")
      (node (ref HC_1) (pin 16))
      (node (ref Driverboard_Connector1) (pin 5)))
    (net (code 4) (name "Net-(Driverboard_Connector1-Pad3)")
      (node (ref HC_1) (pin 17))
      (node (ref Driverboard_Connector1) (pin 3)))
    (net (code 5) (name "Net-(Driverboard_Connector1-Pad1)")
      (node (ref Driverboard_Connector1) (pin 1))
      (node (ref HC_1) (pin 18)))
    (net (code 6) (name "Net-(HC_3-Pad3)")
      (node (ref Mainboard_Connector1) (pin 4))
      (node (ref HC_3) (pin 3)))
    (net (code 7) (name "Net-(HC_3-Pad2)")
      (node (ref Mainboard_Connector1) (pin 3))
      (node (ref HC_3) (pin 2)))
    (net (code 8) (name "Net-(HC_2-Pad9)")
      (node (ref HC_2) (pin 9))
      (node (ref U1) (pin 28)))
    (net (code 9) (name "Net-(HC_2-Pad8)")
      (node (ref U1) (pin 27))
      (node (ref HC_2) (pin 8)))
    (net (code 10) (name "Net-(HC_2-Pad7)")
      (node (ref U1) (pin 26))
      (node (ref HC_2) (pin 7)))
    (net (code 11) (name "Net-(Driverboard_Connector1-Pad2)")
      (node (ref HC_2) (pin 17))
      (node (ref Driverboard_Connector1) (pin 2)))
    (net (code 12) (name "Net-(Driverboard_Connector1-Pad14)")
      (node (ref Driverboard_Connector1) (pin 14))
      (node (ref HC_2) (pin 12)))
    (net (code 13) (name "Net-(Driverboard_Connector1-Pad12)")
      (node (ref Driverboard_Connector1) (pin 12))
      (node (ref HC_2) (pin 13)))
    (net (code 14) (name "Net-(Driverboard_Connector1-Pad10)")
      (node (ref HC_2) (pin 14))
      (node (ref Driverboard_Connector1) (pin 10)))
    (net (code 15) (name "Net-(Driverboard_Connector1-Pad8)")
      (node (ref HC_2) (pin 15))
      (node (ref Driverboard_Connector1) (pin 8)))
    (net (code 16) (name "Net-(Driverboard_Connector1-Pad6)")
      (node (ref Driverboard_Connector1) (pin 6))
      (node (ref HC_2) (pin 16)))
    (net (code 17) (name "Net-(Driverboard_Connector1-Pad17)")
      (node (ref Driverboard_Connector1) (pin 17))
      (node (ref HC_2) (pin 18)))
    (net (code 18) (name "Net-(Driverboard_Connector1-Pad15)")
      (node (ref Driverboard_Connector1) (pin 15))
      (node (ref HC_1) (pin 11)))
    (net (code 19) (name "Net-(Driverboard_Connector1-Pad13)")
      (node (ref Driverboard_Connector1) (pin 13))
      (node (ref HC_1) (pin 12)))
    (net (code 20) (name "Net-(Driverboard_Connector1-Pad11)")
      (node (ref HC_1) (pin 13))
      (node (ref Driverboard_Connector1) (pin 11)))
    (net (code 21) (name "Net-(HC_1-Pad4)")
      (node (ref U1) (pin 3))
      (node (ref HC_1) (pin 4)))
    (net (code 22) (name "Net-(HC_1-Pad7)")
      (node (ref HC_1) (pin 7))
      (node (ref U1) (pin 6)))
    (net (code 23) (name "Net-(HC_1-Pad6)")
      (node (ref HC_1) (pin 6))
      (node (ref U1) (pin 5)))
    (net (code 24) (name "Net-(HC_1-Pad5)")
      (node (ref HC_1) (pin 5))
      (node (ref U1) (pin 4)))
    (net (code 25) (name "Net-(HC_1-Pad3)")
      (node (ref U1) (pin 2))
      (node (ref HC_1) (pin 3)))
    (net (code 26) (name "Net-(HC_1-Pad2)")
      (node (ref HC_1) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 27) (name "Net-(Mainboard_Connector1-Pad2)")
      (node (ref U1) (pin 13))
      (node (ref Mainboard_Connector1) (pin 2)))
    (net (code 28) (name "Net-(Mainboard_Connector1-Pad9)")
      (node (ref Mainboard_Connector1) (pin 9))
      (node (ref U1) (pin 12)))
    (net (code 29) (name "Net-(HC_2-Pad3)")
      (node (ref U1) (pin 22))
      (node (ref HC_2) (pin 3)))
    (net (code 30) (name "Net-(HC_2-Pad6)")
      (node (ref U1) (pin 25))
      (node (ref HC_2) (pin 6)))
    (net (code 31) (name "Net-(HC_2-Pad5)")
      (node (ref U1) (pin 24))
      (node (ref HC_2) (pin 5)))
    (net (code 32) (name "Net-(HC_2-Pad4)")
      (node (ref HC_2) (pin 4))
      (node (ref U1) (pin 23)))
    (net (code 33) (name "Net-(HC_2-Pad2)")
      (node (ref U1) (pin 21))
      (node (ref HC_2) (pin 2)))
    (net (code 34) (name "Net-(HC_1-Pad9)")
      (node (ref U1) (pin 8))
      (node (ref HC_1) (pin 9)))
    (net (code 35) (name "Net-(HC_1-Pad8)")
      (node (ref HC_1) (pin 8))
      (node (ref U1) (pin 7)))
    (net (code 36) (name "Net-(R4.7k1-Pad1)")
      (node (ref U1) (pin 15))
      (node (ref SW1) (pin 4))
      (node (ref R4.7k1) (pin 1)))
    (net (code 37) (name "Net-(R4.7k2-Pad1)")
      (node (ref R4.7k2) (pin 1))
      (node (ref SW1) (pin 5))
      (node (ref U1) (pin 16)))
    (net (code 38) (name +5C)
      (node (ref SW1) (pin 3))
      (node (ref SW1) (pin 2))
      (node (ref SW1) (pin 1)))
    (net (code 39) (name "Net-(Delay_NE555-Pad3)")
      (node (ref Q1) (pin 1))
      (node (ref Delay_NE555) (pin 3)))
    (net (code 40) (name "Net-(HC_2-Pad11)")
      (node (ref Q1) (pin 3))
      (node (ref HC_2) (pin 11)))
    (net (code 41) (name "Net-(Driverboard_Connector1-Pad16)")
      (node (ref Driverboard_Connector1) (pin 16))
      (node (ref Q1) (pin 2)))
    (net (code 42) (name "Net-(R4.7k3-Pad1)")
      (node (ref SW1) (pin 6))
      (node (ref U1) (pin 17))
      (node (ref R4.7k3) (pin 1)))
    (net (code 43) (name +5V)
      (node (ref HC_1) (pin 1))
      (node (ref HC_2) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref Mainboard_Connector1) (pin 10))
      (node (ref HC_1) (pin 20))
      (node (ref HC_3) (pin 20))
      (node (ref C2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref HC_2) (pin 20))
      (node (ref HC_3) (pin 1)))
    (net (code 44) (name GND)
      (node (ref Mainboard_Connector1) (pin 6))
      (node (ref HC_3) (pin 19))
      (node (ref C10nF1) (pin 2))
      (node (ref HC_3) (pin 10))
      (node (ref HC_2) (pin 19))
      (node (ref R4.7k1) (pin 2))
      (node (ref Delay_NE555) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref HC_2) (pin 10))
      (node (ref C4) (pin 1))
      (node (ref R4.7k2) (pin 2))
      (node (ref U1) (pin 10))
      (node (ref U1) (pin 19))
      (node (ref C47uF1) (pin 2))
      (node (ref R4.7k3) (pin 2))
      (node (ref U1) (pin 20))
      (node (ref HC_1) (pin 19))
      (node (ref C2) (pin 1))
      (node (ref HC_1) (pin 10)))
    (net (code 45) (name "Net-(C10nF1-Pad1)")
      (node (ref C10nF1) (pin 1))
      (node (ref Delay_NE555) (pin 5)))
    (net (code 46) (name "Net-(Delay_NE555-Pad7)")
      (node (ref Delay_NE555) (pin 7)))
    (net (code 47) (name "Net-(Delay_NE555-Pad4)")
      (node (ref Delay_NE555) (pin 4)))
    (net (code 48) (name "Net-(C47uF1-Pad1)")
      (node (ref C47uF1) (pin 1))
      (node (ref R47k1) (pin 2))
      (node (ref Delay_NE555) (pin 6))
      (node (ref Delay_NE555) (pin 2)))
    (net (code 49) (name "Net-(Driverboard_Connector1-Pad20)")
      (node (ref Driverboard_Connector1) (pin 20))
      (node (ref HC_3) (pin 17)))
    (net (code 50) (name "Net-(Driverboard_Connector1-Pad19)")
      (node (ref Driverboard_Connector1) (pin 19))
      (node (ref HC_3) (pin 18)))
    (net (code 51) (name "Net-(Delay_NE555-Pad8)")
      (node (ref Delay_NE555) (pin 8))
      (node (ref Mainboard_Connector1) (pin 5))
      (node (ref R47k1) (pin 1)))
    (net (code 52) (name +3V3)
      (node (ref U1) (pin 9))
      (node (ref Mainboard_Connector1) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 18)))
    (net (code 53) (name "Net-(Driverboard_Connector1-Pad4)")
      (node (ref Driverboard_Connector1) (pin 4)))
    (net (code 54) (name "Net-(Driverboard_Connector1-Pad18)")
      (node (ref Driverboard_Connector1) (pin 18)))
    (net (code 55) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 56) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 57) (name "Net-(HC_3-Pad16)")
      (node (ref HC_3) (pin 16)))
    (net (code 58) (name "Net-(HC_3-Pad7)")
      (node (ref HC_3) (pin 7)))
    (net (code 59) (name "Net-(HC_3-Pad6)")
      (node (ref HC_3) (pin 6)))
    (net (code 60) (name "Net-(HC_3-Pad5)")
      (node (ref HC_3) (pin 5)))
    (net (code 61) (name "Net-(HC_3-Pad4)")
      (node (ref HC_3) (pin 4)))
    (net (code 62) (name "Net-(HC_3-Pad8)")
      (node (ref HC_3) (pin 8)))
    (net (code 63) (name "Net-(HC_3-Pad15)")
      (node (ref HC_3) (pin 15)))
    (net (code 64) (name "Net-(HC_3-Pad14)")
      (node (ref HC_3) (pin 14)))
    (net (code 65) (name "Net-(HC_3-Pad13)")
      (node (ref HC_3) (pin 13)))
    (net (code 66) (name "Net-(HC_3-Pad12)")
      (node (ref HC_3) (pin 12)))
    (net (code 67) (name "Net-(HC_3-Pad11)")
      (node (ref HC_3) (pin 11)))
    (net (code 68) (name "Net-(Mainboard_Connector1-Pad8)")
      (node (ref Mainboard_Connector1) (pin 8)))
    (net (code 69) (name "Net-(Mainboard_Connector1-Pad7)")
      (node (ref Mainboard_Connector1) (pin 7)))
    (net (code 70) (name "Net-(HC_3-Pad9)")
      (node (ref HC_3) (pin 9)))))