(footprint "R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 2.66mm, 0.5 to 0.99 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)")
	(tags "resistor shunt WSK2512")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(uuid "4db44122-a6d3-4f3d-8bc8-782b18b396fa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm"
		(at 0 2.65 0)
		(layer "F.Fab")
		(uuid "4eac07f2-4114-421d-ba40-acff2f8f5774")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9af2f612-947e-4724-bd36-448bfcce7af9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0732700d-b5b8-414f-b134-5dbc6c50a970")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.54 1.7)
		(end 0.66 1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f4a6b2c6-0bb6-48fa-9c70-a43ae4360213")
	)
	(fp_line
		(start -0.66 -1.7)
		(end 2.54 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1ee0773b-79a9-44f0-b996-9898b90dcea0")
	)
	(fp_line
		(start -4.38 -1.9)
		(end 4.38 -1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "69740273-c751-4ed8-bb1a-e33edd4df85a")
	)
	(fp_line
		(start -4.38 1.9)
		(end -4.38 -1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "400e9bb8-b8a5-4782-a1c2-c19d6304c15a")
	)
	(fp_line
		(start 4.38 -1.9)
		(end 4.38 1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9c17c8e9-44e3-4613-92ab-faa75681f7a2")
	)
	(fp_line
		(start 4.38 1.9)
		(end -4.38 1.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c9223c1a-3635-4cd7-a21e-28db4c60bb2a")
	)
	(fp_line
		(start -3.175 -1.59)
		(end 3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2c228520-509e-4fae-93a6-b1b6c7c27048")
	)
	(fp_line
		(start -3.175 0.32)
		(end -3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4dfd2afe-5ab6-4222-a2ed-7185047809b6")
	)
	(fp_line
		(start -3.175 0.32)
		(end -2.795 0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "882b0a7b-9713-4831-99ae-0112f77b88f5")
	)
	(fp_line
		(start -3.175 0.94)
		(end -3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ef456043-efce-4cdf-926d-7865b9ea0fe1")
	)
	(fp_line
		(start -3.175 0.94)
		(end -2.795 0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0660d0c6-9e7f-4cc6-8cb3-c088f86fff3a")
	)
	(fp_line
		(start -2.795 0.94)
		(end -2.795 0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7129ec73-1aba-4a44-9f7e-891b737d3091")
	)
	(fp_line
		(start 2.79 -0.94)
		(end 3.17 -0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4f18393e-501e-4221-89ee-f1b72ac351e1")
	)
	(fp_line
		(start 2.79 -0.32)
		(end 2.79 -0.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "297451d8-a49e-48f8-b517-3515c98b812c")
	)
	(fp_line
		(start 2.79 -0.32)
		(end 3.17 -0.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a7b33753-b0a4-4eb8-af12-9f02924c714e")
	)
	(fp_line
		(start 3.175 -0.94)
		(end 3.175 -1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3fe80491-7ba5-4827-95aa-c5514d772b9e")
	)
	(fp_line
		(start 3.175 -0.32)
		(end 3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "107f4b44-eb37-4615-8af0-e0453a7f83f6")
	)
	(fp_line
		(start 3.175 1.59)
		(end -3.175 1.59)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "12229233-616a-40b0-aefd-71ad9b5c15d2")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "f2f9f224-455c-4bad-92b3-1e06a40884a0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.48 -0.635)
		(size 3.3 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "8c0b699f-31c3-4243-b91b-7777f57d94ed")
	)
	(pad "2" smd roundrect
		(at -3.43 1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "d8123fe4-1675-4181-9693-1728438bb1f2")
	)
	(pad "3" smd roundrect
		(at 3.43 -1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e30fc10f-c18f-46b7-8904-8923d6967eff")
	)
	(pad "4" smd roundrect
		(at 2.48 0.635)
		(size 3.3 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
		(uuid "c90b701e-aaf3-4a78-a42f-dab8bac50024")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
